Quartz:

A QoS Architecture for Open Systems

Frank Siqueira

Ph.D. Thesis

Department of Computer Science

TrinityCollege, Universityof Dublin

December 1999

Declaration

Iherebydeclare that:

(a) This thesis has not been submitted as an exerc ise for a degree at this or anyother

University.

(b) This thesis is entirelythe work of the author, except where otherwise stated.

(c) The TrinityCollege Librarymaylend and copythis thesis upon request.

______________________

Frank Siqueira

October 1999

Acknowledgements

Iwould like to express myearnest gratitude to mysupervisor, Dr. VinnyCahill, for always providing useful advice with patience, care and interest. Iwill always be grateful to him for believing in myabilities and for providing me with freedom to explore and investigate the research topics that Ifound interested. Iwould also like to thank him for arranging for myfunding and for heading the research group skilfully.

Iwould like to thank all mycolleagues in the Distributed Systems Group for their direct and indirect contributions to this Thesis, and for the good moments that we spent together in the last three years. Manythanks to the staff of the Department of Computer

Science for the efficient support and friendship provi ded bythem. Iwould also like to thank David O´Flanagan and John Segrave - Dalyfor the contribution given to this research project in the form of application tests.

Finally, Iwould like to thank myfamilyand friends that, despite the distance, never let me feel alone and always provided me with extremelyvaluable emotional support.

Summary

The term `QoS architecture´ is used to describe middleware that provides applications with mechanisms for specification and enforcement of qualityof service (QoS) re quirements. These architectures administer the resources provided bythe underlying system with the intent of fulfilling the QoS requirements imposed byapplications.

Substantial work on QoS architectures can be found in the literature. However, the archit ectures proposed so far consider onlypart of the overall problem of delivering

QoS in open systems.

The QoS architectures currentlyavailable are able to provide applications in a particular application area with the guarantees supported bythe specific network architecture and the operating system to which theyare bound. Most of these architectures, moreover, require QoS to be specified byusing a low - level format that is not appropriate for applications that have a more high - level notion of QoS. Due al so to their close integration with the underlying system, these architectures cannot be deployed over multiple computing platforms. Since theytarget a specific area of application, the area in which these architectures can be used is limited. In most case s the underlying system is not made completelytransparent for the application, which still has to deal with low - level issues. In addition, most QoS architectures ignore dynamic resource adaptation, which can occur due to factors such as resource failure o r system reconfiguration.

This thesis describes the design and implementation of Quartz, a QoS architecture for

QoS specification and enforcement in open systems, designed with the aim of solving the limitations of previous proposals in this area. Quartz i s able to handle the differences between the multiple platforms that maybe present in open systems due to its flexible and extensible structure based on replaceable components. Quartz can also adapt itself byrearranging its internal components, in order to provide mechanisms for QoS specification and enforcement suitable for different areas of application. These requirements are interpreted byQuartz and used to enforce QoS byemploying the resource reservation mechanisms provided bythe network and opera ting system. By adopting this strategy, Quartz makes the underlying resource reservation mechanisms transparent to applications requiring QoS enforcement. Furthermore, Quartz provides support for QoS adaptation bytracking resource adaptations that occur a t lower levels and initiating QoS adaptation whenever needed.

This thesis presents a prototype implementation of the Quartz architecture and a series of applications built on top of it, including a complete framework for the development of multimedia appli cations based on the CORBA architecture. The experience gained by writing these applications shows the usefulness and efficiencyof Quartz as a tool for supporting QoS specification and enforcement for diverse areas of application in open, heterogeneous en vironments.

Table of Contents

1 INTRODUCTION 1

1.1 Delivering QoS in Open Systems 2

1.2 The QuartzQoS Architecture 4

1.3 Contribution 5

1.4 Analysis 6

1.5 Roadmap 8

2 OVERVIEW OFTHE RES EARCH AREA 9

2.1 Multimedia Applications 10

2.1.1 Distributed Multi media 11

2.1.2 Continuous Media 12

2.1.3 Multimedia Technology 14

2.2 Real - Time Applications 15

2.2.1 Real - TimeTechnology 17

2.3 Open Systems 18

2.3.1 Open Systems Technology 19

2.4 Distributed Object Computing 20

2.4.1 CORBA 21

2.4.2 CORBAs ervices 23

2.4.3 CORBA A/V Streams 25

2.5 Quality of Service 27

2.5.1 Def initions 28

2.5.2 QoS Specif ication 30

2.5.3 QoS Mapping andTranslation 30

2.5.4 QoS Enforcement 31

2.5.5 QoS Architectures 32

2.5.6 ISO QoSFramework 33

2.6 Resource R eservation 34

2.6.1 Resource Adaptation 36

2.6.2 ATM 37

2.6.3 Internet Protocols 42

2.6.4 Real - Time Capabilities ofW indows NT 45

2.7 Summary 46

3 STATE OF THEART 47

3.1 XRMand Xbind (Univ. of Columbia) 47

3.2 ReTINAProject (ACTS) 49

3.3 D IMMA (APM - ANSA) 50

3.4 SUMO (Univ. of Lancaster) 52

3.5 TAO (W ashington University at St. Louis) 53

3.6 Arcade (CNET and ENST) 54

3.7 OM EGA and The QoS Broker (Univ. of Pennsylvania) 55

3.8 QoS - A (Univ. of Lancaster) 57

3.9 QuO (BBN Systems and Technologies) 58

3.10 QUANTA(Old Dominion University) 59

3.11 ERDoS (SRI International) 60

3.12 MMN Project (BT - URI) 61

3.13 Analysis of the State of the Art Technology 63

4 DESIGN OF THE QUAR TZ QOS ARCHITECTURE 65

4.1 Requirements 65

4.1.1 Requirements on the Specif ication of QoS 66

4.1.2 Requirements on the Enforcement of QoS 66

4.1.3 Support for Heterogeneity 67

4.1.4 Support for QoS Adaptation 68

4.2 The Quartz Architecture 68

4.2.1 Overviewof the Architecture 69

4.2.2 Internal Structure 70

4.2.3 TheTranslation Unit 72

4.2.4 Application Filters 74

4.2.5 The QoSInterpreter 75

4.2.6 Syste m Filters 76

4.2.7 System Agents 76

4.2.8 The User Interface 77

4.3 QoS Parameters 78

4.3.1 Parameter Formats 79

4.3.2 Application - Specif ic QoSParameters 80

4.3.3 Generic Application - Level QoS Parameters 80

4.3.4 Generic System - Level QoS Parameters 81

4.3.5 System - Specif ic QoS Parameters 81

4.3.6 Translation Rules Between Generic Parameters 82

4.4 Additional Features 83

4.4.1 Dynamic Resource Adaptation andQoS Adaptation 83

4.4.2 Extending the Architecture 85

4.5 Summary 87

5 IMPLEMENTATION 88

5.1 The Quartz Prototype 88

5.1.1 Supported Platf orms 88

5.1.2 Software Model 89

5.2 The Quartz Core 90

5.2.1 Specif ication of QoS Parameters 90

5.2.2 Basic Translation Components 91

5.2.3 Basic System Agents 92

5.2.4 Interaction Between Components 93

5.3 The RSVP Sub - System 95

5.3.1 RSVP Parameters 95

5.3.2 The RSVP Filter 96

5.3.3 The RSVP Agent 97

5.4 The ATMSub - System 97

5.4.1 ATMParameters 98

5.4.2 The ATMFilt er 98

5.4.3 The ATMAgent 99

5.5 TheW indows NT Sub - System 99

5.5.1 W indows NT Parameters 99

5.5.2 TheW indows NT Filter 100

5.5.3 TheW indows NT Agent 101

5.6 Component Testing 101

5.7 Summary 103

6 THE QUARTZ/CORBA FR AMEW ORK 104

6.1 Motivat ion 105

6.2 Description of the Quartz/CORBA Framework 106

6.3 Application Scenarios 109

6.3.1 Media Broadcast 109

6.3.2 On - Demand Media 110

6.3.3 Videoconf erence 111

6.3.4 Media Session with Synchronisation 112

6.4 Implementation of theQuartz/CORBA Framework 114

6.4.1 Im plementation of the CORBA A/V Streams Mechanism 114

6.4.2 Integration of A/V Streams andQuartz 116

6.5 Application: The Distributed Music Rehearsal Studio 118

6.6 An alysis of the CORBA/Quartz Framework 120

6.7 Summary 122

7 VALIDATION AND EVAL UATION 123

7.1 Validation Tests 123

7.1.1 The Remote Copy Application 124

7.1.2 TheTelephone Exchange Application 126

7.1.3 The Distributed Music Rehearsal Studio 130

7.1.4 Results Achieved with the Validation Tests 130

7.1.5 Perf ormance 132

7.2 Fulf ilment of Requirements 133

7.2.1 QoS Specif ication 133

7.2.2 QoS Enforcement 134

7.2.3 Heterogeneity 135

7.2.4 Support for Adaptation 135

7.3 Comparison with other QoS Architectures 136

7.4 Summary 139

8 CONCLUSIONS 140

8.1 Background 140

8.2 The Quartz Architecture 142

8.3 Contribution 143

8.4 Perspectives f or FutureW ork 144

REFERENCES 146

APPENDIX 162

List of Figures

Figure 1 ˘ The CORBA Architecture 22

Figure 2 ˘ Overviewof the CORBA A/VStreams Mechanism 26

Figure 3 ˘ The ATMArchitecture 38

Figure 4 ˘ Internet Next Generation Protocols 43

Figure 5 ˘ Propagation of RSVP Messages 43

Figure 6 ˘ Overviewof the QuartzQoS Architecture 69

Figure 7 ˘ Detailed Structure of the QoS Agent 72

Figure 8 ˘ Translation Paths 73

Figure 9 ˘ Interface of Translation Components 74

Figure 10 ˘ Interface of Component Agents 77

Figure 11 ˘ User Interface of the QoS Agent 78

Figure 12 ˘ Example of QoS Adaptation 85

Figure 13 ˘ UML of Class

QzQoS 90

Figure 14 ˘ UML of Basic Translation Components 91

Figure 15 ˘ UML of Basic System Agents and Upcall Interf ace 92

Figure 16 ˘ Interaction Between Components 94

Figure 17 ˘ Available Technologyf or Distributed Multimedia Applications 105

Figure 18 ˘ The Quartz/ CORBA Media Streaming Framework 108

Figure 19 ˘ Video Broadcast 110

Figure 20 ˘ On - DemandVideo 111

Figure 21 ˘ Video Telephony 112

Figure 22 ˘ Multimedia Document with Synchronisation 113

Figure 23 ˘ UML of theCORBA A/V Streams Mechanism 114

Figure 24 ˘ UML of the FlowEndPoint 115

Figure 25 ˘ UML of theA/V Streams Filter 117

Figure 26 ˘ Usage Scenario of the Distributed Music Rehearsal Studio 119

Figure 27 ˘ Interface of the Distributed Music Rehearsal Studio 120

Figure 28 ˘ The RemoteCopy Application 124

Figure 29 ˘ State Diagram of aTelephone Call 127

List of Tables

Table 1 ˘ Typical Bandwidth of Diff erent Classes of Continuous Media 14

Table 2 ˘ Example s of Parameter Mapping 31

Table 3 ˘ Original ATMClasses of Service and Adaptation Layers 40

Table 4 ˘ Resulting ATM Classes of Service andAdaptation Layers 41

Table 5 ˘ Features Provided by State - of - the - art QoS Architectures 64

Table 6 ˘ Generic Application - Level QoS Parameters 80

Table 7 ˘ Generic System - Level QoSParameters 81

Table 8 ˘ Relationship between Generic Parameters 82

Table 9 ˘ RSVP QoS Parameters 95

Table 10 ˘ Additional Parameters 96

Table 11 ˘ ATMQoS Parameters 98

Table 12 ˘ Example of Translation of QoS Parameters 102

Table 13 ˘ Example of Balancing of QoS Parameters 102

Table 14 ˘ Example of Adaptation of QoS Parameters 102

Table 15 ˘ A/V Streams QoS Parameters 117

Table 16 ˘ Mapping between A/V Streams Parameters andGeneric Parameters 118

Table 17 ˘ Parameters Recognised bythe Data Packet Filter 125

Table 18 ˘ Parameters Recognised bythe Circuit Switch Filter 128

Table 19 ˘ Parameters Recognised bythe Phone Circuit Filter 129

Table 20 ˘ Parameters Recognis ed bythe Deadline Scheduling Filter 129

Table 21 ˘ ApplicationsBuilt Using Quartz 131

Table 22 ˘ Overhead Imposed by Quartz 132

Table 23 ˘ Comparisonof Quartz with other QoSArchitectures 138

1

Introduction

This thesis is concerned with the studyof mechanisms for the provision of qualityof service (QoS) in open, heterogeneous and distributed environments. In order to overcome a serie s of limitations that were identified in similar work previously developed in this area of research, we have designed and implemented the Quartz QoS architecture. In essence, Quartz describes middleware that supports the specification and enforcement of Qo S in open systems.

Quartz provides support for applications that require QoS - constrained services from the underlying system byinteracting with resource reservation protocols present at the lower level. Applications supported byQuartz do not necessarily come from a single application domain. Moreover, the architecture does not depend on the use of a specific underlying operating system or network infrastructure. Bysupporting heterogeneityand distribution, the Quartz architecture is made suitable for op en systems.

This chapter begins byintroducing the problem of supporting QoS in open systems and describing the issues that should be addressed bymiddleware that is responsible for providing mechanisms for the specification and enforcement of QoS. In seq uence, we brieflydescribe our proposed QoS architecture and outline its contribution to this field of research in comparison with other work in the same area. Finally, a roadmap of the remainder of this thesis is given.

1.1 Delivering QoS in Open Systems

With the popularisation of the Internet, the demand for distributed applications has increased considerably. These applications can be verycomplex to implement due to the necessityof dealing with network protocols, addresses, system heterogeneityand any oth er factor incurred from the topologyof the computing platform. Distributed applications are often built on top of distributed computing middleware, which handles the complexitythat originates from the distributed nature of the application on behalf of th e programmer, makes applications easier to implement, increases their portability, and allows them to interoperate with other applications.

Some distributed applications can function properlyon the currentlyavailable networking platforms and operating sy stems. However, there exists a categoryof computer applications that is not satisfied bythe best - effort resource management policies provided bythe majorityof the computing platforms that are currently available. For these applications, the availabilit yof resources provided bythe underlying system is required to be predictable. These applications are said to have qualityof service (QoS) requirements, and include applications varying from real - time control systems to distributed multimedia systems.

A pplications that require a certain level of QoS must specifytheir requirements in a clear and accurate manner byusing QoS parameters. The values of these parameters reflect the requirements imposed bythe application, and can be stored in pre - defined use r profiles containing the QoS constraints imposed on the behaviour of the application or can be obtained bythe application through direct interaction with the user.

The achievement of the specified level of QoS is typicallymade possible through the rese rvation of the resources managed bythe underlying system that are necessaryto provide the network and operating system services used bythe application with the requested level of quality. These resources include network bandwidth, processing time, physi cal memory, and access to multimedia hardware.

Several operating systems and network protocols incorporate mechanisms that allow applications to retain resources for their exclusive use. These mechanisms, called resource reservation protocols, are the key elements that support the provision of QoS guarantees. Unfortunately, most applications do not benefit from these mechanisms because the distributed computing middleware on which theyrelyis still being adapted to make use of such mechanisms. Furthermore , multiple resource reservation protocols coexist in open systems. Consequently, allowing applications to reserve resources via a middleware layer implies that the differences between reservation protocols have to be handled bythe middleware.

Middleware c omponents, usuallyreferred as QoS architectures, are responsible for providing mechanisms for specification and enforcement of QoS that make use of the resource reservation protocols provided bythe underlying system. QoS architectures deal with issues su ch as the translation of QoS parameters comprehensible at the application - level into the parameters understood bythe underlying reservation protocols that control access to the resources provided bythe system. Without the services provided bya QoS archi tecture, these issues would have to be dealt with bythe application.

Research on QoS architectures has resulted in several proposals that can be found in the literature (see [4] for a surveyand [139] for an analysis of the open issues in this area of research). During an extensive surveying of the area, four main limitations that prevent the use of the existing QoS architectures in open systems have been identified byus.

These limitations are:

· mo st architectures require QoS to be specified byusing a low - level format that is not appropriate for applications with a more high - level notion of QoS, or use a format appropriate for a specific area of application, limiting the use of the architecture;

· Q oS enforcement often occurs at either network or operating system level, instead of both, and in some cases the underlying system is not made completely transparent for the application, which still has to deal with low - level issues;

· the use of most archit ectures in open, heterogeneous systems is prevented due to their close integration with the underlying system; and

· most QoS architectures ignore the possibilityof dynamic resource adaptation, which can occur due to factors such as resource failure or syst em reconfiguration.

Bysolving the limitations described above we would have a QoS architecture that, besides handling the complexitythat originates from the necessityof obtaining QoS - constrained services from the underlying platform on behalf of applica tions, would make applications easier to implement and would increase their portabilitybetween different underlying platforms. In addition, this QoS architecture would allow application programmers to use the same high - level interface for specifying QoS r equirements for applications inserted in different application contexts and making use of different networking infrastructures and operating systems.

1.2 The Quartz QoS Architecture

In this thesis we propose a generic architecture for the specification and enf orcement of

QoS in open systems. This architecture provides mechanisms necessaryfor building applications with QoS requirements in open systems, since the QoS architectures currentlyavailable are typicallydependent on a specific underlying system and ar e useful onlyin limited application contexts. Besides, theyoften expose the application to lower - level details and ignore the need of support for resource adaptation. These characteristics tend to limit the application portability, make them more difficu lt to implement, constrain the wayapplications express their QoS requirements, and prevent their use in open, heterogeneous systems.

The Quartz QoS architecture provides support for different application fields and is able to interact with the multiple r esource reservation protocols that maybe available in an open environment. This is achieved byadopting a flexible and extensible component - based design. The design of Quartz is based on a common core in which components are plugged in order to handle the particular characteristics of different applications and resource reservation protocols.

The Quartz QoS architecture allows users to specifytheir QoS requirements according to the notion of QoS present at the application level (e.g. requesting audio wit h CD qualityinstead of specifying the bandwidth needed to transmit the encoded audio over the network). This information is interpreted byQuartz, allowing it to perform resource reservations at a lower level of abstraction in order to fulfil the QoS requ irements imposed bythe application. No strong assumptions are made about the characteristics of the lower - level system, therefore allowing the deployment of the architecture on top of heterogeneous systems with different resource reservation capabilities.

The architecture, furthermore, supports resource reservation protocols that allow the availabilityof resources to changes dynamicallydue to factors such as resource failure, hardware reconfiguration or mobility. This is achieved through the use of reso urce adaptation techniques. Adaptation mayoccur at system level and be masked from the application, or mayrequire the application to be notified in order to adjust its QoS requirements.

QoS enforcement and QoS adaptation at system level occur in a transp arent manner from the application´s point of view. Consequently, the application need not be aware of the resource reservation protocol used at the lower level. Despite providing transparency, Quartz allows the application to control the behaviour of resou rce reservation protocols whenever necessary, and notifications are sent to the application when the requested QoS requirements cannot be fulfilled.

1.3 Contribution

The Quartz QoS architecture provides a combination of features that are not present in other proposals of QoS architectures that are found in the literature.

One of the main features provided byQuartz is the possibilityfor applications to specify their QoS requirements according to their own notion of QoS. Being generic, Quartz does not require QoS to be specified in a standardised format, which would likelybe unsuitable for a wide range of applications. Instead, Quartz allows the application to specifyits QoS requirements byusing its own notion of QoS, and employs a component that is able to interpret this information and convert it into the format that is used internallybyQuartz. The internal format of QoS parameters used byQuartz is completelytransparent to the application.

Quartz is also able to carryforward the translation of the Qo S requirements specified by the application into a format that is suitable for performing resource reservation using the protocols provided byboth the network and the operating system. During this process, QoS requirements are mapped into resources provid ed bythe underlying system, which are then reserved in order to enforce the requirements of the application.

Since network and operating system resources maybe interchangeable, a balancing process has to be performed bythe architecture at this point.

Q uartz provides support for resource adaptation to occur at the lower level. Adaptation is handled byrearranging the balancing of resources internallyor, when this is not feasible, byinforming the application that its QoS requirements cannot be fulfilled and have to be adapted if theyare to be satisfied with the resources that are currently available.

Due to its component - based design, Quartz is able to support multiple resource reservation protocols and application areas. The differences found in the su rrounding environment are handled byplugging new components into the architectural core. These components can be selected from a libraryor provided byapplication developers, who are, therefore, able to extend the architecture according to their particul ar needs.

Furthermore, application simplicityis increased bythe use of Quartz. Byhandling the

QoS - related issues on behalf of the application, Quartz allows the programmer to concentrate on the functional aspects of the application. Due to its capacity to handle the differences between multiple resource reservation protocols present in heterogeneous platforms, Quartz also increases the portabilityof applications.

1.4 Analysis

We have implemented a prototype of the Quartz QoS architecture in order to evaluat e its behaviour and validate its applicabilityin open systems and in different application scenarios. Some test applications that make use of Quartz have been written, including a complete framework for the development of multimedia applications that inte grates

Quartz into a CORBA - based environment.

The Quartz prototype and the applications built on top of it allowed us to conclude that the architecture fulfils the goals imposed on it during the design process. In order to evaluate the achievement of thes e goals, we have:

· Implemented applications inserted in different application contexts and that consequentlyhave different ways of expressing their QoS requirements; Quartz has been shown to be able to interpret this information and identifythe resources that have to be allocated in order to fulfil the requirements of the application.

· Observed through the application examples implemented byus that the QoS requirements of the application are enforced byQuartz through reserving resources provided byboth the network and the operating system; in addition, regardless of the resource reservation protocols in use, the process of resource reservation was shown to become transparent to applications built on top of Quartz.

· Used multiple resource reservation pro tocols for reserving resources for the same application, without the necessityof rewriting the application code that specifies its

QoS requirements, showing that Quartz is able to handle the differences between different underlying systems without anysid e - effects for the application.

· Simulated the occurrence of dynamic resource adaptation and observed that Quartz is able to perform QoS adaptation in order to reflect the new distribution of resources; this process occurs either transparentlyat system leve l byrearranging the balance of interchangeable resources, or bynotifying the application to perform adaptation of its QoS requirements when adaptation at system level is not feasible.

In addition, with the experience obtained bywriting applications tha t make use of

Quartz, we have noticed an increase in their portabilityand the simplicityof their code, since the differences between underlying platforms are handled bythe architecture.

Performance measurements have shown that the impact caused byQuart z on the overall performance of applications that use it to specifyand enforce their QoS requirements is verysmall. We believe that this small overhead will be accepted byapplication programmers that can benefit from the services provided bythe Quartz architecture.

We have also analysed the characteristics of Quartz in the light of other work in the area of QoS architectures and frameworks. To the best of our knowledge, there is no QoS architecture that combines a similar set of features. Most architect ures found in the literature are able to provide a similar set of features but are highlydependent on a particular platform. In general, their mechanisms for specification of QoS are not flexible enough to support a wide varietyof applications, forcing t hem to deal with a notion of QoS that is not suitable for their needs. Quartz, on the other hand, is able to provide efficient tools for specification and enforcement of QoS in open systems, which are intrinsicallydistributed and heterogeneous, and still fulfil the needs of diverse areas of application due to its extensibilityand flexibility.

1.5 Roadmap

The remainder of this thesis is organised as follows. Chapter 2 provides some necessary background to the thesis and presents the technologycurrentlyavail able in the area.

Chapter 3 describes the state - of - the - art work developed in the areas of middleware for distributed multimedia and QoS architectures, analysing their characteristics and limitations. The Quartz architecture is introduced and described in d etail in Chapter 4.

Chapter 5 describes a prototype implementation of Quartz, and Chapter 6 shows how this prototype can be used together with CORBA in order to provide a framework for the development of multimedia applications. Chapter 7 presents a comple te validation and evaluation studyof the Quartz architecture, introducing examples of applications that demonstrate the suitabilityof the architecture as a tool for obtaining QoS - aware services in open systems. Finally, Chapter 8 presents some conclusion s, summarises the contributions of this thesis and unveils some opportunities for future work in this area.

2

Overview of the

Research Area

This chapter provides some background on the area of research with which this thesis is concerned. The following sections introduce the keyconcepts and technologies present in the areas of multimedia and real - time applications, open systems, distributed object computing, qualityof service and resource reservation protocols.

The technologies used byus for implemen ting a QoS architecture and a multimedia framework, which will be presented in chapters 5 and 6 respectively, are also described in detail. These technologies include the Common Object Request Broke r Architecture

(CORBA), Asynchronous Transfer Mode (ATM), the new generation of Internet

Protocols, with special attention to the Resource Reservation Protocol (RSVP) and the real - time capabilities provided byWindows NT.

The technologies described in thi s chapter are seen as important tools for building an environment for QoS specification and enforcement in open systems such as the one targeted bythis thesis.

2.1 M ultimedia Applications

Interactions between computers and other processor - based equipment are based on the exchange of data represented byelectrical signals. This data follows a well - defined encoding scheme that represents some kind of information (e.g. a text file might be encoded using the ASCIIcharacter set, or a compressed file might be encod ed in zip format). However, computer systems are evolving towards becoming not only responsible for handling computer data, but also media such as audio, video and animated graphics.

Media data is represented using digital encoding schemes as is other dat a, although the characteristics of multimedia data distinguish it clearlyfrom regular computer data.

Multimedia typicallyrequires a higher amount of data to be processed and transmitted, presents a higher complexityto encode and decode, and often requir es that time and synchronisation rules are obeyed during reproduction [53] .

Multimedia systems are able to handle multiple kinds of media data in order to support multimedia applications, i.e. programs that, often employing spe cial hardware, are able to encode, transfer, decode and reproduce multimedia data. During the last few years a rapid growth in the demand for multimedia applications has been observed.

Nevertheless, the performance of these applications is still poor due t o limitations in processing power and, in the distributed case, due to limited network bandwidth.

Hardware support for multimedia is increasing fast. Almost everydesktop computer sold nowadays comes with some sort of support for multimedia. Devices such as sound cards, 3D graphics accelerators and digital cameras are becoming more common every day. The latest generations of processors include special instruction subsets designed to improve the performance of media processing (such as Intel´s MMX) and for rendering

3D graphics (such as AMD´s 3D Now!) [120] .

Moreover, a fact that has to be taken into account when studying multimedia applications is the increasing popularityof portable devices, inexpensive gadgets that are small enough to fit in a pocket. Devices such as laptop computers, cellular phones, pagers, and video games are now converging into a single unit, called a personal digital assista nt (PDA) or palmtop computer. Users are likelyto expect to have the same functionalityon these devices as theyhave on their desktop computers. This leads to greater demand for computing power, but at the same time, the size, weight, and power consumptio n of these devices must remain limited. For example, these devices are typicallythe size of a cigarette pack, weigh from 150 to 300 grams (4 to 8 ounces), have only2 to 8 Mb of memory, and are expected to run on the same set of batteries for about a week [85] . Complete operating systems (such as Palm Computing´s PalmOS

[117] and Microsoft´s Windows CE [17] ) provide a fullyfunctional platform for the execution of common software applications such as text editors, e - mail readers, web browsers and personal information managers (PIM). A complete networking infrastructure based on modems and infrared communications is also provided for such devices, but complete support for multimedia is still being introduced.

Another important factor that influences multimedia applications is network performance. The networking infrastructure currentlyavailable for the typical end - user

(i.e. local area networks such as Ethernet and person al computers with modems interconnected bythe Internet) satisfies the common needs of most network applications.

Applications such as Web browsing and chatting require low bandwidth and can even tolerate some degree of network congestion. On the other ha nd, multimedia applications demand higher bandwidth and behaviour in the distribution of network resources that is not provided bythe networking infrastructure in place at the present. Solutions for this problem have started to emerge in the form of reser vation protocols (discussed in

Section 2.6 ) and middleware with support for QoS specification and enforcement (such as the proposals introduced in Chapter 3 ), but the application of these solutions is yet to reach most users [141] .

2.1.1 Distributed Multimedia

Distribution is yet another fact that has to be considered in the studyof multimedia applications. Due to the interactive nature of some multimedia applications, informa tion has to be exchanged through the network, characterising them as distributed multimedia applications.

Distributed multimedia applications have well - defined requirements based on the characteristics of the kind of media that is to be transmitted. Besid es, the technique used for transferring media has to be taken into account. Some kinds of pre - produced media, such as short movies, songs or news reports, have less strict timing requirements than other categories of media. This is because pre - produced med ia can be buffered after transmission and reproduced onlywhen available locally. On the other hand, live media and long video streams that are reproduced while theyare still being transferred through the network require the media transfer and rendering p rocess to be more predictable than that obtained in best - effort systems. This last class of media, which is called continuous media, is discussed in detail in the next section.

2.1.2 Continuous Media

In the face of increasing interest in the transmission of digi tal media over computer networks, the usual communication mechanisms adopted for data transmission have been shown to be unsuitable in some particular cases. This unsuitabilityderives from the distinct characteristics of continuous media.

Continuous medi a can be defined as media where there is a timing relationship that must be observed during the rendering of the media in order to reproduce it correctly.

This timing relationship must be followed otherwise the integrityof the media is destroyed, i.e. the information that was intended to be presented can be lost or misunderstood [132] . In the particular case where media is transmitted over the network and reproduced at a different location, this implies that the destination mus t reproduce the timing relationship that existed at the source. This contrasts with the usual approach adopted for data transmission in which information is usuallyretrieved and delivered upon request. This kind of media does not have an implicit temporal dimension, and is also termed discrete media. The required bandwidth for discrete media depends on the nature of the task to be accomplished, ranging from a couple of bits per second in case of simple sensors, to verylarge volumes of data if we consider a world - wide banking system or a massivelydistributed file system. The acceptable delayis also related to the application, being for example verysmall in manufacturing and control systems and more relaxed in an airline reservation system or an FTP sessi on. Traffic is usually burstyand the timing relation present at the origin typicallydoes not need to be reconstructed at the destination. The reliabilityof data is generallya critical factor in all of these systems.

The requirements of different kinds of continuous media can be classified according to the following parameters:

· Bandwidth required;

· Acceptable end - to - end transmission delayand delayvariation (jitter);

· Transmission reliability(data loss);

· Distribution of traffic during time (burstiness or bit - rate distribution);

· Importance of keeping the original timing relation during the reproduction of media.

In the following paragraphs we analyse different classes of continuous media according to these parameters. In sequence, Table 1 provides a comparison of the bandwidth required bytypical encoding schemes of different classes of continuous media.

Audio. Audio is usuallyencoded as a constant bit - rate (CBR) signal in the majorityof communication systems currently available. However, digital techniques have been adopted to allow compression of audio with verylow loss of quality, resulting in variable bit - rate (VBR) traffic. Compression techniques based on data redundancyand forward prediction are difficult to app lyfor audio, and as a consequence compression algorithms for audio usuallyhave a lower efficiencyif compared to compression algorithms for video. The reproduction of audio with reasonable qualityis basically related to the sampling rate and the number of bits used to represent the signal in a digital stream. The frequencyrange is limited bythe capacityof the human ear, limiting the number of bits needed to encode the signal and the bandwidth necessaryto transfer it through the network. Furthermore, the original timing relationship observed during the generation of the sound must be reproduced at the destination. Some data loss can be tolerated byaudio applications, and delayand jitter can be compensated byusing buffering techniques.

Voice. The hu man voice, despite being a particular categoryof audio, must be studied separatelydue to its importance in communication systems. Voice requires low bandwidth when compared with full audio signals because of its limited frequency range and the low sampli ng rate necessaryfor its comprehension. In addition, voice media is sensitive to delayand delayvariations, but a delayed sample maybe discarded without serious loss of comprehension bythe listener. Apart from the lower bandwidth necessaryfor voice me dia, its traffic characteristics are verysimilar to those of audio signals. Voice can also be encoded as CBR or VBR signals, and compression is usually more efficient than for other categories of audio because of the presence of silent periods.

Video. A v ideo signal can be encoded digitallyas CBR or VBR data, depending on the method used to encode it. The bandwidth required is veryhigh when compared with other sorts of media, and increases considerablywhen slightlybetter resolution is desired. If we co nsider the capacityof the human eye, a rate of 30 frames per second is sufficient to allow a comfortable sensation of movement. The loss of one frame in a long sequence is usuallynot perceptible, and delayed frames need not be exhibited. A low delayvari ation is tolerable, and the reconstruction of the timing relation present at the source time during rendering at the destination must be carried out. Like for audio, delayand jitter can be compensated byusing buffering techniques.

Media Description Band w idth

Voice Low quality (4 bits/sample; 8 kHz sample frequency) 32 Kbps

Phone quality (8 bits/sample; 8 kHz sample frequency) 64 Kbps

Audio CD quality (16 bits/sample; 44.1 kHz sample frequency) 1.4 Mbps

MPEG audio with approx. CD quality 200 to 300 Kbps

Video VHS quality (352x240pix;24bits/pix; 30 frames/s) 60 Mbps

MPEG video with approx. VHS quality 1.5 to 2 Mbps

Pal/Secamquality (544x480pix; 24bits/pix; 30fr/s) 188 Mbps

MPEG video with approx. Pal/Secamquality 4 to 6 Mbps

HDTV quality (~ 1200 lines; 24bits/pix; 30fr/s) 1 Gbps

MPEG video with approx. HTDV quality 20 to 60 Mbps

Table 1 ˘ Typical Bandwidth of Different Classes of Continuous Media

2.1.3 Multimedia Technology

There is currentlya major research effort bei ng carried out on the development of distributed multimedia systems and platforms. Unfortunately, most proposals do not adopt an approach that allows them to handle media in open systems.

Standards for distributed multimedia such as the Multimedia System Services (MSS)

[67] that was proposed bythe International Multimedia Association (IMA) have started to emerge. MMS has as its main purpose to provide support for interaction between multimedia applications in open environments . IMA members include the main software and hardware suppliers and consumers around the world. MSS, as a reference model for design and programming of distributed multimedia applications, is targeted at complex, scaleable, extendible and interoperable appl ications running in an open environment. Being just a reference model, MSS does not specifyhow the multimedia services are obtained from the system.

Another proposal in this area is the MHEG standard [95] , defined bythe Mult imedia and Hypermedia Experts Group (MHEG) of the International Organisation for

Standardisation (ISO). Like MSS, MHEG still does not provide a complete solution for supporting multimedia applications with QoS requirements in open systems since it is basic allya reference model.

Some software development kits such as Microsoft´s DirectX [98] and the Apple

QuickTime architecture [2] consist in useful solutions for the development of multimedia applic ations. However, these technologies lack mechanisms for QoS specification and enforcement, and have limited platform coverage.

A series of state - of - the art proposals of support for multimedia programming will be presented in chapter 3 , but these frameworks and architectures still lack complete support for QoS specification and enforcement in open, heterogeneous systems.

This thesis aims to provide mechanisms in order to overcome the limitations found in supports for the develop ment of multimedia applications. Further in this thesis we will introduce a QoS architecture that is used in a media streaming framework. This framework provides support for the development of multimedia applications with QoS requirements in open systems.

2.2 Real - Time Applications

Real - time systems include those responsible for the control of manufacturing plants, aircraft, nuclear plants and so on. Most of these control applications must avoid critical failures that can lead to catastrophic errors, in which the occurrence of an error can be much more damaging than the benefit provided bythe system. For example, a plane crash is much more damaging for an airline than the completion of a flight safely.

Furthermore, real - time data is not considered valid onlyb ybeing semanticallycorrect.

A delayin the provision of a data item can be much more damaging than the provision of an inaccurate value. So, real - time data must not onlybe semanticallycorrect, but also timelycorrect (i.e., the data must be available w hen it is required bythe system).

Like multimedia applications, real - time applications are not satisfied bybest - effort networking and processing policies. Real - Time applications are time critical by definition, and cannot tolerate unpredictable variation s in the behaviour of the system without the possibilityof causing catastrophic errors.

So far, real - time systems have been isolated from external influence byusing special software and hardware designed for this purpose. However, aiming to reduce costs and simplifymaintenance, real - time systems are evolving towards a more open approach, in which real - time data would flow side byside with non - real - time traffic. In this case, a complex approach for avoiding interference between the two classes of traffi c must be adopted.

Real - time applications typicallyrequire less bandwidth than multimedia applications.

The transfer of the encoded data read bya temperature sensor mayaccount for just a few bytes, for example. However, this data maybe required to acti vate alarms that will prevent a fire, and is therefore of more importance for network transmission and processing than other information that is being transferred through the network and processed bythe same computational system.

Research on real - time sy stems has focused mainlyon two areas of research:

· Real - time operating systems, languages and middleware [23] [122] , which provide mechanisms for implementing real - time applications; and

· Real - time sc heduling algorithms [3] [83] , which select the order of execution of the activities performed bythe system based on priorities and deadlines associated to them.

Despite the solid knowledge obtained with intense research in the area of real - time systems, the techniques employed for supporting real - time computing do not integrate gracefullywith the technologycurrentlyavailable for best - effort applications. The integration of these technologies has e merged as an important research topic, and constitutes a challenge for scientists in this area of research.

2.2.1 Real - Time Technology

Current real - time platforms are mainlyfocused on embedded hardware and specialised software. Several successful real - time env ironments for embedded systems can be found in the literature and commercial, off - the - shelf solutions can be found in the market.

One of the most influential experimental real - time environments originated from the

MARS project [84] , developed at the Universityof Vienna. MARS provides tools for the analysis and deployment of hard real - time systems. Its architecture employs redundancywith self - checking procedures for enabling fault tolerance, including a redundant network bus. At the software level, the MARS real - time operating system

(O.S.) provides tools for the analysis of worst - case execution times and static (prior to execution) real - time scheduling. Communication is based on the time - triggered protocol

(TTP), which provide s a predictable, fault - tolerant communication system.

In the field of commercial products for real - time systems two products share the status of market leaders: QNX Software Systems´ QNX real - time O.S. [62] and WindRiver´s

VxWo rks [151] . Both are microkernel - based, extensible, and POSIX - compatible operating systems, and can be scaled up or down according to the necessities of the target system. Another product with a strong presence in the market is the Chorus O.S.

[ 142] , developed byChorus Microsystems, now a division of Sun Microsystems.

Chorus OS provides real - time guarantees such as QNX and VxWorks, and offers a very rich set of tools for developing and testing real - t ime applications.

Despite the common use of real - time operating systems in embedded environments, the possibilityof their integration with open systems is somewhat limited. Research in this field has been divided into two directions: the integration of r eal - time capabilities into commercial operating systems and the provision of communication paths between real - time and non - real - time operating systems.

Operating systems such as Sun´s Solaris 2.X and Microsoft´s Windows NT provide a set of mechanisms that allow real - time activities to be performed. The approach adopted in both cases encompasses a real - time scheduling class which has priorityover the regular activities performed bythe system. In addition, these operating systems provide mechanisms that sup port higher predictabilityin the execution of code byreducing interference caused bymemorypaging, I/O operations and interrupts.

On the other hand, software vendors are starting to provide communication paths between embedded real - time software and app lications running on non - real - time operating systems. Iona Technologies provides implementations of its CORBA - compatible Orbix ORB for VxWorks and QNX. Chorus has its own implementation of

CORBA, called COOL(Chorus Object - Oriented Layer), which provides a communication path between non - real - time ORBs and applications running on top of the Chorus O.S..

The technologyavailable in the area of real - time systems is still verylow - level for the application programmer, and its close integration with the computin g platform limits its use in open, heterogeneous systems. One of our goals in this thesis is to provide middleware with mechanisms for the specification of real - time requirements. These mechanisms would hide the complexitypresent at the low - level from the programmer of real - time applications, and would allow these applications to interact with different low - level supports through the middleware. This middleware, which will be described further in this thesis, allows not onlyreal - time applications but also other applications with timing constraints (such as multimedia applications) to specifytheir constraints in the form of QoS parameters, which are then enforced bythe QoS mechanisms provided bythe middleware.

2.3 Open Systems

Computational systems are said to be ^open~ when theyallow external components to take part of the computation byusing a well - known interface. Byspecifying their interfaces, software components are allowed to interoperate with their peers, independentlyof the vendor that provides th e component [38] .

The concept of open systems implies that distribution and heterogeneityare key characteristics in these systems. Distribution originates from the fact that a program is not constrained to a single machine o r address space, but can communicate through the network with other software elements. Heterogeneityis present because programs can be written in different languages, and run on different operating systems built on top of different computer architectures, but can still interoperate via standardised interfaces to other software.

The heterogeneityof hardware and software and the complexityof developing distributed applications to run on top of systems with the characteristics mentioned previouslyrequire the use of open computing architectures.

A keyrequirement in open architectures is to provide the programmer with mechanisms to support distribution and heterogeneitytransparencyso that the handling of these issues is simplified. These mechanisms inclu de standard services that are needed by applications in an open environment, such as naming and location services, and a standardised communication mechanism that allows software to communicate with each other. In addition, mechanisms for describing, stori ng and retrieving the interface of a component must be provided in order to allow software to know how to contact their peers.

2.3.1 Open Systems Technology

Middleware providing support for open systems, which make the intrinsic distribution and heterogeneitypr esent in open systems transparent to the application, is widely available and used byprogrammers nowadays.

Reference models such as the ISO Open Systems Interconnection [68] and Open

Distributed Processing [69] models represent an important contribution to this area of research at a theoretical level. However, the most important step for the proliferation of support for open systems was the wide adoption of products based on standards such as

OSF D CE [114] , Microsoft´s DCOM [97] , and OMG´s CORBA [108] . These products allow distributed programs to interact in open environments in order to carryout cooperative task s. This is done byproviding a standard wayof specifying the interfaces supported byprograms, describing the routines (or methods in object - oriented systems such as CORBA and DCOM) that can be called remotelyand their respective parameters. In addition, a communication protocol that allows client programs to remotelyinvoke the routines supported byother programs acting as servers is defined byeach of these standards.

Despite the wide availabilityof standards for open distributed environments, and des pite the intense research efforts focused in this area, the integration of multimedia and real - time support into middleware for open distributed systems is a problem that still lacks a satisfactorysolution [31] [141] . We intend to overcome this deficiencyby proposing an architecture that provides support for the specification and enforcement of the requirements present in multimedia and real - time applications built in open, heterogeneous and distrib uted systems. This architecture will be described in detail further in this thesis.

2.4 Distributed Object Computing

In the last decade the development of software, which was typicallybased on the use of structured design and procedural languages, has rapidly migrated towards the adoption of object - oriented design and programming techniques. Procedural programming languages such as C and Fortran are being replaced byobject - oriented languages such as C++ and Java. Meanwhile, modelling tools that employobject - oriented design, especiallythe tools that are based on the Unified Modelling Language (UML) [22] , have been widelyemployed byprogrammers for the analysis and design of object - oriented software.

The adoption of object - based a pproaches to distributed computing that occurred subsequentlywas a natural evolution. The use of object orientation in distributed systems was further reinforced bythe introduction of standards for interaction between distributed objects.

In a distribute d object environment, objects are used to represent parts of the computation that maybe running on different machines dispersed over the computer network. These objects interact with each other in order to execute cooperative computation. Interaction betw een objects occurs in the wayof remote object invocations, i.e. bycalling methods on remotelylocated objects. To allow remote invocation, a remote object has to know the interface of the target object and call one of its methods, passing the parameters of the call and possiblyreceiving a return value.

Moreover, remote objects can be written in different languages and run on different platforms. In order to allow interaction between different remote objects a common invocation model must be agreed upon.

The interfaces of an object can be specified at different phases of its lifetime:

· Statically: i.e. at compile time, bydescribing the interfaces supported bythe object using an Interface Definition Language (IDL); or

· Dynamically: i.e. at run - time, byavai ling of metadata obtained directlyfrom the object or through an interface repository.

Invocation models have to specifycommunication protocols and message formats to be used for calling methods remotely. An invocation model can support one or more calli ng semantics. Three well - known types of calls classified according to calling semantics are:

· Synchronous calls: block waiting for the target object to conclude the processing of the call and send the result of the operation;

· Asynchronous calls: non - blockin g, with the execution of the caller continuing right after the call is dispatched through the network; and

· Deferred synchronous calls: asynchronous call with the possibilityof a posterior synchronisation, in which the result of the operation can be retrie ved.

Distributed object computing models are supported bymiddleware, which hides the complexityresulting from network communication, handling of network addresses, conversion between data formats and so on. Distributed object middleware provides the pro grammer with powerful tools for the development of distributed applications.

2.4.1 CORBA

With the widespread adoption of object - oriented design and programming techniques for application development, it was natural that this approach reached the area of distrib uted computing. The adoption of object - based approaches in distributed systems was reinforced bythe availabilityof standards proposed bythe Object Management

Group (OMG), a consortium created bysoftware vendors, developers and end - users to promote obje ct technologyfor the development of distributed computing systems.

The OMG has proposed a set of standards for distributed object computing, which compose the Object Management Architecture [105] . The OMA is a framework of st andards and concepts for open systems, centred in the Object Request Broker (ORB).

In this architecture, methods of remote objects can be invoked transparentlyin a distributed and heterogeneous environment using the services provided byan ORB.

The Common Object Request Broker Architecture is the standard ORB defined bythe

OMG [108] . The CORBA specification establishes the role of each component of the

ORB and defines their interfaces. Byintroducing a common architecture, the OMG makes transparent for applications the differences between distinct CORBA implementations and lower - level systems. The components of the CORBA architecture are shown in Figure 1 .

ORB Co re

IDL St ubs

Dynamic

Invocation

Int erface

ORB

Int erface

IDL

Skeletons

Dynamic

Skeletons

Object

Adapter

                                                                                                                     Cl ient Object  Implementat ion

Figure 1  ˘  The CORBA Architecture

In the CORBA environment, each object implementation has its interface specified in

IDL (Interface Definition Language). Remote method invocations are issued by clients
calling methods in local stub objects that are  generated by the IDL compiler and have
the same interface as the corresponding remote objects. Alternatively, the client can
build the request using the Dynamic Invocation Interface (DII). The ORB Core
transmits the request and transfers the control to th e object implementation (i.e., the
server) using an IDL skeleton and the corresponding object adapter. The object
implementation is unaware of the invocation method used by the client to issue the
request.

Dynamic skeletons allow servers to receive calls o n methods that are not specified in
their IDL interfaces, and therefore are not accepted by the IDL skeleton supported by
the object. The dynamic skeleton interface (DSI) is usually adopted to build gateways.

The ORB Interface offers some general - purpose s ervices to CORBA objects through a
well - defined interface. Object implementations can also use services provided by their
corresponding object adapters. OMG specifies the interfaces of a general - purpose Basic

Object Adapter (BOA) which covers the requireme nts of a wide range of object
systems. However, this does not prevent object adapters with more specialised
capabilities being added to the support in order to fulfil the needs of applications with
requirements that are not covered by the BOA.

When the cl ient and the object implementation are located in ORBs that use different
protocols for remote communication, a communication protocol called IIOP (Internet

Inter - ORB Protocol) is used to allow interoperability. In addition, the OMG has
approved mappings o f the IDL interfaces for the main programming languages in order
to allow objects written in different languages to interoperate.

CORBA has become a de facto  standard for distributed object computing. Several
legacy applications in sensitive areas such as banking and telecommunications have
been ported to CORBA platforms, and new applications have been built based on

CORBA in order to obtain easy interoperability with other applications.

2.4.2  CORBAservices

The CORBA Services Specification [107]  intends to provide the OMA architecture and

CORBA with a set of standard mechanisms that are often necessary in a distributed
environment.

In particular, the following services of major importance to distributed systems were
proposed by the O MG:

·

                         a Naming Service;

·

                         a Life Cycle Service;

·

                         an Event Service;

·

                         a Transaction Service; and

·

                         a Security Service.

Naming Service.  A naming service allows components to discover other components in
the distributed environment with which they can interact and execute cooperative tasks.

It is basically a location service that associates identifiers to handles (i.e. references)
that provide a way to contact the desired component in the distributed system.

The CORBA Naming Service binds names, inserted into hierar chically organised name
contexts, to CORBA objects.

Life Cycle Service.  A life cycle service is basically a configuration service. It defines
services and conventions for creating, deleting, copying and moving components in a
distributed system.

The CORB A Life Cycle Service defines the interface to a `Factorý object that allows
the creation of objects using factories, as well as a `LifeCycle´ interface with remove,
copy, and move operations.

Event Service.  An event service implements a decoupled communic ation model, based
on the publish/subscribe paradigm. In this communication model, one or more
publishers (or suppliers) can send messages related to a specific topic, while a group of
subscribers (or consumers) receive the messages asynchronously. Through  this
mechanism, suppliers can generate events without knowing the identities of consumers,
and consumers can receive events without knowing who supplied them.

The CORBA event service is used by applications whose interaction model can be more
easily model led as events than as method invocations. Despite providing a useful
alternative to the traditional invocation mechanism implemented by CORBA, the event
service cannot be used by applications with constraints on the latency of events. In order
to overcome this limitation, the OMG has introduced the notification service [11] , an
extension of the event service that allows QoS constraints to be associated to events.

Transaction Service.  A transaction service organises interactions  between distributed
objects establishing delimiting transactions and commitment points. The CORBA
transaction service not only supports multiple transaction models, but it also allows
interoperability between different transaction models.

Security Service .  A security service controls identification of human or software
entities in order to verify that they have authorisation to execute a requested action. The

CORBA security service allows identification and authentication of distributed objects
and impleme nts access control, in order to verify if a particular entity has authorisation
for calling a specific operation (method) of an object. Furthermore, it allows secure
communication over insecure network links, with protection of the integrity and
confidenti ality of messages transferred between objects.

Additional Services.  In fact, a complete set of services useful in some specific
applications was defined by OMG. Other important services are:

·

                         Time Service: supplies time information and allows the definition  of periodic (i.e.

                         recurrent time - triggered) calls.

·

                         Licensing Service: controls the utilisation of specific objects in the distributed

                         system, inhibiting improper use of intellectual property.

·

                         Properties Service: provides the ability to dynamically associa te properties (any IDL

                         value) with objects.

·

                         Relationship Service: allows the definition of relationships between CORBA

                         objects.

·

                         Query Service: allows users and objects to invoke query operations on collections of

                         objects.

·

                         Persistency Service: provides mech anisms used for retaining and maintaining the

                         state of persistent objects.

·

                         Concurrency Control: allows the co - ordination of multiple access to shared

                         resources through the provision of several lock modes, and permits flexible

                         resolution of access conflicts .

·

                         Externalisation Service: defines conventions and protocols for representing state

                         information related to an object in the form of a stream of data, allowing this

                         information to be stored or transferred to other locations.

2.4.3  CORBA A/V Streams

Despite its ad equacy for transmission of best - effort data, CORBA, like its counterparts,
originally did not have support for streaming continuous media. The immediate solution
for the implementation of multimedia applications would be the use of CORBA for
transmission o f control data, while the stream data would have to be transferred using a
lower - level network protocol that provides mechanisms for QoS specification or
resource reservation. However, it is not reasonable to use high - level middleware to
provide protocol a nd distribution transparency for transmitting best - effort data, and on
the other hand expose the programmer to the lower - level protocols used for
transmission of stream data.

It is highly desirable that distributed object middleware provide the same kind of high -
level abstraction, which is available for best - effort data, to deal with continuous media.

To make CORBA suitable for continuous media, OMG has defined streaming
mechanisms to be introduced at application level in the CORBA architecture [109] .

The CORBA streaming mechanism defines a set of abstractions to deal with stream data
in multimedia systems. These abstractions are illustrated by Figure 2 .

Flow

Stream

Control

Stream

Endpoint

Flow

Endpoint

                                 Vi rt ual

                                  Device

Stream

Endpoint

Flow

Endpoint

Vi rt ual

Device

Object Request B roker

                                                                             Figure 2  ˘  Overview of the CORBA A/V Streams Mechanism

Virtual device objects abstract multimedia devices (i.e. cameras, speakers, etc) used by
multimedia applications. A stream control object allows the user to control the media
flow (i.e., start a nd stop it) as well as add and remove parties from a multi - party
connection.

Stream endpoints transfer stream data through the network, getting data from and
delivering data to virtual devices. Each endpoint has one or more media flows, which
are abstract ed as flow endpoint objects located at each end of the flow. Flow endpoints
are classified as producers and consumers according to the role performed by them in
the transfer of data.

A binding operation establishes a stream between two virtual devices and defines the

QoS parameters associated to the stream. Two binding semantics are allowed. The
simple local binding uses the virtual device and returns a stream control object. Besides,
in the third - party binding mechanism, a stream control object can bind tw o remote
virtual devices and keep control over the data flow.

A set of QoS parameters for audio and video streams is defined by the specification (for
example, the number of bits per sample and the number of channels for audio, or the
resolution and the c olour depth for video). The QoS parameters associated with a stream
can be modified through the stream control object, through the stream endpoint or
through individual flow endpoints.

Figure 2  shows an application scenario in whi ch a video streaming application is built
using the CORBA  streaming mechanism. The image generated by a video camera is fed
by a virtual device to a flow producer, which establishes a connection with the flow
consumer and then feeds the virtual device asso ciated to the video screen with the image
produced by the camera. The characteristics of the media stream, i.e. the number of
flows of audio and video and the QoS parameters associated to them, are specified when
the devices are bound. The stream endpoint handles the network connection between the
two or more partners, and the control of the media flow and of the membership of the
connection is done through the stream control object.

With the introduction of the stream mechanism, the CORBA architecture beco mes
suitable for the provision of the communication services necessary for multimedia
applications, and can be adopted as the common middleware for control and  transfer of
media. However, the mechanisms used for QoS enforcement are not defined by the

CORBA  A/V streams specification. In order to solve this deficiency, this thesis
proposes middleware that provides QoS mechanisms that, when integrated with

CORBA, can provide a full framework for the development of distributed multimedia
applications.

2.5  Quality of Service

Despite the evolution of computer hardware, resources such as network bandwidth,
processing time and memory are becoming scarce because of the complexity of a
special category of applications. We are experiencing the proliferation of application s
with very different sets of requirements, ranging from real - time embedded control
systems to multimedia applications running on desktop computers connected to the

Internet. With the migration of real - time systems from specialised architectures to open
en vironments, guaranteed services and limited response times with very low (or even
zero) error rates are required to allow consistent real - time behaviour. On the other hand,
multimedia applications such as multi - party conferencing, audio and video broadcast ,
and distributed cooperative applications are becoming common for the end - user. This
class of application can tolerate some error, but requires limited response times and
specific throughput. At the moment, the quality of the output generated by these
app lications is inadequate due to the existing limitations of bandwidth and processing
power experienced by the networks and computing systems currently available.

The main problem faced by this category of applications is to guarantee that the services
exec uted by the underlying system on behalf of the application will be performed
respecting all the necessary requirements. A myriad of resources may have to be
provided by the system to allow these requirements to be fulfilled, ranging from local
resources su ch as memory and CPU to network bandwidth and other remotely located
resources.

Quality of Service, or QoS for short, is the keyword used to represent the set of
requirements imposed by a user (human being or software component) on the
performance of the services provided to an application.

2.5.1  Definitions

QoS  is defined by the ISO OSI/ODP group as `a set of qualities related to the collective
behaviour of one or more objects´ [70] . Other authors try to clarify this definition. Fo r
example, Vogel et al. [146]  state that QoS `represents the set of quantitative and
qualitative characteristics of a distributed multimedia system necessary to achieve the
required functionality of an application´.

In this th esis we adopt a very similar definition, with the main difference residing in the
fact that we do not constrain the application of QoS to distributed multimedia systems,
but also extend it to incorporate any system with constraints related to response time ,
performance, and output quality.

ISO, along with the concept of QoS, defines a complete terminology for dealing with

QoS. However, they consider the application of QoS only for the specification of
communication services at network level. We adopt their  terminology slightly modified
to encompass diverse application fields.

According to ISO, a QoS characteristic  is `a quantifiable aspect of QoS´ such as
bandwidth or memory usage. A QoS measure  is defined as `one or more observed
values relating to a QoS characteristic´ such as the measured value of bandwidth or
memory being used by an application at an instant in time.

A QoS information  is any `information related to QoS´. QoS information can be
classified as a QoS requirement , when expressing `a require ment to manage one or more

QoS characteristics´, or as QoS data , if the information is a measured value, a warning,
or any QoS information used by the system in an enquiry. QoS information is further
classified as QoS parameters , when exchanged between ent ities, or QoS context , when
retained in an entity.

A QoS operating target  is `QoS information that represents the target values of a set of

QoS characteristics, derived from QoS requirements´, such as the necessary value of
bandwidth to be provided to an application to allow it reach its requirements. `A group
of user requirements that leads to the selection of a set of QoS requirements´ is called a

QoS category . One example of QoS category  is a user requirement such as `VHS
qualitý for a video session, l eading to the selection of QoS requirements for frame size,
number of frames per second, colour scheme, and so on.

QoS mechanisms  are responsible for the establishment, maintenance, enquiry and
management of QoS. QoS establishment  creates the conditions to  attain the desired set
of QoS characteristics for an activity before it occurs; QoS maintenance  keeps the set of

QoS characteristics at the desired values while the activity is in progress; and QoS
enquiry  consists in `the use of QoS mechanisms to determi ne properties of the
environment related to QoS´.

QoS management  is a set of activities performed by the system to support QoS
monitoring, control and administration. QoS monitoring  is the use of QoS measures to
estimate the values of QoS characteristics,  while QoS control and administration

(usually referred as `QoS control´ for short) are responsible for providing conditions so
that a desired set of QoS characteristics is attained.

QoS management functions  allow a specific QoS requirement to be met. QoS  alerts  are
messages issued when limits or thresholds are crossed.

Finally, a QoS policy  is defined as `a set of rules that determine the QoS characteristics
and QoS management functions´ to be used by the system in a particular case.

The concepts define d by ISO are widely accepted, but are commonly used more freely.

QoS characteristics, parameters, data and information are commonly used as synonyms,
while the study of QoS mechanisms is mainly focused on QoS establishment, with
maintenance, enquiry and ma nagement often being relegated to a second plan despite
their important role in the achievement of QoS.

2.5.2  QoS Specification

The desired quality of service has to be conveyed to QoS mechanisms in the form of

QoS parameters. Parameters can be expressed in ver y different formats, varying
according to the application field, the corresponding abstraction level, or even personal
taste.

QoS mechanisms should be flexible enough to accept different formats of QoS
parameters and interpret them correctly. For example,  a QoS parameter such as

`frequency range´ for an audio application would be completely meaningless for an
application based on data transfer. The same could be said about a parameter such as

`window size´, which is useful for video but unintelligible for audio.

Two main abstraction levels can be identified in systems subject to QoS specification:

the application level and the system level. Parameters specified at different levels are
related, but differ strongly in meaning. An application parameter is gen erally related to
an idea present only at this level, for example, the number of frames of video shown per
second in a video broadcast application. At system level this corresponds to network
bandwidth to transfer data, maximum error and delay, processing time to compress and
decompress the information, memory, access to specialised hardware, etc.

The application fields and the system components in which QoS mechanisms can be
utilised vary enormously. Any attempt to define a common set of parameters for Qo S
specification to be employed by the user to specify its QoS requirements would likely
constrain his expressiveness and make the process of QoS specification more difficult.

Therefore, a compromise must be achieved between the needs of different applicati on
fields regarding the manner in which QoS requirements are expressed and the
generalisation necessary for specifying QoS parameters to be enforced by QoS
mechanisms.

2.5.3  QoS Mapping and Translation

QoS parameters have to be translated between different level s of abstraction to be
meaningful for the mechanisms present at that level. Translation implies that a mapping
exists between parameters at different levels. Mappings are not always one - to - one
between parameters, but may be one - to - many, many - to - one or many - to - many.

                        One - to - One  One - to - Many  Many - to - One  Many - to - Many

                                               Error

                                                 Rate

                                                          ß

                               ATM Cell

                              Loss Ratio

Deterministic

Guarantee
ß

Deterministic Scheduling;

Deterministic Transport;

Memory Paging Blocked

Video Resolution;

Colour Depth
ß

Network

Bandwidth

Network Bandwidth;

Packet Size
ß

Token Bucket Size;

Token Bucket Rate

Table 2  ˘  Examples of Parameter Mapping

Table 2  shows some examples of parameter mappings. Although the mapping may be
complex, the process of translation usually consists in simple arithmetic operations over
a limited set of variables.

Mappings and translation mechanisms have to be bi - directional in order to allow the
transfer of QoS information from the bottom layers of the system to the top o nes,
reporting QoS measures to the application using QoS parameters comprehensible at this
level of abstraction.

For the particular case in which several different application fields and lower - level
components must be supported, the translation process ha s to deal with different sets of
parameters appropriate for the environment in which it is being used. Since the creation
of direct (one - step) translators for N application fields deployed on top of M low - level
components would need the definition of N * M  translators, this solution seems to be
unacceptable.

To allow support for diverse application fields and resource reservation protocols, a way
of extending the mapping and the translation mechanisms must be provided. The
addition of support for a new app lication field or reservation protocol should be as easy
as possible. In other words, the addition of support for a new kind of application should
not imply writing one translator for every reservation protocol supported by the
architecture, and vice - versa .

2.5.4  QoS Enforcement

After obtaining the QoS requirements of the application in the form of QoS parameters
and translating them into a format that is appropriate at a lower level of abstraction,
mechanisms for QoS enforcement have to be used in order to fulf il these QoS
requirements.

QoS enforcement is necessary in order to guarantee that the QoS requirements imposed
by the application will be fulfilled. This can be achieved by controlling and monitoring
the use of the resources provided by the underlying sys tem, either directly by the QoS
mechanism or indirectly by means of a resource reservation protocol [103] . Since the
handling of resources would add even more complexity to QoS mechanisms, the second
solution is the most widely  adopted. Resource reservation protocols are discussed in
more detail in item 2.6 .

The allocation of system resources is even more complex if we consider that multiple
resource reservation protocols can be present in the platfo rm. Since one of our main
goals in this thesis is to provide support for heterogeneous systems, the presence of
multiple reservation protocols must be taken into account during the design of the
mechanisms for QoS enforcement being proposed by this thesis.

2.5.5  QoS Architectures

QoS architectures consist in middleware components that are responsible for integrating
mechanisms for QoS specification and enforcement in computational systems. The
mechanisms provided by QoS architectures are used by applications in o rder to have
their QoS requirements observed by the underlying system.

To allow the utilisation of the features provided by networks and operating systems with
reservation capabilities at user level, several QoS architectures have been defined in the
lite rature [4] [24] [27] [102] [156] . However, most of the QoS architectures proposed so
far target only a specific con figuration of operating system software and communication
infrastructure. This tight dependency on a specific environment constrains their
application in open systems, where heterogeneity is always present. ATM - based
systems combined with real - time operati ng systems are the most popular platforms for
the development of QoS architectures, because of their suitability for the
implementation of QoS mechanisms based on the reservation of system resources.

Some architectures are also targeted at very specific ap plication fields, with video
conferencing being the one where the technology is more mature because of several
research projects that explored this topic.

2.5.6  ISO QoS Framew ork

The ISO QoS framework [70]  consists of a model that ^ defines the architectural
principles, the concepts and the structures that underlie the provision of QoS~ in the
basic reference model of Open Systems Interconnection (OSI).

The OSI basic reference model is provided with QoS entities that take part in QoS
management. Two classes of entities are defined within the ISO QoS framework:

·

                         System QoS entities: entities which have a system - wide role, i.e. are cross - layer;

                         and

·

                         Layer QoS entities: entities associated with the operation of a particular subsystem

                         prese nt in a specific layer.

System QoS entities interact with layer QoS entities in order to monitor and control the
performance of the system.

The following layer QoS entities are defined by ISO:

·

                         N - Layer Policy Control Function (N - PCF): receives the QoS requ irements and

                         determines the policy that is to apply to the operation of the N subsystem;

·

                         N - Layer QoS Control Function (N - QCF): selects the entities that will participate in

                         the provision of communication services by taking into account the QoS

                         requirements  received from N - PCF; and

·

                         N - Layer Protocol Entity (N - PE): checks if the QoS requirements imposed on a

                         communication service can be supported, possibly renegotiating them with peer N -

                         PEs or indicating a failure when a requirement cannot be accepted.

At the  system (cross - layer) level, the ISO QoS framework defines two functions and a
set of entities. They are:

·

                         a System Quality Control Function: a system - wide capability for tuning the

                         performance of the various protocol entities that are in operation;

·

                         a Syst em Policy Control Function: a function that ensures system - wide consistency

                         to  the policies implemented by each individual N - PCF in a layer; and

·

                         Management Entities: responsible for supporting OSI system management and

                         general management operations and no tifications necessary for QoS management

                         (such as QoS data metrics and time management, for example).

As can be easily seen, the ISO QoS framework only defines a reference model for QoS
specification and management at the network level. This follows the ap proach
undertaken by ISO for the definition of the OSI reference model. Despite being a good
starting point for understanding the structure of middleware that provides support for

QoS specification and enforcement, the ISO QoS framework covers QoS only at the
network level and lacks a more detailed architectural specification.

2.6  Resource Reservation

The deployment of a distributed application on fast machines interconnected by a
network with sufficient bandwidth does not necessarily guarantee that an applica tion
will behave as expected.

The services available at the network and operating system level have to take into
account the requirements of the application that is using these services during their
execution. This does not mean that low - level details hav e to be accessible at application
level, introducing more complexity to be dealt with by the programmer. Instead, we
consider that resource reservation mechanisms will have to be provided to allow
applications to easily control and manage the use of networ k and operating system
resources. This strategy allows the communication support to guarantee the availability
of bandwidth for the application and to impose an upper limit on the communication
delays, for example. In the same way, the operating system is able to guarantee the
availability of resources such as processing power and memory for the use of the
application.

In order to achieve the desired system performance, QoS mechanisms have to guarantee
the availability of the shared resources needed to per form the services requested by
users. The concept of resource reservation provides the predictable system behaviour
necessary for applications with QoS constraints.

Aiming to provide more guaranteed availability of resources for applications, networks
and  operating systems are incorporating mechanisms for resource reservation.

Reservation mechanisms have to keep track of the use of the limited set of resources
provided by the system, and receive requests from new users interested in using these
resources. New requests are subject to admission tests based on the usage of the
resources and the guarantee levels that satisfy the user. Reservations are then accepted,
if there are resources available, or rejected if not. The problem of allocating limited
resource s becomes even more complex if we consider that current computational
systems are basically heterogeneous, subject to mobility and constant reconfiguration,
but still have to provide a dependable and accurate service in a limited response time.

The concep t of resource reservation, like QoS, originated from work on communication
networks and was subsequently extended to other components of computational
systems.

In the area of computer networks, we can mention the development of ATM as a
significant advanc e towards the provision of QoS - constrained communication services.

Aiming to provide similar behaviour, but working at the logical network level, the IETF
is proposing a new suite of protocols for the Internet. The suite of protocols is based on

IP version  6 (IPv6) in conjunction with a reservation protocol (RSVP) and a new
transport protocol named RTP. Both ATM and the new Internet protocol suite will be
described in detail later.

At the operating system level, some work has been developed to extend conven tional
operating systems in order to provide more predictable behaviour suitable for
applications with QoS constraints. Microkernel - based operating systems such as Mach

[145]  have been extended to provide time - constrained servi ces. Conventional
commercial versions of UNIX, such as Sun´s Solaris and IBM´s AIX, are also being
adapted to provide behaviour suitable for applications with QoS constraints. In addition,
some experimental operating systems [59] [89] [123]  provide mechanisms for resource
reservation that can be used by applications that need to have guaranteed access to
system resources.

Each existing reservation protocol has its own inte rface and its own set of parameters or
reservation messages for the specification of the resources to be reserved for use by the
application. The handling of differences between multiple reservation protocols by QoS
mechanisms then becomes a complex task t hat has to be considered carefully in the
design of middleware that is intended to provide QoS constrained services.

2.6.1  Resource Adaptation

One important trend in research into resource reservation protocols is resource
adaptation [52] .

Some authors consider resource reservation as a guaranteed method of delivering a
specified QoS to an application during its entire lifetime [36] [88] [101] . Anot her school
of thought proposes the development of adaptive applications capable of dealing with
changes in resource availability during the provision of service [25] [26] [30] . A third
idea based on resource adaptation, which mixes both approaches mentioned previously,
has been considered as a viable and necessary alternative to either.

Several drawbacks appear in efforts to provide guaranteed resource reservation services
for the following reasons:

·

                         the physical structure of the whole computer system may change due to hardware

                         reconfiguration and computer mobility, and changes in the distribution of resources

                         may become necessary;

·

                         monitoring services may detect that the Q oS requested by an application is not being

                         achieved with the resources that were allocated for it, and then decide to allocate

                         new resources;

·

                         the system may reclaim resources that are not being utilised or that are necessary for

                         more important activities .

On the other hand, adaptation is very limited for services with strong requirements, and
does not solve the problems that applications with QoS requirements face when they try
to use the best - effort systems currently available.

Resource reservation com bined with adaptation entails a more flexible approach for
providing QoS to applications [52] . In this approach, resources can be seen by
applications as being guaranteed during some time, but their availability can vary over
l ong periods. Applications are responsible for estimating their initial resource
requirements and for negotiating their reservation with resource providers. During run -
time the application has to be able to adapt its behaviour based on feedback received
fro m the system.

QoS mechanisms have to be aware of the possibility of resource adaptation, making it
transparent to the application whenever possible. When the agreed QoS is not reachable
with the resources available, the application has to be informed that  the previously
agreed QoS has to be renegotiated. Applications have to be ready to handle this kind of
situation without disruptions in the service being provided to the user. In other words,
applications holding resources that are subject to changes in their availability because of
resource adaptation have to be able to degrade gracefully when it occurs.

2.6.2  ATM

Asynchronous Transfer Mode (ATM) [16] [113]  is a communications standard proposed
by the T elecommunication Standardisation Section of the International

Telecommunications Union (ITU - T) as the transport mode for the Broadband Integrated

Services Digital Network (B - ISDN) [71] .

ATM networks aim to integrate traffic wi th different flow characteristics and service
requirements. The type of traffic to be supported by ATM networks ranges from real -
time data such as voice and high - resolution video, which can tolerate loss of data but
not delay, to non - real - time traffic such  as computer data and file transfer, which can
tolerate delay but not loss of information.

The flow can vary from CBR traffic as required by non - compressed audio or video, to
the bursts of data typical of computer systems where the average arrival time bet ween
bursts may be quite large and randomly distributed.

The main idea behind ATM is to transmit small data packets (ATM cells)
asynchronously without error recovery at the network level. Each ATM cell consists of

53 bytes of data, of which 5 bytes are us ed by the ATM header. The adoption of an
asynchronous approach allows better performance in the presence of bursts of data with
low latency. Error correction and data recovery can be implemented at higher levels if
necessary, according to the characteristi cs of the data being transmitted.

The transmission of data is completely connection - oriented, with data flowing through

ATM channels. Each channel is identified by a channel number, which is composed of a

Virtual Channel Identifier (VCI) and a Virtual Pat h Identifier (VPI). The channel
number appears in the header of each ATM cell.

ATM supports point - to - multipoint and multipoint - to - multipoint connections in addition
to the usual point - to - point communication. New members ˘  either senders or receivers ˘
can be added dynamically to multipoint connections by using the ATM signalling
protocol. It is important to notice that communication is always unidirectional in
multicast connections (i.e., data flows from senders to receivers only), and traffic
characteristi cs and service requirements (QoS) must be the same for every member.

Some manufacturers of ATM equipment still do not provide full support for multipoint
communication.

There is no defined mapping between ATM and the seven layers of the OSI Reference

Model  [68] . The ATM Reference Model goes beyond the OSI model, introducing the
concept of planes subdivided in layers in a three - dimensional structure. The use of
planes allows the representation of features such as control and mana gement in parallel
with data transfer. The structure of the ATM architecture is shown in Figure 3  and
described below.

Physical Layer

ATM Layer

                                                                                  ATM Adaptation Layer ATM Adaptation Layer

                                                                                                  High-Level Layers High-Level Layers

Control Plane

User Plane

Layer Management

Plane Management

Figure 3  ˘  The ATM Architecture

The three planes defined by the ATM architecture are:

·

                         User Plane: for transporting user information.

·

                         Control Plane: deals with channel control, connection control, and signalling

                         information.

·

                         Management Plane: implements layer management and plane management.

The layers  are divided as follows:

·

                         Physical Layer: performs bit - level functions, adapting the cell - based approach to the

                         transmission medium.  The physical layer is subdivided into:

                        ·

                                                 Physical Medium (PM): contains only the medium dependent functions. It

                                                 provides bit  transmission and alignment, performs line coding and also

                                                 electrical/optical conversion when necessary. PM layers for optical fibre, and

                                                 coaxial and twisted pair cables are defined in the reference model. This layer

                                                 also includes bit - timing functions such  as insertion and extraction of timing

                                                 information.

                        ·

                                                 Transmission Convergence (TC): takes care of generation, recovery and

                                                 adaptation of transmission frames, adapting the cell flow according to the

                                                 transmission system. TC also performs the cell delineation  function, enabling the

                                                 receiver to recover the cell boundaries, and calculates and verifies the header

                                                 checksum (HEC), allowing correction of header errors. TC also inserts idle cells

                                                 in the medium in order to adapt the rate of the ATM cells to the capaci ty of the

                                                 transmission system, and suppresses all idle cells received.

·

                         ATM Layer: is the core of the ATM network architecture. This layer performs the

                         following functions:

                        ·

                                                 Cell header generation/extraction: adds the appropriate ATM cell header (except

                                                 fo r the HEC value) to the cell received from the ATM adaptation layer (AAL) in

                                                 the transmit direction, and does the opposite (i.e., removes the cell header) in the

                                                 receive direction. Only cell data fields are passed to the AAL.

                        ·

                                                 Cell multiplexing and demulti plexing: multiplexes cells from individual virtual

                                                 paths (VPs) and virtual channels (VCs) into a single cell stream in the transmit

                                                 direction. It divides the arriving cell stream into individual cell flows (VC or

                                                 VP) in the receive direction.

                        ·

                                                 VPI and VCI translation: performed at the ATM switching and/or cross - connect

                                                 nodes. The values of VPI and VCI fields of each incoming cell are translated

                                                 into new VPI and VCI values in the outgoing cell according to the characteristics

                                                 and the state of the ATM switch.

                        ·

                                                 Generic Flow Control (GFC): supports control of the ATM traffic flow in a

                                                 customer network. This is defined only at the user - to - network interface (UNI);

                                                 GFC does not exist in the network - to - network interface (NNI) cell.

·

                         ATM Adaptation Layer (AAL): perfo rms the adaptation of higher layer protocols.

                         AAL is divided into two sub - layers:

                        ·

                                                 Segmentation and Reassembly (SAR): performs segmentation of the higher layer

                                                 packets of data into a suitable form for the payload of the ATM cells of a virtual

                                                 connection; a t the receive side, it reassembles the contents of the cells of a

                                                 virtual connection into data units to be delivered to the higher layers.

                        ·

                                                 Convergence Sublayer (CS): performs message identification and time/clock

                                                 recovery. This layer is further divided in to a Common Part Convergence

                                                 Sublayer (CPCS) and a Service Specific Convergence Sublayer (SSCS).

Four classes of service (namely A, B, C and D) were originally identified by the ITU - T,
each one providing a data flow appropriate to a different set of appli cations with similar
traffic characteristics. For each class of service a corresponding adaptation layer (AAL1
for class A traffic, AAL2 for class B, and so on) was defined. Table 3  summarises the
original relationship between cla sses and AAL types.

                             Class of Service  A  B  C  D

                                   Original AAL  AAL1  AAL2  AAL3  AAL4

                            T iming Relation  Preserved  Not Preserved

                                                   Bit Rate  Constant  Variable

                        Connection Mode  Connection Oriented  Connectionless

                                                   Original

                                                        T arget

                                      Applications

Circuit emulation,
non - compressed
audio and video.

Compressed
audio and
video.

Virtual circuit
services (X.25,

Frame Relay, etc.).

Datagram service,

IP over AT M,

LAN emulation.

                                                           Table 3  ˘  Original ATM Classes of Service and Adaptation Layers

However, du ring the specification process it was recognised that this approach needed
to be modified. As a result, new AAL types and classes of traffic were defined, and
different combinations between them were allowed when appropriate. Table 4  shows
the resulting classes of services and AAL types.

AALs 3 and 4 were merged because of their similarities, giving rise to AAL3/4.

Nevertheless, the 4 - byte per cell overhead required by the headers and trailers necessary
to provide connectionless se rvice multiplexed over a single ATM channel constrained

AAL3/4 adoption to class D services, and AAL5 was created to provide a more efficient
interface for class C services. AAL5 is also used by the ATM signalling protocol (ITU -

T Q.2931) and by a new class  Y, known as available bit - rate (ABR), which is suitable
for delay - tolerant applications.

                                    Class  A  B  C  Y  Q.2931  X  D

                                     AAL  AAL1  AAL2  AAL5  AAL0  AAL3/4

                                     T ime  Preserved  Not Preserved

                            Bit Rate  Constant  Variable

                 Conn. Mode  Connection Oriented  Conn - less

                 Exampl es of

                   Application

                                                                                                          Circuit

                                                                                                 emulation

Compressed
audio/video

Conn - oriented
services

Available

Bit Rate

Signalling  Cell - relay  Conn - less
services

                                                       Table 4  ˘  Resulting ATM Classes of Service and Adaptation Layers

A class X, or unassigned  bit - rate (UBR), was also introduced for provision of cell - relay
service for applications with minimum QoS requirements, i.e., delay - tolerant and
subject to cell loss. Class X employs a null AAL (also known as AAL0) to access the
cell - relay service provide d by the ATM layer.

Class B service is not currently available, because there is no standard or vendor -
specific proposal for AAL2.

ATM is a technology under development. Despite not being completely standardised,
this technology is evolving rapidly and b eing widely accepted in the computer network
market, with applications in both local and wide area networks. A large number of
vendors are providing ATM hardware, with a reasonable degree of interoperability
between equipment from different vendors.

QoS an d Resource Reservation . During the connection establishment process, the
application can specify the desired QoS for an ATM channel based on parameters such
as maximum number of cells per second, statistical variation of the volume of data
being transmitte d, maximum end - to - end delay, and maximum jitter allowed. A
connection is refused when the network cannot support the required QoS level. The
acceptance or refusal of a QoS specification is determined during an admission process,
and rejection may occur due  to lack of network resources.

The API used for requesting QoS varies from vendor to vendor, and also depends on the
abstraction layer at which the specification is taking place. The format of QoS
parameters can also vary considerably. A common approach fo r QoS specification uses
extensions to the sockets API based on
ioctl()
 calls.

2.6.3  Internet Protocols

The next version of the Internet suite of protocols, known as Internet Next Generation,
provides resource reservation and guaranteed end - to - end QoS at applica tion level.

The work carried out by the IETF (Internet Engineering Task Force) is orthogonal to the
subnetwork - specific solutions for broadband integrated services networks (such as

ATM) because it targets the logical network.

All this effort to adapt th e Internet to a new communication framework is being
developed in parallel with the new version of the IP network protocol, known as IPv6

(version 6) [34] [40] [64] . IPv6 is designed to support a larger set of addresses (128 bits
instead of 32) while maintaining compatibility with the current version. Additionally,

IPv6 has the following characteristics:

·

                         IP packets can be associated to a flow through the use of a field in t he IP header;

·

                         multicast communication is improved through the addition of a scope definition

                         field in the IP header, limiting the geographical amplitude of multicast messages;

·

                         a new communication paradigm, called anycast, has been introduced;  anycast

                         sup ports groups of receivers to which messages are sent only to the nearest member

                         of the group;

·

                         packet options are implemented in a more flexible and extensible way, using

                         multiple option fields outside the area of the IP header; and

·

                         support for authentica tion and QoS specification is allowed through the definition of

                         traffic flows with particular requirements and characteristics.

The new suite of Internet protocols being developed by the IETF is illustrated by

Figure 4 .

At the network layer, the IETF has two parallel activities underway. The first is
addressing the provision of a Stream Transport Protocol (ST - II). The alternative activity
is based on a Resource Reservation Protocol (RSVP) running over IP. Both solution s
support multicast communication, resource reservation, bandwidth management and

QoS specification, but the approach adopted in their design differs in several
fundamental points.

                                                                          Application Level

                                                                          T ransport Level

                                                                          Network Level

                                                                          Sub-Network Level S

UB

-

NETWORK

RSVP

RTP

RTSP

A

PPLICATIONS

T CP UDP

ST -II IP

Figure 4  ˘  Internet Next Generation Protocols

ST - II [41]  is a connection - oriented network protocol, designed to coexist with IP, which
allows resource reservation determined by the origin of the flow. New receivers
interested in participating in an on going connection have to contact the origin to request
their inclusion. An associated control message protocol, SCMP, is responsible for
initiating and modifying connections, allowing resource specifications to be changed to
fulfil the requirements of a sp ecific receiver.  The main disadvantage of the approach
adopted by ST - II is related to the bottleneck imposed by the excess of tasks assigned to
the source of the media, which constrains the scaling of receiver groups.

On the other hand, RSVP [19]  is based on the establishment of flows over a
connectionless network service (IP version 4 or 6), allowing reservation of resources for
a specific flow when necessary. The multipoint communication service is designed to
scale to very large groups through the use of flow specifications defined by receivers.

Sender

                                                                                                               Receiver #1
Receiver #2
Receiver #3

Router #1

Router #2

Path message

Reservation message

Figure 5  ˘  Propagation of RSVP Messages

Figure 5  shows the exchange of RSVP messages in a multicast fl ow. Each receiver
interested in a communication flow enters the corresponding multicast group and waits
for a path message that describes the composition of the flow. The receiver then decides
in which part of the flow it is interested (e.g. only the black  and white component of a
coloured video flow, only the audio of a film, etc.) and generates a filter. A flow
specification ( flowspec ) describing the required characteristics of the flow is also
generated by the receiver. It then arranges both the filter a nd the flowspec  in a
reservation message, which is propagated periodically in the direction of each individual
origin of the flow. Routers along the path are responsible for reserving the resources
needed for the flow described by the reservation message. Reservation messages are
short - lived, having to be periodically refreshed by the receivers. This results in soft state
information being stored by the routers along the path. In the absence of refresh
messages, the reservation expires. The storing of soft state is an appropriate approach
for implementing reservation of resources in the Internet, which was originally designed
as a stateless infrastructure in order to tolerate failure and to scale gracefully.

At transport level, the usual Internet transport  layers, TCP and UDP, are being adapted
to take advantage of the new characteristics of IPv6. Furthermore, a new protocol called

Real - Time Protocol (RTP) has been proposed.

RTP [131]  provides higher level services such as encap sulation, multiplexing and
demultiplexing, encoding, synchronisation, error detection and encryption. RTP can
make use of the other transport protocols (TCP or UDP) or access the network layer
directly (IP or ST - II). A transport control protocol named RTCP  is responsible for
group management, connection control, and QoS monitoring.

An application protocol developed by Netscape Corporation and Real Networks was
accepted by IETF as a draft standard. The Real - Time Streaming Protocol (RTSP) offers
a ^WWW - based and HTTP - friendlỹ interface to allow on - demand delivery of real - time
media over the Internet [132] . RTSP is built on top of the currently available transport
protocols (RTP, TCP and UDP). The protocol provides mechanisms to re quest delivery
of real - time data, specify the transport layer to be used and the destination for the
delivery, request information about the encoding format, control the flow of data
through the stream, and to access portions of data when applicable (i.e.,  in case of
recorded media).

With the introduction of these protocols, the IETF intends to provide a complete suite of
mechanisms for the transmission of continuous media and real - time data through the

Internet.

QoS and Resource Reservation . The most commo n method used by Internet
applications for specifying their requirements is by using RSVP, and it implies defining
a token bucket model [19]  for the data traffic generated by the application. According to
this model, the transm ission capacity of the network is modelled by a bucket that is
filled with tokens in a constant rate; for each data unit transferred through the network, a
token must be taken from the bucket; the size of the bucket limits the occurrence of
network bursts.

A series of calls to the sockets API is necessary to set up RSVP and then perform
reservations of network resources by specifying parameters such as the size of the token
bucket, the token rate, packet size, etc. Like ATM, RSVP performs an admission
proce ss that determines whether the requirements can be met by the network or not. In
addition to the token bucket style of reservation, RSVP also provides other methods for
specifying resource reservations. However, these new methods are still in the process o f
being defined by the IETF and added to the RSVP API.

2.6.4  Real - Time Capabilities of Window s NT

The Microsoft Windows NT operating system provides a set of mechanisms that make
it possible to be used by applications with timing constraints. By definition, Wind ows

NT is a general - purpose O.S. with soft real - time capabilities and not a hard real - time

O.S. that provides deterministic response times [96] . Despite lacking support for hard
real - time computing, Windows NT still consists of  a useful platform for the deployment
of multimedia applications and non - critical real - time applications [144] .

The real - time mechanisms provided by Windows NT consist of:

·

                         A real - time scheduling class, which isolates real - time tasks from the ones satisfied

                         by the best - effort scheduling policy that is used by default by the system scheduler;

·

                         Mechanisms for blocking memory paging, which makes the access times to the

                         physical memory more predictable;

·

                         Asynchronous I/O, which allows applications to queue an I/O operation and

                         continue processing without having to either wait or respond to an end - of - I/O event;

·

                         Bounded latency for handling interrupts; and

·

                         Synchronisation mechanisms such as timers, events, mutexes and semaphores.

These mechanisms are accessible for the application programmer either through the

Windows 32 - bit (Win32) API or through the Windows Sockets (WinSock) API. In
particular, WinSock extends the sockets API by providing alternative versions of the
original API calls with additional parameters, which allow the user to execute
asynchronous I/O and to specify QoS requirements in the form of a traffic descriptor,
for example.

Later in this thesis we will make use of the real - time mechanisms provided by Windows

NT in orde r to build middleware that provides support for applications with timing
constraints imposed on their computation.

2.7  Summary

This chapter has situated the area of research in which this thesis is inserted. Concepts
in the fields of multimedia and real - time a pplications, open systems, distributed object
computing, QoS and reservation protocols have been presented.

The immediate goal of this thesis is, by using the knowledge gathered in these area of
research, to provide an environment in which QoS can be achie ved in the deployment of
critical applications (such as multimedia and real - time applications) in open systems.

Technologies such as resource reservation and distributed object computing have a key
role in providing a solution for this problem.

In this cha pter we have also presented a series of well - established technologies which
can be used for building a QoS architecture suitable for open systems. On the one hand
we have reference models such as MSS and the ISO QoS Framework that provide a
series of insig hts that can be used for designing the QoS Architecture. On the other
hand, technologies such as CORBA, real - time operating systems, ATM and the new

Internet protocols indicate the sort of support that a QoS architecture can rely upon.

3

State of the Art

The following sections present a number of frameworks and architectures that provide

QoS mechanisms for applications with QoS requirements. During this surveying study,
we have identified a series of limitations that prevent the use of state - of - the - art
tec hnology to provide support for QoS specification and enforcement in open systems.

These limitations are targeted by a new proposal of QoS architecture, which will be
described in the next chapter of this thesis.

3.1  XRM  and Xbind (Univ. of Columbia)

The eXtend ed Reference Model (XRM) and the Xbind platform [88]  have been
designed and implemented by the Comet group at the University of Columbia.

XRM models the communication architecture of networking and multimedia computing
platfor ms using three components: the broadband network, the multimedia network, and
the services and applications network.

The broadband network is defined as the physical network. Upon this physical
infrastructure resides the multimedia network, whose primary function is to provide
support for services with end - to - end QoS guarantees. The user has contact only with the
service abstractions provided by the services and applications network.

The services visible at the multimedia network level are provided by Xbi nd, a
programming platform for creating, deploying and managing multimedia services.

Xbind is basically a conceptual framework for creation, deployment and management of
multimedia services on ATM networks, which allows the specification and control of
end - to - end QoS.

Xbind adopts an open signalling concept called ^hardware independent signalling~. The
main idea entails creating a separation between switching software and hardware. This
allows, for example, the installation of signalling software on an ATM  switching
platform from a third party vendor, simplifying the service creation, deployment and
management.

Functionally, Xbind consists of a kernel that provides end - to - end QoS over broadband
networks, including software components for implementing mecha nisms for distributed
network resource allocation, broadband signalling, real - time switch control, multimedia
transport and device management.

The associated binding architecture presents the service provider with a set of open
binding interfaces with mul timedia and QoS capabilities. Additionally, the Binding

Interface Base (BIB) allows an easy integration of control (connection establishment
and resource allocation), network management and service management.

The Xbind kernel has been ported and tested o n several operating systems and different
types of ATM equipment. The CORBA architecture was adopted as the lower level for
implementing the binding architecture, providing interoperation between multiple
platforms.

Xbind is an example of a multimedia pro gramming framework that provides network -
level QoS mechanisms. Some degree of system heterogeneity is provided by the use of

CORBA and by the different versions of the Xbind kernel that were built on different
platforms. However, it lacks some features tha t are required by applications with QoS
requirements deployed in open systems. Heterogeneity at the resource reservation
protocol level is not supported due to the tight integration of the system with the
network protocol (i.e. ATM). Low - level details rega rding the network transport are not
hidden completely from the programmer. In addition, Xbind does not provide support
for QoS adaptation, and there is no mechanism for extending the programming
framework.

3.2  ReTINA Project (ACTS)

Real - Time TINA [18]  is a cooperative project sponsored by the European ACTS
program that was carried out by Chorus Systems, Alcatel, Siemens, HP, CSELT, France

Telecom, British Telecom, Telenor, APM, O2 Technology and Broadcom.

The main goal of the ReTI NA project was to develop a distributed processing
environment (DPE) with support for interactive real - time and multimedia services,
following standards such as CORBA [108]  and ODP [39] . Support for  real - time and
multimedia traffic is obtained with the encapsulation of multiple communication
protocols within an ORB, providing flexible bindings and interaction models, and with
fine - grained control of resources in order to provide QoS guarantees.

ReTIN A adopts a binding protocol based on the ODP reference model for establishing
connections (i.e. bindings) between objects. This protocol introduces binding factory
objects responsible for the provision of binding models appropriate for real - time and
multim edia applications, such as third - party and multiple bindings, and with
specification of QoS for bindings. In order to provide QoS guarantees for bindings, the
resources necessary to achieve the desired QoS must be reserved for the use of the

`ODP capsule´ (address space) of the corresponding object.

In addition to the core of the DPE, which encompasses the ReTINA ORB, several
peripheral services make up the ReTINA environment. These services are based on the

CORBA services defined by the OMG, including tra ding, notification and events,
security, replication and transaction services as well as telecommunication - specific
services such as connection managers and QoS providers.

Stream abstractions are supported by means of extensions to the IDL language that
al low stream interfaces to be specified. Stream interfaces have operations responsible
for transferring frames of media and do not have return values or argument
directionality specification. Arguments specify the format of the frames transmitted
through the  stream. Stream interfaces are referenced via regular CORBA object
references that may be passed as arguments of operations or stored by the CORBA
name service.

The ReTINA environment is based on a multi - platform ORB, which runs with a real -
time `profile´ over the Chorus micro - kernel [14 2]  and with a non - real - time `profile´
over generic operating systems. Furthermore, ReTINA provides a set of application
development, configuration and management tools aimed at facilitating the p rocess of
deploying applications on top of the ReTINA environment.

ReTINA combines support for real - time and multimedia applications, but QoS
specification mechanisms still are not user - extensible. Like Xbind, it enforces QoS only
at network level, and imp ortant features that are necessary in an open environment such
as support for QoS adaptation are still missing.

3.3  DIM M A (APM - ANSA)

The DIMMA (Distributed Interactive MultiMedia Architecture) project [116]  proposes
to extend cur rently available distributed computing architectures in order to incorporate
real - time and multimedia capabilities. This research project was carried out by the

APM - ANSA Laboratories.

The main objectives of the DIMMA project were:

·

                         to extend distributed com puting object models such as CORBA for supporting real -

                         time and interactive multimedia applications;

·

                         to incorporate support for new paradigms of communication best suited for

                         multimedia and real - time systems such as streams (e.g. audio/video communication)

                         and signals (real - time processing) in distributed systems;

·

                         to identify extensions needed to support distributed services management, fine -

                         grained control and monitoring of resource usage and management (e.g. explicit

                         binding);

·

                         to define an architecture fo r QoS negotiation, management and control; and

·

                         to investigate of the interworking of distributed object models (e.g. CORBA vs.

                         ODP) at the computational level (e.g. IDL translations) and at the engineering level

                         (e.g. transport protocols).

The adopted app roach consists in using a set of distributed computing environments

(ANSAware [91] , DCE [114] , and various ORBs) and operating systems (ranging from
desktop to real - time operating systems) as a basi s for constructing a higher - level API.

DIMMA adopts several partial models for structuring the distributed environment. An
object model incorporates features appropriate to real - time and multimedia
environments. An interaction model adds the concept of str eams and group
communication to the traditional client - server model. In addition, a control model
regulates both synchronous and asynchronous communication. Implicit and explicit
bindings are provided through the adoption of binding managers at both client  and
server sides. The QoS model addresses the requirements present in multimedia and real -
time environments, allowing specification and control of end - to - end quality of service.

Finally, the scheduling model provides resource allocation, priority scheduli ng
mechanisms and deadline control.

DIMMA provides a stub generator toolset that supports several kinds of IDLs and the
generation of client and server stubs for multiple platforms (e.g. ODP, CORBA). The
toolset is built around the Abstract Syntax Tree con cept (AST), as a syntax - free way to
capture the semantics of interfaces. The stubs generated are, whenever possible,
independent from the engineering details such as transport used, and marshalling
algorithms. The AST also serves as a data interchange form at between the tools and
services in the DIMMA development and runtime environment (type and scope checker,
interface repository, and trader).

The AMBER project [86] , also carried out at APM - ANSA Laboratories, provides a

CORBA - compliant environment suitable for distributed multimedia and
telecommunication applications by applying solutions proposed by APM in the

DIMMA project and also from TINA and ODP. The approach adopted is based on the
incorporation of the concept of stream  interfaces to the CORBA IDL and the extension
of object adapters in order to support streams.

DIMMA and AMBER, like the other systems presented before in this chapter, still have
limited support for QoS specification and enforcement. Despite their wide p latform
coverage, these architectures do not take into account the possibility of having multiple
reservation protocols in open systems. In addition, mechanisms for the application
programmer to extend the QoS mechanisms are not provided by both architectu res,
which also lack support for QoS adaptation.

3.4  SUM O (Univ. of Lancaster)

The SUMO Project (SUpport for Multimedia in Operating systems) [35]  was developed
by the Distributed Multimedia Group at Lancaster University and by C NET at France

Telecom. SUMO is a microkernel - based system that aims to provide facilities to support
distributed real - time and multimedia applications in ODP - based platforms.

The SUMO project provides the application programmer with a QoS - driven API, a
co nnection - oriented communication system with connection - dedicated resources and
facilities for monitoring and controlling the QoS of multimedia applications.

A set of key architectural principles was adopted in the design of SUMO. They are:

·

                         upcall - driven a pplication structuring, whereby communications events are initiated

                         by the system rather than by the application;

·

                         split - level system structuring, which means that key system functions are carried out

                         cooperatively between kernel and user level components;  and

·

                         decoupling of control and data transfer, i.e. the control is carried out asynchronously

                         with respect to the transfer of data.

The Chorus microkernel [142]  was used as a vehicle for providing the operating system
level se rvices as well as basic real - time support. The design of the SUMO distributed
real - time/multimedia support system was implemented partly in kernel space and partly
as a user - level library that is linked to native Chorus applications.

In parallel with the d evelopment of SUMO over Chorus, the necessary requirements to
support synchronisation of continuous media in open distributed processing
environments were investigated by the creators of SUMO [36] . Sophisticated support
for syn chronisation was proposed as a result of this work. The coordination of
multimedia presentations, and the maintenance of timing relationships between distinct
data transmissions and of event - based synchronisation points is allowed through the
cooperation o f invocation mechanisms with new services introduced at system level,
called streams and synchronisation managers. These services allow the verification of
synchronisation constraints imposed on the exhibition of distributed media.

The use of the SUMO syst em as a support infrastructure for CORBA was also
investigated [37] . The developers of SUMO have proposed extensions to the CORBA
computational model in order to incorporate interfaces for multimedia streaming, and

QoS `annotat ions´ (i.e. specifications) on interfaces along the lines suggested by the

ISO Reference Model for Open Distributed Processing (RM - ODP) [69] .

SUMO concentrates on providing QoS at operating system level only. Its use is limite d
in open systems due to the lack of support for multiple reservation protocols; its area of
application is limited to multimedia; mechanisms for extending the run - time support are
not provided; and it lacks support for QoS adaptation.

Other research init iatives related to multimedia and group communication, as well as
end - to - end QoS over integrated services networks, are also being undertaken by the

Distributed Multimedia Group at Lancaster University.

The experience gained with the SUMO project was empl oyed by the research group for
developing the QoS - A architecture, which is described in section 3.8 . Conclusions of
this project also contributed for the MMN project, described in section 3.12 .

3.5  TAO  (Washington University at St. Louis)

The TAO project intends to optimise the performance of CORBA implementations for
performance - sensitive applications such as hard real - time systems (e.g. avionics) and
constrained latency systems (e.g. teleconferencing) .

Earlier studies and performance measurements [127] [128]  identified severe bottlenecks
in the currently available CORBA implementations, which limit their utilisation for
building applications wit h real - time requirements. To allow the development of a

CORBA - compliant platform suitable for this kind of application, several changes in the
way that the ORB processes remote method invocations were proposed in order to take
real - time constraints into ac count. In addition, support for high - speed networks (e.g.

ATM) and mechanisms for QoS specification and enforcement were identified as
aspects that have to be added to the ORB.

Aiming to overcome the limitations that constrain the use of CORBA technology in
performance - sensitive systems, a real - time ORB called TAO (also known as ^the ACE

ORB~) has been designed and implemented [129] [130] .

The proposed approach to solving the observed performance pr oblems introduces a real -
time object adapter, responsible for processing real - time requests, and an ORB
scheduler which implements both dynamic and offline real - time scheduling algorithms.

Changes are introduced at protocol level in order to allow applicat ion programmers to
plug customised communication protocols into the ORB.

Other improvements at the protocol level include the introduction of scheduling queues
for processing requests and optimisations in data copying, marshalling operations, and
in the m ultiplexing of requests over communication links. At the system level, TAO
employs a highly optimised real - time I/O subsystem and a high - speed networking
infrastructure.

TAO is an example of real - time middleware that provides real - time applications with
me chanisms for imposing QoS constraints at operating system level. Being compatible
with CORBA, TAO allows applications to interact in an open environment

Nevertheless, it does not have support for enforcing end - to - end network - level QoS
constraints, and depe nds heavily on an optimised O.S. kernel. In addition, TAO lacks
important features such as platform transparency, extensibility and support for
adaptation.

3.6  Arcade (CNET and ENST)

The Arcade project [42]  was proposed by CNET (F rance Telecom Research Centre) and
the Department of Informatics at the École Nationale Supérieure des Télécomunications

(i.e. the French National Superior School of Telecommunications). Arcade is
conceptually a platform that aims to provide support for di stributed multimedia
applications. Its main concern is the area of system - level QoS.

Arcade provides a scheduling framework that automatically derives scheduling
information from temporal QoS constraints. This framework allows the description of
high - leve l temporal QoS constraints in the form of arithmetic equations using a
language called QL (QoS Language). These equations are translated automatically into
scheduling information used by a user - level scheduler. This scheduler works together
with the operat ing system scheduler, to make a best effort at allowing applications to
meet their deadlines.

In this framework, both schedulers follow the Earliest Deadline First (EDF) policy.

Temporal QoS equations are translated into deadlines and used as parameters f or the
scheduling of system threads. An application is implemented as a multithreaded process
with one or more objects, and each invocation of a method of an object creates or
activates a thread.

A library of lightweight user - level threads is employed for  implementing the
framework, allowing that switches between threads of the same application occur
without interaction with the system kernel. Arcade is based on a variation of the Chorus
kernel with extensions to support the EDF policy.

Like TAO and SUMO,  Arcade is not able to enforce QoS at network level, since it
concentrates on providing QoS at the O.S. level. Its main difference is the definition of
more complex specification and translation mechanisms based on the QL language.

Nevertheless, Arcade sti ll suffers from the same limitations that prevent the use of the
systems described previously for providing QoS in open systems.

3.7  OM EGA and The QoS Broker (Univ. of Pennsylvania)

The OMEGA Architecture [101]  is a QoS architectur e for provision of real - time
guarantees in distributed multimedia systems. In order to provide service guarantees, the
research effort focused on local and global resource management in distributed systems.

The QoS Broker [102]  is the main component of the OMEGA Architecture. It is
basically a middleware component responsible for the negotiation of QoS levels to be
delivered to the application by the underlying system. The requirements specified by the
application are translate d by the QoS Broker and result in the negotiation of resource
allocations with the operating system and the network.

Resource reservation is based on QoS parameters associated to the specific media
device, and handled internally by the QoS Broker. A trans lator is employed to obtain
lower - level QoS requirements from the application - level parameters specified by the
user, adopting a fixed set of translation relations for each media type. The translation is
bi - directional, allowing dynamic changes in resource  reservations to be reported to the
user as application - level QoS parameters. The obtained parameters result in the
reservation of network and operation system resources, both local and remote.

Consequently, a local QoS Broker aiming to perform reservation s of remote resources,
called a `buyer´, is responsible for interacting with other QoS Brokers located remotely,
known as `sellers´ of resources. A `buyer/seller protocol´ is provided by the architecture
to allow sellers to advertise their services and buy ers to contact sellers and therefore
avail of their resources.

The QoS Broker employs orchestration services (i.e. mechanisms for balancing resource
usage) and relies on information stored in resource databases to achieve a balance
among the resources tak en from multimedia devices, operating systems and the
network. The underlying operating system is assumed to have real - time capabilities,
allowing that its temporal behaviour be predicted by the QoS Broker and used to
perform the orchestration of resources .

In addition to the QoS Broker, the OMEGA Architecture provides a communication
model that consists of two protocols at distinct abstraction levels. The Real - Time

Application Protocol (RTAP) is responsible for tasks such as call management, device
manage ment, synchronisation, and media delivery at application level; and the Real -

Time Network Protocol (RTNP) implements functions for connection management,
error correction, rate control, and network access at the transport level. These protocols
provide gua ranteed communication services over specified communication channels,
which are obtained by applications and configured by them through the QoS Broker.

The OMEGA architecture and the QoS Broker were validated through two practical
experiments [104] . In the first application, a robot interconnected to a dedicated ATM
network was operated and monitored remotely by workstations running the AIX
operating system with real - time extensions. In the second example, a video - on - demand
app lication with lip synchronisation was implemented on a platform composed by SGI

Indy machines running the IRIX operating system, interconnected by a 10Mbps

Ethernet LAN.

OMEGA has more complete QoS enforcement mechanism than the architectures
described in  the previous sections. Besides being able to perform reservations at both
operating system and network levels, OMEGA provides a complete QoS translation
mechanism that makes the underlying platform transparent for the application.

However, OMEGA does not allow the application programmer to extend the
architecture, does not offer provision for multiple reservation protocols, and its support
for adaptation consists of simple notification mechanisms.

3.8  QoS - A (Univ. of Lancaster)

The Distributed Multimedia Resea rch Group at Lancaster University have developed a

QoS Architecture, called QoS - A [24] , which offers a framework for specifying and
implementing the required performance properties of multimedia applications over
high - performan ce ATM - based networks.

The architecture incorporates the following notions to an environment composed of
machines interconnected by an ATM network:

·

                         flow: single media streams that represent the production, transmission and

                         consumption of media data;

·

                         ser vice contract: agreement between users and service providers regarding the QoS

                         level to be achieved; and

·

                         flow management: monitoring and maintenance of the contracted QoS levels.

QoS - A makes possible the provision of data flows with an associated level o f QoS
through the tight integration between devices, end - system and network. QoS - A provides

`system - wide´ QoS, including end - systems, communications systems and networks,
through the use of QoS mechanisms that span across all architectural layers.

A struc ture of layers and planes integrated with the layers and planes of the ATM
architecture (see Figure 3  in Section 2.6.2 ) provides a QoS - configurable communication
mechanism, while thread scheduling algo rithms based on QoS constraints provide the
desired behaviour at system level. In addition, devices are built with the intent of taking
advantage of both scheduling and communication with QoS capabilities.

Three planes compose the QoS - A architecture:

·

                         the  Protocol Plane is responsible for data transfer. It is subdivided into a user plane,

                         for transmission of media data, and a control plane, responsible for control data,

                         because of the essentially different requirements of these distinct categories of data.

·

                         the QoS Maintenance Plane is responsible for monitoring and maintaining the QoS

                         levels specified by the user in the service contracts that are accepted by the

                         architecture. Based on the information monitored from the system, this layer

                         configures the ava ilable resources aiming to provide the QoS levels agreed with the

                         user.

·

                         the Flow Management Plane executes flow establishment procedures (including

                         admission control and resource reservation), QoS renegotiation, QoS mapping and

                         translation, and QoS adapta tion.

The first two planes are subdivided into layers as follows:

·

                         the distributed systems platform provides services for multimedia communication

                         and QoS specification.

·

                         the orchestration layer is responsible for media synchronisation and jitter correcti on.

·

                         the transport layer provides a basic QoS - configurable communication service.

·

                         the lower layers ˘  network, data link and physical layer ˘  provide the basis for the

                         communication service.

QoS - A is implemented over an enhanced Chorus micro - kernel and en hanced protocols
for multimedia built on a local ATM network. Like OMEGA, it is able to translate QoS
requirements and reserve resources provided by both the network and the operating
system. Its QoS adaptation mechanism is more complex than the one provid ed by

OMEGA, since it is able to perform transparent QoS adaptation (i.e. without involving
the application) and not only notify the application when QoS changes. However,

QoS - A still has limitations similar to the ones present in OMEGA and that make both
architectures unsuitable for open environments. QoS - A is not able to interact with
different resource reservation protocols due to its tight integration with the underlying
system. In addition, its area of application is constrained to multimedia systems,  and its

QoS mechanisms cannot be extended by the application programmer.

3.9  QuO (BBN Systems and Technologies)

The Quality of Service for CORBA Objects (QuO) architecture [156]  provides QoS
abstractions that can be used by CORBA objects distributed in a wide area network.

QuO extends CORBA´s Interface Description Language (IDL) with a QoS Description
language (QDL).

The QDL language allows QoS to be described at object level (i.e. methods per second)
instead of at communication l evel (i.e. bits per second). By using QDL, users describe:

    ·

                             QoS contracts between a client and a server object in terms of usage of the server

                             and the QoS requirements imposed on services provided by the server;

    ·

                             the internal structure of objects and the amo unt of resources they require; and

    ·

                             the resources available in the system and their status.

QoS regions can also be described with QDL, allowing the application to adapt to
changing conditions by changing from one QoS region to another.

QuO defines archi tectural components that are responsible for dealing with QoS
enforcement, measurement and adaptation on behalf of the application. These
architectural components are regular CORBA objects that are generated based on the

IDL and QDL descriptions.

QuO prov ides a complete framework for application development that reduces the
programming effort required for writing applications with QoS requirements. However,
it still has limitations similar to the ones present in OMEGA and QoS - A. Despite being
compatible wi th CORBA, its use in open systems is limited by the fact that there is no
support for multiple reservation protocols. In addition, its efficiency as a programming
support is limited by the fact that the CORBA object model is not suitable for most real -
time  and multimedia applications.

3.10  QUANTA (Old Dominion University)

The Quality of service Architecture for Native TCP/IP over ATM networks (QUANTA)

[43]  is an architecture that provides mechanisms for QoS specification and enforcem ent
for applications by using communication services based on Internet protocols running
over ATM.

Basically, it allows applications that need a network service with predictable
performance to specify a region of operation (ROP) in terms of user - level QoS
parameters. Applications are characterised according to classes of service, such as the
classes defined for ATM. Each class has a translator that converts parameters specific to
that class into generic network QoS parameters, such as throughput, delay, lo ss, etc.

These generic parameters are then translated into end - system protocol - dependent
control parameters by a protocol - dependent translator. These parameters are used to
configure the lower - level network service.

QUANTA supports TCP/IP and UDP/IP over AAL5/ATM, and AAL5/ATM directly.

The communication protocols are optimised in order to apply scheduling algorithms on
the delivery of packets, according to the class of service of the application.

Feedback is received from the network by a resource manage r, which uses this
information for performing adaptation at network and application levels. The resource
manager is a global component that maintains information about all the resources in the
system. Whenever necessary, the resource manager modifies the p arameters of the
packet scheduling algorithm in order to fulfil the QoS requirements of the application.

Ultimately, it is capable of degrading the performance of applications by changing their
region of operation.

QUANTA was implemented on an infrastruct ure consisting of Sun workstations with

ATM cards connected to two Fore Systems ASX - 100 switches, which provide a
maximum bandwidth of 100 Mbps. The necessary alterations at protocol level are made
possible by using the Streams package provided by Sun Micr osystems.

Despite providing support for QoS enforcement only at network level, QUANTA offers
a solid platform for the development of applications with QoS requirements situated in
different application areas and running on diverse network and reservation p rotocols.

Nevertheless, its support for adaptation is limited, and the architecture cannot be
extended by the application programmer in order to use different resource reservation
protocols.

3.11  ERDoS (SRI International)

ERDoS (End - to - End Resource Management o f Distributed Systems) [26] [27] [143]  is a
middleware infrastructure capable of providing QoS support for applications with soft

QoS requirements. By using the support pr ovided by ERDoS, applications with soft

QoS requirements such as multimedia applications are able to run on top of non real -
time systems. This is achieved by using QoS adaptation techniques that minimise the
adverse effects of the non real - time behaviour o f the system on the application.

ERDoS is a three - layer architecture that separates applications from the computing,
storage and communication resources that constitute the system. At the higher layer,
application agents translate application - specific QoS  requirements into end - to - end QoS
metrics understood by ERDoS. The middle layer is composed by the system manager,
which houses the adaptive resource management algorithms. These algorithms, based
on the global view of the system and on the requirements of  the applications, decide
which applications to degrade in case of resource shortage. At the bottom layer,
resource agents monitor the behaviour of the resources present in the system and notify
the system manager when the QoS of an application is missed. Whenever the
occurrence of resource shortage is detected, the system manager selects one or more
applications that are requested to adapt their requirements, allowing other applications
to meet their QoS requirements.

ERDoS provides a development toolkit t ogether with an instantiation environment and a
run - time support. This infrastructure helps the programmer to write new applications on
top of ERDoS and to instantiate applications stored in an application repository.

Resource agents have been implemented on Solaris, QNX and Real - Time Mach.

ERDoS distinguishes itself from the other QoS architectures presented before in this
chapter by the use of purely adaptive techniques instead of relying on QoS enforcement
mechanisms. Purely adaptive techniques provide o nly best - effort QoS guarantees, since
they do not use admission control policies. Consequently, ERDoS is unsuitable for
applications with more severe QoS constraints, such as hard real - time applications and
some commercial multimedia applications (e.g. pay - per - view). ERDoS also has better
support for open systems than the architectures described previously in this chapter due
to the use of multiple protocols and due to the capacity of extending its QoS
specification and adaptation mechanisms. However, it is  unclear if the application
programmer can write new application and resource agents in order to extend the
architecture or if only the developers are able to do it.

3.12  M M N Project (BT - URI)

The Management of Multiservice Networks (MMN) project [147]  is a British Telecom

University Research Initiative (BT - URI) concerned with the provision of support for

QoS management within distributed multimedia middleware environments using
integrated services networks (i.e. ATM). The project c omprises a five - year plan for six
research institutions in the United Kingdom (University College London, University of

Cambridge, Imperial College, University of Lancaster, Loughborough University and

Oxford Brookes University).

Applications with QoS req uirements are supported by MMN through the adoption of a

CORBA - based object model together with mechanisms for the streaming of continuous
media. Extensions to CORBA are proposed in the form of an enhanced object model

[37] . St reams are implemented as binding objects (inspired on the binding objects used
by the Xbind architecture) and defined by using augmented interface definitions.

At the highest level of abstraction, a Component Definition Language (CDL) is used by

MMN to def ine the overall composition and configuration of objects within the
distributed environment. CDL encapsulates the IDL interfaces and incorporates the
features introduced by MMN, such as QoS specifications and streams.

At the lower level, mechanisms for res ource management are provided by the

Distributed Resource Management Architecture (DRMA) [150] . DRMA uses resource
capacity regions to describe the resources that have to be allocated by the architecture in
order to guarantee t he QoS requirements imposed by applications. In order to control
the use of these resources, DRMA provides a set of resource adaptation mechanisms.

These mechanisms are responsible for monitoring the use of the resources provided by
both the network and th e operating system, and for initiating resource adaptation
whenever the boundary of a resource capacity region is reached.

A framework for building communication protocols from reusable components is also
part of the MMN project. Components may be primiti ve or constructed from other
components. The flexible structure of the communication system allows protocol layers
to be added to or removed dynamically from the protocol stack during the lifetime of a
communication session in order to react to changing le vels of QoS.

A set of graphical tools, textual notations and design methods for configuring systems is
also proposed for the management of the network services, including QoS mechanisms.

Configuration management tools provided by the framework aim to simp lify the
specification of distributed services, and are able to instantiate components, bind
interfaces, and allocate components to nodes. Dynamic configuration allows protocol
developers to redefine the component structure of the communication system and to
recover from component failures. In addition, developers can group objects in domains
and divide configuration management responsibility.

The different experiments that make up the MMN project are being performed using a
number of different distributed programming platforms, including Darwin/Regis,

AnsaWare, Xerox Parc ILU and Orbix. The final objective of MMN is to fully integrate
all the proposed features into a CORBA - compatible architecture suitable for multimedia
applications.

MMN is an ongoing proje ct, and most of its results still remain to be validated.

Nevertheless, the design principles adopted in the MMN project make us believe that,
despite providing support for heterogeneity through the configurable and extensible
component - based communication  system, its applicability is constrained to a limited
area of application. This occurs due to the adoption of resource adaptation techniques in
detriment of QoS enforcement mechanisms together with QoS specification
mechanisms and an object model that is suitable only for applications with soft QoS
requirements.

3.13  Analysis of the State of the Art Technology

Our study of the state - of - the - art revealed that several partial solutions for the provision
of services at the middleware level for applications with QoS  constraints are available in
the literature. However, a generic middleware for QoS - aware applications in open
systems still remains to be proposed. Tab le 5  shows the features desired to be present in

QoS architectures in four dif ferent areas: QoS specification, QoS enforcement, support
for heterogeneity and support for QoS adaptation. These features are then compared
with the ones provided by state - of - the - art QoS architectures and frameworks.

We have identified middleware that eff iciently targets limited application areas such as
distributed multimedia (e.g. Xbind) and real - time processing (e.g. TAO), and are
typically concerned only with constraints found at either network (e.g. DIMMA and

QUANTA) or operating system levels (e.g. S UMO and Arcade). In addition, most of
the work in this area of research limits its target platform by adopting architectural
designs highly dependent on a particular platform, with the most common case being

ATM networks.

X
b
i
n
d

R
e

T

I

N

A

D

I

M

M

A

S

U

M

O

T

A

O

A
r
c
a
d
e

O

M

E

G

A

Q
o

S

˘

A

Q
u

O

Q

U

A

N

T

A

E

R

D
o

S

M

M

N

Multimedia Support

>

>

>

>

>

>

>

>

>

>

>

                                                                                                            Real - Time Support

>

>

>

>

>

>

>

                                  QoS

     Specification

Extensible

>

>

                                                                                                      Network Reservation

>

>

>

>

>

>

>

                                                                                                                    O.S. Reservation

>

>

>

>

>

>

                                  QoS

      Enforcement

Transparent

>

>

>

>

>

>

>

                                                                                                                 Multiple Protocols

>

>

>
           Support for

   Heterogeneity

Extensible

>

>

Notification

>

>

>

>

>

>
           Support for

            Adaptation

Transparent

>

>

                                                           Tab le 5  ˘  Features Provided by State - of - the - art QoS Architectures

The lack of support for multiple reservation protocols and of support for extending the

QoS mechanisms present in architectures such as QoS - A and OMEGA constrain their
u se in open systems. Furthermore, adaptation mechanisms can be limited (e.g. in QuO)
or completely absent (e.g. in ReTINA). When adaptation mechanisms are available,
they often try to replace the use of QoS enforcement mechanisms, such as in ERDoS
and MMN, resulting in a support suitable only for applications with soft (i.e. best - effort)

QoS requirements.

The features necessary for providing support for diverse applications with QoS
requirements in open systems were taken into account during the developmen t of a new

QoS architecture, called Quartz, which is presented in the next chapter of this thesis.

Design of the Quartz

QoS Architecture

This chapter introduces Quartz, a generic QoS architecture designed specifically to
address the requirements of s upporting diverse applications with QoS constraints in
open systems. We begin by describing the main requirements imposed on the
architecture. We then describe in detail the architectural design adopted to address these
requirements. The approach adopted i n the design of Quartz results in a very flexible
and extensible architecture, capable of supporting multiple areas of application and
different underlying systems as required to provide QoS - constrained services in an
open, distributed and heterogeneous en vironment.

4.1  Requirements

A complex combination of requirements has to be addressed by a QoS architecture in
order to provide support for applications that require QoS - constrained services in an
open environment. The fulfilment of these requirements represe nts an important
challenge in the development of QoS architectures.

4.1.1  Requirements on the Specification of QoS

As discussed in section 2.5.2 , a QoS architecture must allow high expressive power in
the specification of QoS requir ements. QoS requirements should be specified according
to the notion of QoS understood by the user at his level of abstraction. Any limitation
constraining the expressiveness of the user would force him to deal with a notion of

QoS with which he is not fam iliar, and would reduce the applicability of the
architecture.

Furthermore, since different notions of QoS might be present at the application level
because of the multiplicity of application areas that are targeted by the architecture,

Quartz must be abl e to interpret a potentially infinite set of QoS parameters. This might
be achieved by adopting mechanisms that would allow the architecture to be extended
in order to understand new QoS parameters.

The parameters specified by the user must be interpreted accordingly by the architecture
in order to perform the reservation of resources at the lower level of abstraction. This
implies translating the parameters from their original format into parameters that are
understood internally by the architecture. The a rchitecture has also to map these
parameters into resources available at the lower level and then interact with a suitable
reservation protocol in order to allocate the corresponding resources for use by the
application. This mapping process might not alwa ys be one - to - one (i.e. one QoS
parameter resulting in one kind resource to be reserved) but can be one - to - many, many -
to - one or many - to - many ( Table 2  in section 2.5.3  shows examples of parameter
mapping s). This implies that resources might be interchangeable, and that finding an
appropriate balance between requirements and resources is another task that has to be
performed by the architecture.

These requirements imply that a sophisticated mechanism for s pecification of QoS
parameters and interpretation of this information must be adopted by the Quartz
architecture in order to fulfil the QoS requirements imposed by applications.

4.1.2  Requirements on the Enforcement of QoS

After feeding the QoS architecture wit h information to identify itself together with its

QoS requirements, applications are not obliged to use directly any QoS mechanism
available at the lower - level. Applications can rely on the QoS architecture, which will
enforce the required QoS by interpre ting the QoS requirements specified by the
application and then use the reservation protocols provided by the network and the
operating system in order to reserve resources.

In addition, the QoS architecture must provide transparency of reservation mecha nisms
from the application´s point of view. Transparency is necessary in order to reduce the
amount of work needed for applications to impose requirements on services that they
avail from the underlying system.

Adopting this strategy for QoS enforcement, we hide from the application the
differences between the way different lower - level systems allow resources to be
reserved in order to fulfil QoS requirements. This has the important effect of increasing
the portability of applications across different plat forms.

4.1.3  Support for Heterogeneity

The QoS architecture is expected to provide features that make it appropriate to be used
in open, distributed and heterogeneous environments. This implies that the architecture
is required to be able to use the different pr otocols and hardware that coexist in an open
environment.

For example, if the application is able to transfer data using both ATM and TCP/IP, the

QoS architecture has to be able to perform QoS reservations for both protocols. This
should be done by the ap plication by adapting itself internally instead of requiring a
different implementation of the architecture to be linked to the application code. In
order to achieve this goal, the Quartz architecture is not only required to be portable to
different platfo rms, but it has also to able to handle QoS for an application when the
underlying reservation system changes (for example, in case of hardware
reconfiguration or failure) without requiring a recompilation. This level of flexibility
might be achieved by usi ng an architectural design based on interchangeable
components, in which components able to handle QoS for different reservation
mechanisms can be plugged into the architecture dynamically.

In addition, by concentrating the task of dealing with a reservat ion protocol within a
single component, support for new reservation protocols can be added to the
architecture without the necessity of porting the whole infrastructure. Instead, this is
achieved by providing a new component that is able to handle the new reservation
protocol. This adds to the architecture the capacity of interacting with the new
reservation protocol, and providing the resources made available through this protocol
to applications built on top of the architecture.

4.1.4  Support for QoS Adaptation

The QoS architecture is required to allow dynamic changes in the distribution of
resources to be performed by the system in order to interact properly with any adaptive
protocols that might be present at lower level. This must occur without causing loss o f
service consistency at application level.

As discussed in section 2.6.1 , the reservation of resources might change because of
dynamic changes in the structure of the system, resource failure or the usage of
prioritised polic ies for the distribution of resources. Resources might also be claimed
back by the system when an irregular resource usage pattern is detected by monitoring
mechanisms.

Any change in the reservation of resources at lower - level must be made known to the
app lication by using QoS parameters that are understood at its level. This implies that
the QoS architecture has to perform a reverse translation of parameters and then inform
the application that its QoS has changed.

Since in some cases resources are interch angeable, dynamic changes may be overcome
at lower level by requesting additional resources managed by a different resource
reservation protocol. In this case, all the adaptation is masked at the lower level and the

QoS seen by the application remains the same.

4.2  The Quartz Architecture

This section describes the QoS architecture proposed in this thesis. The following sub -
sections identify the main architectural components and define their role in the
provision of services subject to QoS requirements. The int erfaces of the components of
the architecture and the messages exchanged between them are also described.

4.2.1  Overview  of the Architecture

The Quartz QoS architecture is composed of a QoS Agent running on top of the several
resource reservation protocols avai lable in the host system. Applications use the
services provided by the QoS Agent to obtain the desired level of QoS from the system.

Figure 6  situates the Quartz architecture in a computational system. At the application
level, applications with QoS requirements (such as multimedia applications, real - time
applications, or any other application with QoS requirements) interact with Quartz
through interfaces that are specialised for the corresponding area of application.

  Application

  Lev el

  Middleware

  Lev el

  Underl yi ng

  S ystem

Network

                                                                                                                        Resources

O.S.

Resources

O.S.

Resources

Network

Resources

Quartz QoS Agent

CSCW

                                                                                                                       Application

Real-T ime

Application

Multimedia

Application #2

Multimedia

Application #1

Applet #3

Applet #2

Applet #1

...

...

...

...

                                                                                                             Figure 6  ˘  Overview of the Quartz QoS Architecture

The QoS Agent , which is the major component of the Quartz architecture, receives the

QoS requirements specified by applications and interacts with the underlying system in
order to enforce these requirements.

The location of the QoS Agent in the distributed environment is an implementation
issue. In most implementations of Quartz, the QoS Agent is likely to be located on the
same machine as the application, and may  be either linked to the application (i.e. one

QoS Agent per application) or running as a system service (i.e. one QoS Agent per
node). The mechanism used by the application to interface with the QoS Agent is also
implementation - dependent, and can be one o f sockets, local or remote method calls,

RPC, etc. Communication between different QoS Agents is not necessary, since the
tasks that require a deeper knowledge of the capabilities of the (possibly distributed)
application or that require a global view of t he underlying system are solved at their
corresponding levels of abstraction, and are outside of the scope of the architecture.

Consequently, issues such as QoS negotiation between peers (e.g. in a client - service
style interaction between applications) and  service degradation due to resource
adaptation are handled directly by the application, while other issues such as interaction
with other resource providers (e.g. along a network path) are dealt with by the
reservation protocol.

The underlying system cont ains resources that are used by the application. It is typically
composed by several sub - systems, which can be grouped in two main areas: the
network infrastructure (e.g. ATM or Internet protocols) and the operating system (e.g. a
real - time or desktop oper ating system with reservation capabilities). Networks and
operating systems are seen as resource providers by the QoS Agent. The resources
themselves are not represented in the figure because the manner in which they are
structured varies significantly, an d this would be impossible to represent. Each resource
provider allows its resources to be allocated through a resource reservation protocol.

The QoS Agent must know how to interact with each of the resource reservation
protocols present in the system, usi ng their interfaces in order to allocate resources on
behalf of applications.

There are no severe assumptions on the behaviour of the reservation mechanisms
provided by the resource providers present in the underlying system. In case a particular
resource  provider does not supply a resource reservation protocol but provides simple
mechanisms for accessing resources, similar behaviour might be achieved by placing a
resource management layer between the QoS Agent and the resource provider ( [92]  is
an example of how this can be done). This layer would be responsible for controlling
and administering the resources made available by the corresponding resource provider.

In addition, it would monitor the availability of resources and i ssue notifications when
thresholds that prevent the QoS requirements of the application to be fulfilled are
reached. Similarly, any lack of functionality in a particular resource reservation protocol
can be complemented or masked by a management layer plac ed on top of the
reservation protocol.

4.2.2  Internal Structure

The QoS Agent is a placeholder into which other components can be plugged in order to
interact with the surrounding environment. In general, the QoS Agent is responsible for
giving access to the un derlying QoS mechanisms necessary for providing services with
the quality requested by the application. The QoS requirements imposed by the
application are enforced by reserving resources provided by the underlying system. The
sub - systems present in the un derlying system provide the actual means of organising the
access to its resources by offering a resource reservation protocol. Because of the
intrinsically open nature of the target environment, several component - specific
reservation protocols may be avai lable.

The QoS Agent is responsible for two main tasks:

·

                         Interpreting the QoS requirements specified by the application in the form of QoS

                         parameters, translating them from the format understood by the application into a

                         format suitable for performing reso urce reservations; and

·

                         Interacting with the underlying resource reservation mechanisms in order to allocate

                         the resources necessary to perform the service subject to QoS requirements.

Being a placeholder for other components, the QoS Agent does not perfo rm these tasks
directly. Instead, it relies on other components that are specialised for translation of QoS
parameters and interaction with resource reservation protocols. Since the translation
process depends directly on the application and on the resourc e being used, and since
the interaction with the reservation protocol depends on the interface provided by this
particular protocol, specialised components will be used for performing each of these
tasks. These components will be plugged into the QoS Agent  whenever necessary. The
resulting internal structure of the QoS Agent is represented in Figure 7 .

The translation of QoS parameters between the different formats used at different levels
in the architecture is performed by the t ranslation unit . In addition, the translation unit
balances the usage of interchangeable resources provided by the different sub - systems

(i.e. the network and the operating system) present in the underlying system.

The translation unit contains QoS Filter s  and a QoS Interpreter . QoS Filters can be
subdivided into application and  system filters , one for each application field and for
each sub - system present at the lower - level, respectively. Filters are responsible for
translating between QoS parameters unde rstood internally by Quartz and any external
format. The QoS Interpreter handles parameter formats used internally by Quartz at
different abstraction levels and balances requirements between sub - systems present at
the lower level.

                                                                                                                         Quartz Qo S Agent

 Network O.S.

Quartz Application

 Translation Unit

Application Filter

QoS Interpreter

Application-Specific QoS Parameters

Generic Application-Level QoS Parameters

System Filter System Filter

Generic System-Level QoS Parameters

System Agent

System Agent

Reservation

Protocol

Reservation

Protocol

System -Specific QoS Parameters

Figure 7  ˘  Detailed Structure of the QoS Agent

The QoS Agent also encapsulates multiple system agents , which are responsible for
interacting with reservation protocols administering the use of the resources provided by
the underly ing system. The system - specific agents get the values of QoS parameters
determined by the translation unit and perform the reservation of the resources provided
by the corresponding sub - system (i.e. the network or the operating system) by using the
associa ted reservation protocol.

The following sections detail the role played by each component of the architecture and
specify their external interfaces.

4.2.3  The Translation Unit

A translation mechanism based on the use of a set of generic parameters is adopted b y

Quartz to encompass the problem of specification of QoS requirements in an
environment composed of multiple application areas and different reservation protocols.

In order to avoid having a translator for each combination of application field and
reserv ation protocol, we have adopted a three - step translation process. Users specify
their application - specific QoS parameters , which are first translated into a set of generic
application - level parameters  defined by Quartz. These parameters are further transla ted
into a set of generic system - level parameters  and balanced between the network and the
operating system. Finally, generic system - level parameters are translated into system -
specific QoS parameters  understood by each of the reservation protocols used by  the
application.

Despite the definition of two standard sets of generic parameters, the expressiveness of
users is not affected because they deal only with QoS parameters understood at they
level of abstraction and meaningful for his application field. T his is made possible by
the adoption of application - specific filters that handle QoS parameters understood at
application level. The same occurs at the system level, where system - specific QoS
parameters are used in order to provide a bridge between the gen eric parameters used
internally by Quartz and the parameters understood by the reservation protocols present
at the lower level.

The translation unit ˘  and the components that form it ˘  implement two paths of
translation:

·

                         the direct path of translation, w hich goes from the application to the lower layers of

                         the architecture and that is used when the application requests the provision of QoS -

                         constrained services; and

·

                         the reverse path of translation, which goes from the lower layers towards the

                         application and is used to inform the application of changes in QoS caused by

                         dynamic adaptation of the resources allocated by the underlying system.

The translation paths are illustrated in Figure 8 .

Application-Specific QoS Parameters

Generic Application-Level QoS Parameters

Generic S ystem-Level QoS Parameters

S ystem-Specific QoS Parameters

                          Direct Path

                                                          of

                          Translation

Reverse Path
of

Translation

Figure 8  ˘  Translation Paths

The components that form the translation unit ˘  i.e. application and system filters and
the QoS interpreter ˘  accept two types of message through their public interfaces,
illustrated by Figure 9 . The first one,

TranslateQoSDownwards
, results in upper -
level parameters being translated into lower - level ones. This message is issued by a
component situated a level of abstraction above the component receiving the message,
following through the di rect path of translation. The second type of message,

TranslateQoSUpwards
, implements the reverse path of translation and is used when

Quartz needs to inform the application that the QoS parameters have changed due to
resource adaptation. This message is i ssued by a component located a layer below the
component that receives the message.

TranslateQoSDownwards

TranslateQoSUpwards

Translation Component

Figure 9  ˘  Interface of Translation Components

4.2.4  Application Filters

An application filter is associated with a particular a rea of application. Applications that
have similar notions of QoS are expected to employ the same application filter,
specifying QoS requirements by using the same set of application - level QoS
parameters. On the other hand, applications that have different  ways of expressing QoS
requirements use different sets of application - level QoS parameters, and consequently
require different application filters.

Application filters obtain QoS parameters understood at application - level for the
particular area of applic ation, interpret them, and determine the values of a pre - defined
set of generic application - level QoS parameters, which are used internally by Quartz.

The reverse translation process ˘  i.e. from generic application - level QoS parameters
into application - spe cific QoS parameters ˘  is also implemented by application filters.

For the application filter, receiving a message of type

TranslateQoSDownwards
results in translating the application - specific QoS parameters carried by the message
into generic application - level QoS parameters. The second type of message,

TranslateQoSUpwards
, performs the reverse process of translation.

4.2.5  The QoS Interpreter

The translation between parameters related to different levels of abstraction is executed
by the QoS Interpreter provid ed by the architecture. By using a fixed (but still user -
replaceable) component for the main translation step, we simplify the work done by
application and system filters, making it easier for the application programmer to write
replacement filters wheneve r they become necessary.

The QoS interpreter also balances parameters between the sub - systems present at the
lower level, i.e. the network and the operating system. This is performed by a balancing
unit  encapsulated within the QoS interpreter. The balancin g process is necessary
because resources present at lower - level may be interchangeable, and a trade - off has to
be reached between using more or less network resources in comparison to operating
system resources. Resource balancing at this level is made pos sible because of the
definition of generic parameters that are used by Quartz internally. The trade - off
between requirements that are interchangeable for a particular application (e.g. the
decision of performing data compression and then require less bandw idth and more
processing power) has to be handled directly by the application. Alternatively, this
decision can be made by the application filter. Similarly, the trade - off between
interchangeable O.S. resources and between interchangeable network resources  has to
be decided by either the resource reservation protocol or by the corresponding system
filter, since only them have the knowledge necessary to perform balancing at this level.

The interface of the QoS interpreter is the same as the other translatio n components.

Whenever it receives a

TranslateQoSDownwards
 message, the QoS interpreter
translates generic application - level QoS parameters into generic system - level QoS
parameters, balancing them between the network and the operating system. On the other
hand, a

                                                          TranslateQoSUpwards
 message results in generic system - level parameters
being translated into generic application - level parameters. The QoS parameters carried
by the

                                                       TranslateQoSUpwards
 message do not necessarily reach the application
because transp arent QoS adaptation can be performed by Quartz, compensating the
resources lost during adaptation with resources obtained from another resource
provider. The process of QoS adaptation is described in detail in item 4.4.1 .

4.2.6  Syst em Filters

System filters are associated with sub - systems present in the underlying system. These
filters can be subdivided into network filters and operating system filters, according to
the sub - system with which they interact. Since sub - systems that can be present in the
underlying system use different forms of representation for QoS parameters, a different
system filter is provided in order to interpret these parameters.

In order to obtain the value of the system - level QoS parameters understood by the
un derlying reservation mechanisms, system filters translate the generic system - level
parameters used internally by Quartz. In case of a dynamic change of system - level QoS
parameters caused by resource adaptation, these parameters are translated upwards by
th e system filter.

Direct and reverse translation are performed by system filters upon receipt of the

TranslateQoSDownwards
 and

TranslateQoSUpwards
 messages respectively.

4.2.7  System Agents

Quartz is able to handle the differences between multiple reservation pr otocols by using
system agents.

Different resource reservation protocols provide distinct interfaces for applications
using them. Consequently, applications targeting heterogeneous systems have to be able
to handle these different interfaces in order to r eserve the resources provided by the
system. In Quartz, each different reservation protocol is associated with a corresponding
system agent, which hides differences among protocols by providing a common
interface to the rest of the architecture.

A system agent allocates the resources necessary for the application to fulfil its QoS
requirements by using the resource reservation protocol associated with it. The QoS
requirements specified by the application in the form of QoS parameters meaningful at
applicat ion level are interpreted by the translation unit and passed on to the system
agents corresponding to the reservation protocols present in the underlying system. The
system agent then uses the interface provided by the associated resource reservation
proto col in order to allocate the resources that are necessary to fulfil the requirements
specified by the application.

In addition to enforcing QoS requirements by means of resource reservation, system
agents receive notifications from the lower - level system w henever a resource fails or is
claimed back by the system. This notification is carried towards the upper layers of the
architecture, passing by the reverse translation path provided by the translation unit until
potentially reaching the application.

QoSRequest

  QoSReport

Protocol-Specific Interface

S ystem Agent

Resource Reservation Protocol

Figure 10  ˘  Interface of Component Agents

The interface of the system agent is illustrated in Figure 10 . Interfacing with system
agents takes place via two different types of message:

QoSRequest
 and

QoSReport
.

The first message is sent to the system agent in order to request the provision of QoS -
constrained services, and carries the QoS parameters corresponding to the requirements
imposed by the application translated into the parameter  format understood by the
system agent. The second type of message is produced by the system agent in order to
indicate that QoS has changed at lower - level, and carries the new level of QoS
supported by the system after the changes.

4.2.8  The User Interface

The  QoS Agent provides a very simple interface to the QoS Application. The messages
exchanged between the QoS Agent and the application and the interface between the

QoS Agent and the reservation protocols provided by the underlying system are
represented in Figure 11 .

To request a service with a specific level of QoS to be provided by the environment, the
application issues a

QoSRequest
 message. This message carries a list of variables
identifying the QoS parameters and setting thei r respective values.

QoSRequest

  QoSReport

  Protocol-Specific Interface       Protocol-Specific Interface

O.S. Resource

Reservation Protocol

QoS Agent

QoS Application

Network Resource

Reservation Protocol

Figure 11  ˘  User Interface of the QoS Agent

The application is notified about changes in the QoS provided by the system through

QoSReport
                                                                                   messages. This message is originated by the s ystem agent when it receives
a QoS notification from the reservation protocol through the protocol - specific interface,
informing that resource adaptation has occurred. The QoS parameters resulting from the
adaptation are translated upwards and delivered in  the form of a

QoSReport
 message to
the application. The application is then responsible for adapting the service to the new

QoS provided by the system, allowing a graceful degradation of the service provided to
the user.

It is important to notice that th e same format of messages is accepted by the individual
system agents. The main difference is that these messages carry parameters
comprehensible at application level, obtained directly from the application when QoS is
requested or after the translation pr ocess performed by the translation unit when a
dynamic adaptation occurs. Despite the differences in parameter formats, the user can
interact directly with an individual system agent by using the same message syntax.

4.3  QoS Parameters

As described before, the  Quartz QoS Architecture deals with four distinct classes of

QoS parameters depending on the level abstraction. Two of them are generic classes and
are standardised by the architecture: the generic application - level QoS parameters and
the generic system - le vel QoS parameters. The other two classes of parameters are
defined according to the application area or the resource reservation protocol.

4.3.1  Parameter Formats

Parameters are described as <name,value> pairs. To allow the easy identification of the
correspon ding abstraction level and consequently identify the translation process to
which the parameter has to be submitted, we have adopted a scoped namespace.

Parameters are scoped with the name of the abstraction level in which they are
meaningful.

Generic QoS  parameters are scoped with

App::
 and

Sys::
 for application -  and
system - level parameters respectively. System - level parameters are further subdivided
into two sets: a set of QoS parameters scoped with

Net::
 related to the network, and
another scoped with

O S::
 for parameters related to the resources which are provided by
the operating system. This is necessary to identify when the network and the operating
system share the responsibility for the fulfilment of a requirement (parameters scoped
with

                                    Sys::
                                                                                 ) or i s related to only one of them (and scoped with

Net::
 or

OS::
). For
example, a certain delay seen at application level is usually a global value which results
from the composition of two partial delays: one derived from the network and the other
from the op erating system. A bandwidth requirement is applicable only to the network,
while a requirement such as the class of service guarantee provided by the system (e.g.

best - effort, unloaded or deterministic) is valid for both the network and the O.S..

A simila r strategy is adopted for application -  and system - specific parameters. For
example, parameters for an MPEG rendering application could be scoped with

Mpeg::
,
subsequently translated into generic application parameters scoped with

App::
,   then
into system p arameters scoped with

Sys::
, and finally into system - specific parameters
scoped with

                                                                                           Rsvp::
 (for resource reservation protocol) and

Posix::
 (for POSIX -
compliant operating systems) for example.

In general, users specify parameters at their own abstraction level. In cases where they
want to specify the QoS to be provided by the system at a lower level, parameters can
be specified using the scoped name corresponding to the appropriate abstraction level.

These parameters will be ignored by the first translatio n steps and then caught by the
corresponding translation component.

When a parameter is described without a scope, the architecture assumes that it
corresponds to the current abstraction level.

In addition to scopes, parameter names can also be suffixed with the modifiers

Min

 and

Max

                            for specifying limit values.

4.3.2  Application - Specific QoS Parameters

These parameters are specific to the application area in which Quartz is being used. For
example, Quartz can be used in a multimedia environment in which QoS p arameters
such as `video frame rate´ and `resolution´ are adequate and require an application filter
able to understand them and translate them into the format used internally by Quartz

(i.e. generic application - level QoS parameters).

However, in a differ ent application scenario, such as in real - time systems, an
application would be more likely to express its QoS requirements in the form of
deadlines for the processing and for the transmission of data. In this case, a different
application filter, which un derstands different application parameters and translates
them into generic application - level QoS parameters, is adopted by Quartz.

The different sets of application - specific QoS parameters that are used by the
application examples built on top of Quartz w ill be described in section 7.1 .

4.3.3  Generic Application - Level QoS Parameters

Table 6  describes the generic application - level QoS parameters defined by the QoS

Architecture and recognised by the translatio n unit of the QoS Agent.

 Parameter Name  Modif iers  Description

 App::DataUnitSize  Min,Max
Size of data units produced by the application (in bytes)

 App::DataUnitRate  Min,Max
Rate of data units produced by the application (in units/s)

 App::EndTo EndDelay  Min,Max
Time between data production and consumption (in msec)

 App::ErrorRatio  Max
Acceptable error (in bits per million)

 App::Guarantee  ˙
Level of service guarantee (best - effort, unloaded, etc.)

 App::Cost  Max
Financial cost (currency per secon d)

 App::SecurityLevel  ˙
Security mechanism (none, encrypted, etc.)

                                                                                                          Table 6  ˘  Generic Application - Level QoS Parameters

Generic application - level QoS parameters represent the overall QoS requirements of the
application as they are s een at application level. At this level there is no distinction
between the sub - systems that are providing resources to the application.

The set of application - level QoS parameters has been chosen by observing the notion of

QoS present at the application level in different areas of application and then finding a
common way of representing QoS requirements at this level. As a result, we have
obtained a small set of QoS parameters that can be easily mapped into the different
forms of specifying QoS that are used in different areas of application.

4.3.4  Generic System - Level QoS Parameters

System - level parameters are subdivided into two groups: network and operating system
parameters. Table 7  lists and describes these parameters.

Parameter Name  Modif iers  Description

Net::Bandwidth  Min,Max
Bandwidth provided by the network (in bytes/s)

Net::PacketSize  Min,Max
Size of data packets (in bytes)

Net::Delay

                                                                                            and

                                                                                                                      OS::Delay
Min,Max
Transmission and processing delays (in seconds)

Net::Err orRatio  Max
Acceptable transmission error (bits per million)

Sys::Guarantee  ˙

Levels of service guarantee provided

(best - effort, unloaded, deterministic, etc.)

Net::Cost

                                                                                   and

                                                                                                             OS::Cost
Max
Financial cost (currency per second)

Net::SecurityLevel  ˙
Securi ty mechanism (none, encrypted, etc.)

Table 7  ˘  Generic System - Level QoS Parameters

At the system level, the division of requirements between sub - systems (i.e. the network
and the operating system) becomes clearly represented by the  definition of network and
operating system parameters, reflecting what is present in the underlying system. The
set of generic system - level parameters has been defined based on the parameters used
by resource reservation protocols present at lower level. The generic system - level
parameters are easily mapped into the QoS parameters used by a large number of
reservation protocols that may be present at network and operating system levels in an
open, heterogeneous environment.

 4.3.5  System - Specific QoS Parameters

 Different resource reservation protocols accept reservations based on different formats

 of QoS parameters. For example, despite both being network reservation protocols with

 similar capabilities, RSVP uses token bucket specifications compared to the bandwi dth -

 driven approach used by ATM. A similar situation occurs with reservation protocols

 provided by operating systems. Different scheduling algorithms and resource allocation

 schemes result in different ways to express QoS requirements at this level.

 Due t o the different ways in which resource reservation protocols are used to express

 QoS requirements, different formats of QoS parameters have to be used at the lower

 layers of the architecture. In order to accommodate these differences, Quartz employs

 multip le sets of QoS parameters, which are specific for a particular reservation protocol.

 These parameters have to be derived from the generic system - level QoS parameters

 generated by the QoS interpreter. System filters are responsible for this translation step .

 The different sets of system - specific QoS parameters defined by us to be used with the

 resource reservation protocols that are supported by the prototype of Quartz will be

 described in Chapter 5 .

 4.3.6  Translation Rules Betw een Ge neric Parameters

 There is a clear mapping between the two generic sets of QoS parameters defined

 previously. Table 8  describes the relationship between them. The mapping between

 generic parameters also takes into account the limit  values (i.e. maximum and minimum

 values) specified by the application.

                                                                                      At Application Level   At System Level

App::DataUnitSize * App::DataUnitRate
Þ

Net::Bandwidth

                                                                                   App::DataUnitSize
Þ

Net::PacketSize

                                                                               App::EndToEndDelay
Þ

Net::Delay + OS::Dela y

                                                                                            App::ErrorRatio
Þ

Net::ErrorRatio

                                                                                                App::Guarantee
Þ

Sys::Guarantee

                                                                                                                     App::Cost
Þ

Net::Cost + OS::Cost

                                                                               App::SecurityLevel
Þ

Net::SecurityLevel

                                                                                                                Table 8  ˘  Relationship between Generic Parameters

The division of cost and delay betwe en the network and the operating system is
calculated by the balancing agent encapsulated by the QoS interpreter. This calculation
is based on data structures kept by the balancing agent describing the state of the
network and the operating system in terms  of load, cost, and any other data useful to
obtain a balance in the use of resources from the network and the operating system. By
analysing this information, the QoS interpreter obtains the split factors that are used for
dividing QoS requirements betwee n the network and the operating system.

4.4  Additional Features

The following items detail two further important characteristics of the Quartz
architecture: its support for dynamic resource adaptation and rebalancing of resources;

and the capacity of the archi tecture to be reconfigured in order to support different
application areas and resource reservation protocols.

Dynamic resource adaptation is made possible by the monitoring of QoS notifications
sent by the resource reservation protocols and by translatin g QoS parameters from the
form used by each of the resource reservation protocols into the high - level format
understood by the application.

The reconfiguration of the architecture can take place by allowing the application
programmer to select the appropr iate components from a library or, in case they are not
available, by allowing him to write new components that can be plugged into the QoS

Agent.

4.4.1  Dynamic Resource Adaptation and QoS Adaptation

A common feature generally neglected by available QoS archite ctures is the provision
of support for dynamic resource adaptation.

Resource adaptation occurring at lower levels results in adjustments in the QoS
provided by the system to the application. Consequently, in addition to performing
reservations, a QoS arch itecture has to catch notifications issued by the resource
reservation protocol informing it of dynamic resource adaptation, and then proceed with

QoS adaptation at a higher level.

The QoS Agent catches notifications issued by resource reservation protocol s through
the corresponding system - specific agent and performs QoS adaptation when needed.

QoS adaptation can be performed by Quartz at both system and application level.

In some cases, resource adaptation can be accommodated by performing QoS adaptation
at system level, without interfering with the QoS seen by the application. In the Quartz
architecture, some QoS requirements such as cost and delay are fulfilled by the sum of
resources provided by both the operating system and the network. The component
responsible for dividing QoS requirements between sub - systems is the balancing agent,
which is basically a resource trader that is encapsulated by the interpreter.

When one of the operating system or the network reduces the resources allocated for the
appl ication, the balancing agent tries to execute a process called `rebalancing of
resources´. This process tries to compensate for the loss of resources from one side by
requesting more resources from the other. When this is possible, the resource adaptation
is compensated by rebalancing generic system - level parameters, and the QoS seen by
the application is not affected. In this case, the adaptation is completely transparent
from the application´s point of view. However, rebalancing of resources is possible o nly
with interchangeable resources, and it might fail in case additional interchangeable
resources are not available and cannot be allocated to compensate the loss of resources
that occurred due to adaptation.

If QoS adaptation at system level does not suc ceed, Quartz must start QoS adaptation at
application level. In this case, the QoS Agent tells the application to adapt its
requirements in order to decrease the consumption of resources. It sends a message to
the application indicating that its QoS requir ements will not be fulfilled because the
amount of resources originally allocated for it has been reduced. Consequently, it is
necessary for the application to adapt its QoS requirements in order to adjust its
behaviour to the resources available in the co mputing platform. This can be done by
reducing the quality of a video stream or by changing the compression method used for
data transfer for example. Alternatively, the degrading strategy can be implemented
within the application filter, which then become s responsible to decide how to degrade
quality on behalf of the application.

When the need to perform QoS adaptation at application level is reported to the
application, the QoS Agent must indicate the new QoS provided to the application after
the dynamic change in the allocation of resources. Since the application is unaware of
low - level details regarding the allocation of resources, the new QoS must be expressed
in the form of application - level QoS parameters. This is made possible by using the
reverse tr anslation path provided by the translation unit. In this case, a set of system -
specific QoS parameters is translated into application - specific QoS parameters.

Figure 12  illustrates how QoS adaptation occurs at both system and ap plication level. In
this example, a user is in his office and has his laptop connected to the local area
network. The user is taking part in a collaborative work session, and requests the
application to establish a connection with a maximum delay of 70 mil liseconds between
partners. This is achieved by the application by obtaining a 40 ms delay from the
network and allocating the remaining 30 ms for the operating system to perform data
processing. When the user leaves his office and prepares to leave the bu ilding, his
machine connects to the infrared network. However, this medium is unable to guarantee
the same delay, which has to be raised to 50 ms.

Offic e

Building

Street

OS Delay

Network Delay

Total Delay

0

10

20

30

40

50

60

70

80

90

100

                                                                                                                 Delay

                                                                                                             (ms ec )

Figure 12  ˘  Example of QoS Adaptation

Quartz is able t o compensate for this loss by raising the usage of operating system
resources, resulting in an O.S. delay of 20 ms. Consequently, the global delay is
maintained and the user doesn´t notice any change in QoS. When the user leaves the
building, the computer starts using the cellular network. In this case the network delay
rises to a value (80 ms) that can no longer be compensated by the operating system, and
then Quartz asks the user to adapt its requirements in order to accommodate a higher
delay.

4.4.2  Extending  the Architecture

The structure of the QoS Agent is highly portable, reusable and extensible, because the
particular needs of application fields and resource reservation protocols are
encapsulated by application filters, and system filters and agents resp ectively. Changes
at application or system level imply the replacement of filters and system - specific
agents, or the plugging of new ones into the QoS Agent. Since these components have a
standardised interface, they can be replaced in order to reflect cha nges in the
environment without requiring any modification of the QoS Agent´s code or in the
application.

The component - based internal structure of the QoS Agent allows the architecture to be
easily extended by the application programmer. This can be done by writing new
components that are plugged into the QoS Agent when needed. Predefined and user -
defined components can be stored in a library and then used when the corresponding
resource reservation protocol is in use, in case the component in question is a system
filter or agent, or when the application can be classified into the application area
corresponding to the application filter. The components can be combined freely, since
there is no interdependence between them.

The addition of support for a new resource reservation protocol requires that a new
system agent and a new system filter be written by the programmer. The system agent is
responsible for the interaction with the new reservation protocol, while the system filter
is responsible for translati ng QoS parameters between the set of QoS parameters
understood by this new protocol and the generic parameters used internally by Quartz.

Adding support for a different area of application requires only that the component
responsible for interpreting QoS p arameters meaningful in this context (i.e. the
corresponding application filter) be provided by the application programmer.

Filters are simple and easy to implement because they deal with parameters described at
the same level of abstraction, i.e., applica tion filters translate user parameters specified
at application level into generic application parameters, while system filters translate
generic system parameters into system specific ones. The most complex translation step,
which involves mapping between  different abstraction levels and balancing
requirements between components, is executed by the QoS interpreter provided by

Quartz. Since system agents are restricted to dealing with a single reservation protocol,
the knowledge necessary to implement them is limited.

4.5  Summary

This chapter has described in detail the main contribution provided by this thesis, which
is the Quartz QoS Architecture.

After listing the requirements imposed on the architecture, we have introduced the
component - based structure of t he architecture. We have established the role of each
component in the overall task of providing mechanisms for QoS specification and
enforcement in open environments transparently from the resource reservation protocols
present in the computing platform. In addition, we have specified the interfaces of the
internal components of the Quartz architecture and the messages used by these
components to interact with their peers.

We have also described the sets of generic QoS parameters that are used internally by

Quartz to represent the application -  and system - specific QoS parameters.

Furthermore, two important characteristics of Quartz have been described: its capacity
to handle resource adaptation and its potential to be reconfigured by replacing
components in  order to adapt to changes in the surrounding environment.

5

Implementation

This chapter describes a functional prototype of the Quartz architecture that has been
implemented as part of this thesis. The following sections describe the main core of the
impl ementation (i.e. the components that are not system -  or application - specific) and
later introduce the components that are plugged into the core in order to interface with
the resource reservation protocols supported by the target environment and to provide

QoS mechanisms suitable for the application areas to be supported by Quartz.

5.1  The Quartz Prototype

A functional prototype of Quartz has been implemented in order to analyse its
behaviour and validate the applicability of Quartz in the provision of QoS - con strained
services for applications with QoS requirements. The computing platform supported by
this prototype and the software model used for its implementation are described in the
following sections.

5.1.1  Supported Platforms

The platform on which Quartz was de ployed consisted of a network of PCs running the

Windows NT operating system. This platform was chosen because of the fact that it is
recognised as an industry de facto  standard, in addition to its soft real - time capabilities

[96] . The real - time capabilities provided by Windows NT, despite being still limited

[144] , are similar to those provided by other commercial operating systems such as

Sun´s Solaris. We have also taken into account for choosing the operating system that
resource reservation protocols for Windows NT, including preliminary versions, are
easy to obtain and experiment with, in most cases at no cost.

Two different network - level resource reservation protocols are supported by the
prot otype: ATM and RSVP. These protocols were described in items 2.6.2  and 2.6.3
respectively. We have opted for using ATM and RSVP due to the fact that they are the
two most widely used network - level r esource reservation protocols.

We use the implementation of RSVP developed by Intel, called PC - RSVP, currently in
beta version. For ATM, we use ForeRunner LE 155 Mbps PC cards and a Fore Systems

ASX 100 switch. We also rely on the device driver and the Win sock2 service provider
that are supplied by Fore Systems together with the hardware.

The programming environment used for the implementation was Microsoft Visual C++

5.0. It was chosen because of its close integration with the computing platform in which
t he development took place.

5.1.2  Softw are Model

In the prototype that we have implemented, the components of the Quartz architecture
and the messages exchanged between them are represented as C++ classes [46] .

Each component that m akes up part of the Quartz prototype is implemented as a C++
object. All components are linked with the application within the same address space.

As a result , t he Quartz prototype run s  only at user level  and does not require any change
to  the O.S. kernel ,  making the architecture  more portable and flexible .

Messages are exchanged between components by means of method invocations.

Consequently, each message recogni sed by a component corresponds to a public
method that can be invoked by the other components. The contents of the message are
passed as parameters to the method.

Resource reservation protocols are typically implemented as Windows NT services. The
reservat ion mechanisms provided by the operating system are integrated with the kernel.

5.2  The Quartz Core

The Quartz Core consists of the components of the prototype that are independent of the
underlying system and of the application area. These components are: t he data structure
used for specification of QoS parameters, the QoS Agent, the QoS Interpreter, and a
default filter called the bypass filter. In addition, the core provides base classes for
system agents, which are specialised as operating system agents a nd network agents.

5.2.1  Specification of QoS Parameters

The mechanisms for specification of QoS provided by Quartz are based on class

QzQoS
,
which stores parameter names and their corresponding values. This class provides
methods to set and retrieve the values of these parameters from its internal data store.

Figure 13  shows the representation of class

QzQoS
 in the Unified Modelling Language

(UML) [22] .

QzQoS
m _param : char [][]
m _value : unsigned long []
m _count : unsigned int = 0

SetParam ( )

GetParam ( )

GetCount ( )

ClearAll ( )

Figure 13  ˘  UML of Class

QzQoS

Class

                                         QzQoS
                                                                                        stores a list of parameters, which are represented by a parameter name and
the corresponding value, and a parameter counter. An unsigned long field is used for
storing the value of the parameter or the address of a  data structure where more complex
parameter values can be stored.

Methods

                                                               SetParam()
,

GetParam()
,

GetCount()
 and

ClearAll()
 are provided for
manipulating the list of parameters. These methods are used for setting a parameter,
getting the value of a param eter, get the number of parameters stored by the class, and
to clear all parameters respectively.

5.2.2  Basic Translation Components

The base class for translation components is called

QzTranslation
. This class defines
the methods that perform translation of QoS  parameters in both directions of translation.

These methods are

TranslateQoSDownwards()
, which implements the direct path of
translation, and

                                                                                                           TranslateQoSUpwards()
, which implements the reverse path.

Two translation components derived from

QzTranslation
 are included in the Quartz

Core: the bypass filter and the QoS interpreter. The UML of the translation components
is shown by Figure 14 .

The bypass filter is a default QoS filter that simply forwards QoS parameters without
modifyi ng them. By using this filter as the application filter, it is possible for the
application to specify QoS requirements in the form of generic system - level QoS
parameters.

The QoS interpreter, implemented by class

QzInterpreter
, translates between the
gene ric sets of QoS parameters defined by Quartz and balances requirements between
the network and the operating system, performing adaptation when necessary.

The execution of balancing and adaptation is delegated by the interpreter to the
balancing unit, whi ch is implemented by class

QzBalancingUnit
. This component
stores split factors that are used to divide QoS requirements between the network and
the operating system. S plit  factors have the same values for agents running on the same
machine and  reflect the current c apacity of the network and the operating system to
provide interchangeable resources . The  values of split factors are defined according to
the  global state of the system and  are  modified every time adaptation occurs .

QzBalancingUnit
m _delay_split : float
m _delay_var_split : float
m _cost_split : float
m _cost_max_split : float

Balance ( )

                                                                                                                    QzBypassFilter QzInterpreter
m _balancing_unit : QzBalancingUnit

QzTranslator

TranslateQoSDownwards ( )

TranslateQoSUpwards ( )

Rebalance ( )

                                                                                                                 Figure 14  ˘  UML of Basic Translation Components

5.2.3  Basic System Agents

Class

                                         QzSystemAgent
 defines the standard interfac e of a system agent and implements
method

                                                         QoSRequest()
 for specifying QoS and some additional methods needed for
initialisation (method

Init()
) and for close control of the notification and adaptation
process to be used by the application when necessary. T hese methods are

QoSNotify()
                                                                                                      for notifying the application of resource adaptation and

 QoSAdapt()
for initiating adaptation. In addition, agents contain pointers to the corresponding QoS
filter, to the interface used to upcall the application and to the str ucture with the current

QoS parameters. They have also a flag to identify the state of the QoS reservation (i.e.

to indicate whether the QoS parameters are currently being enforced by the associated
resource reservation protocol or not).

Class

                                           QzSystemAg ent
 is specialised by

QzNetworkAgent
 and

QzOSAgent
, which
are the base classes for network and operating system agents respectively.

The application interfaces with only one component of the architecture: the QoS Agent,
implemented by class

QzQoSAgent
, whi ch like system agents is also derived from class

QzSystemAgent
                                                                                                                       . The

QzQoSAgent
 class has a pointer to the network and operating
system agents and for the interface used for upcalling the application.

Figure 15  shows the UML repre sentation of the basic system agents, the QoS Agent and
the upcall interface.

QzUpcall

QoSReport ( )

QoSError ( )

QoSWarning ( )

QzSystemAgent
m _filter : QzTranslator *
m _upcall : QzUpcall *
m _active : bool = false
m _qos : QzQoS

Init ( )

QoSRequest ( )

QoSNotify ( )

QoSAdapt ( )

QzOSAgent

                       QzNetworkAgent

QzQoSAgent
m _netagent : QzNetworkAgent *
m _osagent : QzOSAgent *
m _translator : QzTranslator *

                                                                          Figure 15  ˘  UML of Basic System Agents and Upcall Interface

The QoS Agent is a skeleton in which the components of the Quartz  core are put
together with the components that depend on the application area and the underlying
system. These components can be plugged into and removed from the QoS Agent in
order to reflect changes in the surrounding environment. The replacement of
com ponents encapsulated by the QoS Agent does not affect the interface with the user,
which still sees the interface of the QoS Agent as the standard means of interaction with

Quartz.

The application has to support the upcalls defined by class

QzUpcall
 which are used
for reporting errors, warnings and dynamic changes of QoS parameters. These are
implemented by methods

QoSReport()
,

QoSError()
 and

QoSWarning()
respectively. Applications using Quartz must support this interface by inheritance or
encapsulation. Th e QoS Agent also inherits from

QzUpcall
 in order to receive
notifications, errors and warnings from network and operating system agents, which are
then forwarded to the application.

5.2.4  Interaction Betw een Components

The Quartz prototype is ready to be used b y an application after the application
initialises the QoS Agent and identifies itself. The QoS Agent is responsible for
initialising the other components of the architecture.

Figure 16  illustrates the interaction between the comp onents of the Quartz prototype
when QoS is requested (action [1]) and when adaptation takes place (action [2]).

First, the application calls method

QoSRequest()
 on the QoS Agent, passing its QoS
requirements in the form of a

QzQoS
 structure with applicati on - level QoS parameters.

Then, the QoS Agent calls the application filter and the interpreter, which translate and
balance the QoS parameters, and requests QoS from both the O.S. agent and from the
network agent. These agents ask their corresponding filter s to translate the QoS
parameters and, in the possession of system - specific QoS parameters understood by
them, perform resource reservations by using their corresponding reservation protocols.

With the reservations accepted by the reservation protocols, th e resources become
available for the application.

Figure 16  ˘  Interaction Between Components

QoS Agent:

QzQoSA gent

Application:

QzUpcall

App. Filter:

QzTranslator

Interpreter:

QzInterpreter

OS Filter:

OS Agent:

QzOSAgent

 Network Filter:

 QzNetworkFilter

Balancing Unit:

QzBalancingUnit

Network Agent:

  QzNetworkAgent

QoSRequest

TranslateQoSDownwards

(Reserve Resources

)QoSRequest

)Balance

(Use Resources

)(Adaptation Takes Place

)TranslateQoSUpwards

QoSReport

TranslateQoSUpwards

Rebalance

[A] QoS Request

(Reserve Additional Resources

)[B] QoSReport

(Adapt

)(Use Resources

[2][1]

At some stage in the computation, the network or the O.S. might start resource
adaptation (in the example, this is performed by the net work). The new QoS parameters
are then translated upwards by the corresponding system filter and reported to the QoS

Agent in the form of a call to the

QoSReport()
 method. The QoS Agent passes these
parameters to the interpreter, who asks the balancing age nt to try to rebalance them. If
the rebalance succeeds (option [A] in the figure) the QoS Agent tries to get additional
resources from the O.S.. If the rebalance fails (option [B]) the QoS Agent informs the
application of the new QoS by calling

QoSReport()
 on the application, which then has
to adapt its requirements.

5.3  The RSVP Sub - System

The following sections present the system agent and the system filter for the RSVP
protocol, together with the QoS parameters recognised by them.

5.3.1  RSVP Parameters

The QoS p arameters defined for RSVP use a token bucket to model the data traffic. The
parameters recognised and translated by the RSVP filter are listed in Table 9 . In
addition, three other parameters are also supported by RSVP. These para meters are very
system - specific and do not have a form of representation at the application level.

Consequently, they are not translated by the RSVP filter, but can be specified by the
user to fine - tune the behaviour of the network support. These parameter s are listed in

Table 10 .

Parameter Name  Description

RSVP::TokenRate  Rate at which tokens are produced (in bytes/s)

RSVP::BucketSize  Size of the bucket (in bytes)

RSVP::PeakRate   Maximum data rate (in bytes/s)

RSVP::MinPoliced  Minimum amount of data subject to the policy (in bytes)

RSVP::MaxPktSize  Maximum packet size (in bytes)

RSVP::Rate  Rate (in bytes/s; only for deterministic service)

RSVP::SlackTerm  Slack (in microseconds; only for deterministic service)

RSVP::FlowTyp e  Type of data flow (deterministic, best - effort, etc)

Table 9  ˘  RSVP QoS Parameters

Parameter Name  Description

RSVP::DataTTL  Time to live (in hops; local area by default)

RSVP::ReservationStyle  Style of reservation filter (fixed filter by default)

RSVP::Policy  Policy to be used by the policy control component

Table 10  ˘  Additional Parameters

The meaning of the RSVP parameters is exactly the same as defined by the RSVP
specification. Consequently, after th e QoS parameters are translated into RSVP - specific
parameters, the RSVP agent just has to arrange them in a suitable data structure and
pass this structure to the RSVP protocol in order to perform a resource reservation.

5.3.2  The RSVP Filter

The system filter f or RSVP is implemented by class

QzRSVPFilter
, which is
responsible for translating QoS parameters understood by RSVP. It inherits from class

QzTranslation
                                                                                                                        and implements the translation methods defined by this class. The
translation process occurs in two w ays, downwards from the generic set of system -
specific QoS parameters defined by Quartz into RSVP - specific QoS parameters, and
upwards from RSVP - specific parameters into generic system - level parameters.

The translation between generic system - level paramete rs and RSVP parameters implies
creating a token bucket in order to describe the traffic requirements specified by the
application. The rules described below execute the mapping between generic system -
level parameters and RSVP parameters:

·

                         RSVP::TokenRate
 is  equal to

Net::Bandwidth
.

·

                         RSVP::PeakRate
 and

RSVP::Rate
 have the same value as

                         Net::BandwidthMax
.

·

                         If

                                                Net::BandwidthMax
 is not specified, it is considered to be equal to

                         Net::Bandwidth
.

·

                         RSVP::BucketSize
 is equal to

Net::Bandwith
 or the difference between

                         Ne t::BandwidthMax
 and

Net::Bandwidth
 if higher.

·

                         The value of

RSVP::MaxPktSize
 is the same as

Net::PacketSizeMax
, and

                         RSVP::MinPoliced
 is equal to

Net::PacketSizeMin
.

·

                         RSVP::FlowType
 is derived from

Net::Guarantee
.

·

                         The value of

                                                                                                                 RSVP::SlackTerm
 is the same as

N et::DelayVariation
.

Parameters

                                                                               Net::PacketSize
,

Net::Delay
,

Net::ErrorRatio
,

Net::Cost
, and

Net::SecurityLevel
 have no equivalent at the RSVP level. In order to allow the
reverse translation from parameters at RSVP level into parameters at application leve l,
these parameters are forwarded to the RSVP agent, which stores them and passes them
upwards when a reverse translation occurs.

5.3.3  The RSVP Agent

The system agent for RSVP has been implemented as a class called

QzRSVPAgent
.

Upon initialisation, details ab out the link that is subject to QoS  have to be specified by
the application (or by middleware working on behalf of it) by calling the

Init()
method of the QoS Agent before requesting the provision of QoS - constrained service.

Information such as the commun ication protocol (TCP or UDP), the host name or its IP
address, the port, and the communication role (i.e. sender, receiver or both) is passed to
the RSVP agent by using the

Init()
 method. In addition, a pointer to the upcall
interface that is to be called  in order to report QoS adaptation, errors or warnings has to
be passed to the RSVP agent upon initialisation.

After initialisation, the RSVP agent performs resource reservations upon the receipt of a

QoSRequest
                                                                                             message (i.e. whenever method

QoSRequest()
 i s called) by interacting
with the interface that it shares with the RSVP protocol. In addition, the RSVP agent
issues

                                              QoSReport
 messages when adaptation occurs at lower - level (i.e. calls method

QoSReport()
                                                                                                      on the upcall interface).

5.4  The ATM  Sub - System

A sys tem agent and a system filter for ATM have also been implemented in order to
allow Quartz to perform reservations in ATM networks.

5.4.1  ATM Parameters

The parameters defined for the ATM sub - system are listed in Table 11 . These
paramet ers correspond to the fields of the data structure used for performing resource
reservations using Fore Systems´ ATM Service Provider for Winsock2. Consequently,
the ATM Agent has just to collect this information, fill in a data structure and call the
appr opriate routine provided by Winsock2 in order to perform a reservation.

Parameter Name  Description

ATM::PeakCellRate  Max. rate in which cells are produced (in cells/s)

ATM::SustainableCellRate  Long - term cell rate (in cells/s)

ATM::QoSClass   Type of data  flow (CBR, VBR, best - effort, etc)

ATM::MaxBurstSize  Maximum cell burst (in ms)

ATM::Tagging  Tag non - compliant cells as subject to be discarded

Table 11  ˘  ATM QoS Parameters

It is important to notice that these parameters differ significantly from those used for the

RSVP protocol, but are similar to the generic system - level QoS parameters defined by

Quartz. This happens because RSVP uses a token bucket model for QoS specification,
while both Quartz and ATM adopt bandwidth - oriented  QoS parameters.

5.4.2  The ATM Filter

The ATM filter is implemented by class

QzATMFilter
, which translates ATM
parameters understood by the ATM Agent. Like other filters, the ATM Filter inherits
from class

                                                                             QzTranslation
. The translation process occurs in two way s, downwards
from the generic set of generic system - level QoS parameters defined by Quartz into

ATM - specific QoS parameters, and upwards from ATM - specific parameters into
generic system - level parameters.

The translation from generic system - level QoS parame ters into ATM - specific QoS
parameters is mainly concerned with bandwidth. Whenever the provision of QoS -
constrained services is requested, the reservation of the necessary bandwidth is
performed. The value of

ATM::PeakCellRate
 is taken from

Net::BandwidthM ax
,
while the value of

ATM::SustainableCellRate
 corresponds to

Net::Bandwidth
.

The QoS class is defined based on the characteristics of the bandwidth, i.e. if it is
constant or variable.

ATM::MaxBurstSize
 and

ATM::Tagging
 are specified directly
by the appl ication when it finds it necessary. The additional network parameters that
have no equivalent at ATM level (i.e. cost, packet size, etc.) are forwarded to the ATM
agent, which stores them and sends them back upwards when needed in order to
perform the reve rse translation.

5.4.3  The ATM Agent

The system agent for ATM is implemented by class

QzATMAgent
, which specialises
class

                                     QzNetworkAgent
. During the initialisation of the agent, the identity of the socket
through which the QoS - constrained data will flow has to be specified.

The ATM Agent gets the ATM QoS parameters from the translation unit and performs
reservation of bandwidth by interacting with the ATM service provider for Winsock2.

In addition, it reports any change in QoS occurring in the network to the ap plication by
translating QoS parameters upwards and then issuing upcalls through the

QzUpcall
interface provided by the application.

5.5  The Window s NT Sub - System

At the operating system level we have adopted Windows NT as the platform for the
deployment of th is prototype of Quartz. As a result, a system agent and a filter have
been developed for this operating system.

The provision of QoS in Windows NT is limited. We make use of the real - time priority
class and of mechanisms for memory locking to provide a mo re predictable service,
which is still non - deterministic. By using these mechanisms, we can guarantee unloaded
behaviour to applications (i.e. shield the application from overload conditions) making
use of the reservation mechanisms provided by operating s ystem.

5.5.1  Window s NT Parameters

Only two QoS parameters are defined for Windows NT. They are:

·

                         WinNT::PriorityLevel

·

                         WinNT::MemoryPaging

WinNT::PriorityLevel
 defines the priority level at which the process executes. This
is used by the operating system to sched ule access to the processor. Processes in

Windows NT are divided into two priority classes. These classes are the

NORMAL_PRIORITY_CLASS
, which is subject to the usual time - sharing policy
implemented by Windows, and the

REALTIME_PRIORITY_CLASS
, which has
pr ecedence over the normal class and over system services. The NT scheduler handles
threads directly, taking into account not only the priority class but also the thread
priority, which is left for the user to assign.

WinNT::MemoryPaging
 determines if the me mory allocated by the process will be
subject to paging operations, which introduce unpredictable delays and may degrade
performance. Values allowed are true (i.e. 1) or false (0).

5.5.2  The Window s NT Filter

QzWinNTFilter
                                                                                                                        translates QoS parameters understood to  Windows NT. It inherits
from class

                                                                              QzTranslation
 and implements the translation methods defined by this
class. The translation process occurs in two ways, downwards from the generic set of
system - level QoS parameters defined by Quartz into NT - specific QoS  parameters, and
upwards from NT - specific parameters into generic system - level parameters.

Translation between generic system - level parameters and Windows NT parameters is
quite simple, since only the parameter

OS::Guarantee
 is taken into account. If best -
effort service guarantee is requested, the value of

WinNT::PriorityClass
 is set to

NORMAL_PRIORITY_CLASS
 and

WinNT::MemoryPaging
 to true. If unloaded service
guarantee is requested,

WinNT::PriorityClass
 is set to

REALTIME_PRIORITY_CLASS
 and

WinNT::MemoryPa ging
 to false. Deterministic
behaviour is not supported by Windows NT, and unloaded behaviour is assumed if
deterministic service is specified.

Parameters

                                                                                OS::Delay
 and

OS::Cost
 have no equivalent at Windows NT level. In
order to allow the reverse transla tion, these parameters are forwarded to the Windows

NT agent, which stores them and sends them back upwards when needed.

5.5.3  The Window s NT Agent

The system agent for Windows NT has been implemented in C++ as a class called

QzWinNTAgent
                                                                                                              .

                                                                                                                        QzWinNTAgent
 inherits  from class

QzOSAgent
, which is a subclass
of

                  QzSystemAgent
.

During initialisation of the QoS Agent, the process and the thread for which operating
system resources will be allocated has to be identified by specifying the corresponding
process and thread i dentifiers through the initialisation (

Init()
) method. By default,
these values are assumed as being the current process and its main thread.

Whenever it receives a request for enforcing QoS, the Windows NT agent sets the
priority class of the application and the locking state of memory pages according to the
value of the QoS parameters obtained after the translation process.

5.6  Component Testing

Before testing the whole prototype of the architecture, which will be done by using
application examples and will be described in section 7.1 , the translation components
have been tested individually.

The translation components have been tested with the assistance of an application that
allows us to select application and system filters, and then perform the translation of
parameters listed in a file. The translation can be performed in both directions (i.e.

downwards or upwards). Filters and the direction of the translation are defined based on
arguments passed to the application when it is called from the command line. The
output of the application shows the transformation suffered by the QoS parameters
contained in the input file during the three translation steps performed by the translation
unit.  Several test cases have been studied w ith the help of this application, and we have
observed that the mapping between parameters at different levels is correctly executed
by the translation components.

Table 12  shows an example of A/V streams parameters being transla ted into ATM and

Windows NT parameters (Note: A/V streams parameters will be described in section

6.4.2 ; for the moment, it is enough to know that they represent the horizontal and
vertical resolution of a video screen, the num ber of bits used to represent the colour of
each pixel, and the number of video frames generated per second).

Tests  have shown that the translation unit is able not only to translate the  parameters
listed in Table 12  downwards, but  it can also translate them upwa rds without any loss of
information.

                             Parameter Set  Parameter Values

           Application - Specific

                          QoS Parameters

             (A/V Streams App.)

A/V::VideoResolutionHorz = 354 pixels/line

A/V::VideoResol utionVert = 240 pixels/column

A/V::VideoColourDepth = 24 bits/pixel

A/V::VideoFrameRate  = 30 frames/sec

         Generic Application -

     Level QoS Parameters

App::DataUnitSize = 253440 bytes/unit

App::DataUnitRate = 30 units/sec

App::Guarantee = Unloaded

      Generic Syst em - Level

                          QoS Parameters

Net::Bandwidth = 7603200 bytes/sec

Net::PacketSize = 253440 bytes

Sys::Guarantee = Unloaded

                         System - Specific

                          QoS Parameters

(ATM & Windows NT)

ATM::PeakCellRate = 5280 cells

ATM::SustainableCellRate = 5280 cells

ATM::QoSClass = CBR

WinNT::ProrityLevel = REALTIME_PRIORITY_CLASS

WinNT::MemoryPaging = TRUE

                                                                                                      Table 12  ˘  Example of Translation of QoS Parameters

                             Parameter Set  Parameter Values

         Generic Application -

     Level QoS Parameters

App::EndToEndDelay = 500 msec

App ::EndToEndDelayMin = 450 msec

App::EndToEndDelayMax = 550 msec

App::Cost = 6 pence/sec

App::CostMax = 9 pence/sec

      Generic System - Level

                          QoS Parameters

Net::Delay = 300 msec

Net::DelayMin = 270 msec

Net::DelayMax = 330 msec

OS::Delay = 200 msec

OS::DelayMin  = 180 msec

OS::DelayMax = 220 msec

Net::Cost = 4 pence/sec

Net::CostMax = 6 pence/sec

OS::Cost = 2 pence/sec

OS::CostMax = 3 pence/sec

                                                                                                            Table 1 3  ˘  Example of Balancing of QoS Parameters

                                                              State  Parameter Values  Notes

    Normal Working State

Net::Delay = 300 msec

OS::Delay = 200 msec

Total Delay = 500 msec

Split Factor = 0.6

                             After Resource

                                           Adaptation

Net::Delay = 400 msec

OS::Delay = 200 msec

Total Delay = 600 msec

Split Factor = 0.6

      After QoS Adaptation

                          at System - Level

Net::Delay = 4 00 msec

OS::Delay = 100 msec

Total Delay = 500 msec

Split Factor = 0.8

                                                                                                        Table 14  ˘  Example of Adaptation of QoS Parameters

The test cases also include simulations of QoS balancing and of QoS adaptation. In the
first case, which is i llustrated by Table 1 3 , parameters delay and cost are balanced
between the network and the O.S. supposing  a split factor of 0.6 for delay (i.e. 60% of
the delay is caused by the network and 40% by the O.S.) and of 0.66 for cost. In a
s econd moment, illustrated by Table 14 , we simulate the occurrence of resource
adaptation, making the network increase its delay from 300 to 400 milliseconds. The
translation unit then performs a rebalancing process, increasing the  split factor to 0.8
and causing the O.S. delay to decrease to 100 milliseconds. If this new delay is accepted
by the O.S., the original total delay of 500 milliseconds is restored and the process of
resource adaptation is contained at system level without  involving the application;

otherwise, the application is asked by Quartz to accept a higher delay.

In order to complete the evaluation of the behaviour of individual components, we have
also tested the correctness of each one of the system agents. The sy stem agents have
been tested individually by feeding them with sets of QoS parameters understood at this
level (i.e. without interference from the translation unit). The agents have shown to be
able to interpret these parameters and perform the correspondi ng resource reservations
by using the associated reservation protocol.

Adaptation has also been tested by simulating the receipt of notification messages from
the resource reservation protocol. These messages are issued by the reservation protocol
at run - time in order to indicate that the allocation of resources has changed. The system
agents have been shown to recognise these messages and have performed the
appropriate upcalls in order to trigger adaptation at the higher layers.

5.7  Summary

This chapter has p resented a prototype implementation of the Quartz QoS architecture.

This prototype provides support for Windows NT, RSVP and ATM, and can be easily
extended in order to support other network infrastructures and operating systems.

The prototype presented in  this chapter was used as the basis for a framework for the
development of multimedia applications and for a series of evaluation tests, which are
described in the next two chapters.

6

The Quartz/CORBA

Framework

In order to provide a complete support for m ultimedia applications, we have integrated

Quartz into a framework based on the CORBA architecture. The Quartz/CORBA
framework allows continuous media, which has intrinsic QoS requirements, to be
transmitted between applications running in open systems. In  this framework, the

CORBA architecture provides mechanisms for the exchange of control and
synchronisation messages, as well as for audio and video streaming. Quartz is
responsible for enforcing the QoS requirements imposed by the application on the
trans mission of audio and video streaming data.

A more detailed description of the Quartz/CORBA framework is presented in the next
section. Further sections describe application scenarios in which the framework is used
for transferring media streams with QoS co nstraints; the implementation of the

Quartz/CORBA framework; and also the development of an application for music
rehearsal over the Internet built on top of the framework. An analysis of the
characteristics of the framework and a comparison with similar p rogramming supports
for multimedia conclude this chapter.

6.1  M otivation

The use of multimedia applications for transmission of audio and video over the Internet
has become a reality due to the accessible prices of multimedia hardware (such as audio
cards and  video cameras) and the increasing speed of network connections. Users of this
sort of application, however, still face quality limitations in both sound and image, since
the infrastructure on top of which the application is built (i.e., the Internet and d esktop
operating systems) provides only best - effort services. These limitations have
constrained the effective use of these multimedia applications in areas such as business
and telecommunications, where quality must be ensured in order to enable the servi ce
provider to charge for the service. Multimedia applications, in addition, suffer from
limited compatibility with heterogeneous software and hardware platforms.

Two distinct categories of data are handled by distributed multimedia applications. First
we have the control data, which can tolerate some delay but has to be reliable. This
behaviour can be provided by using best - effort logical networks such as TCP/IP
directly, or by adopting middleware for distributed computing such as CORBA. On the
other hand,  continuous media are subject to QoS requirements, which are not possible to
enforce by using middleware built on top of a best - effort networking infrastructure. The
provision of QoS - constrained services for multimedia applications requires the use of

QoS - aware middleware that use the QoS mechanisms present in the underlying system
in order to enforce the QoS requirements of the application.

Figure 17  shows a generic multimedia application with control and media data. T he
remote communication in an application like this may use the available network
protocols directly, or may adopt a middleware platform that allows transparency
regarding issues like remote communication and physical location of the partners.

Multimedia Application

Control Data Media Data

Middleware

TCP

IP

Best-Effort Network

Middleware

RTP, etc.

IP with R

SVP
, etc.

QoS-aware Network

                              Figure 17  ˘  Available  Technology for Distributed Multimedia Applications

Since we do not want multimedia applications to have to interact directly with lower -
level network protocols, extending current middleware is re quired in order to allow
distributed multimedia applications to impose QoS constraints on the transmission and
processing of audio and video data.

Another aspect that has to be taken into account by multimedia applications is media
synchronisation [35] . The synchronisation mechanisms necessary in a multimedia
system can be implemented at application level by using:

·

                         information carried in - band together with the encoded media (i.e. timestamps) that

                         allows the reconstruction of th e media sequence by the receiver (intra - stream

                         synchronisation); and

·

                         events issued in order to define synchronisation points between distinct video

                         streams (inter - stream synchronisation and event synchronisation).

The application code is responsible for ha ndling this information and rendering the
media according to the corresponding synchronisation requirements. The
synchronisation cannot be executed at support level because the differences between the
processing and rendering times of different media at ap plication level have to be taken
into account.

6.2  Description of the Quartz/CORBA Framew ork

The CORBA architecture has been extended by the OMG in order to make it more
suitable for application areas such as multimedia.

The CORBA streaming mechanism, which was described in section 2.4.3 , adds
mechanisms for the transmission of continuous media and for the specification of QoS
requirements to the CORBA architecture, making it suitable for handling both control
and media data.

The  notification service [11]  is an extension to the CORBA event service that allows
objects to issue events with delivery constraints associated to them. It can be used by
multimedia applications to issue events in order to defin e synchronisation points, which
are then caught by the destination of the media to reconstruct the timing relation present
at the source of the media.

However, despite having been extended in order to provide new communication
mechanisms that make it suit able for multimedia applications, CORBA does not specify
how QoS is enforced at lower level by these new communication mechanisms. Aiming
to overcome this limitation, we have integrated Quartz into the CORBA environment in
order to provide a framework for the development of multimedia applications with QoS
requirements.

The Quartz/CORBA framework is composed by the objects defined by the CORBA

A/V Streams mechanism ˘  virtual devices, stream control objects, stream and flow
endpoints ˘  put together with the QoS Agent, the ORB and the CORBA notification
service.

Virtual device objects abstract multimedia devices (i.e. cameras, speakers, etc) used by
multimedia applications. A stream control object allows the user to control the media
flow (i.e., start and stop  it) as well as add and remove parties from a multi - party
connection. Stream endpoints transfer stream data through the network, getting data
from and delivering data to virtual devices. Each endpoint has one or more media flows,
which are abstracted as fl ow endpoint objects (subdivided into flow producers and
consumers) located at each end of the flow.

Flow endpoints also issue synchronisation events through the notification service. The
notification service is employed in the context of the Quartz/CORBA framework as the
basis of a mechanism for imposing inter - stream synchronisation constraints. In this
context, events issued by flow producers in order to define synchronisation points are
caught by flow consumers to perform media synchronisation.

The data delivery is subject to QoS requirements, which are agreed on by the devices
during a negotiation process and then requested during the creation of the stream, i.e.

during the binding of two or more virtual devices. After the binding takes place, the

QoS pa rameters associated with a stream (such as video resolution, number of audio
channels, etc.) can be modified through the stream control object.

In the framework, the process of QoS translation and enforcement of QoS is delegated
to the QoS Agent. This make s the middleware more portable and simplifies
significantly the way in which the media streaming mechanisms are built due to the
separation between QoS enforcement and media transfer.

Flow

Stream

Control

Stream

Endpoint

Flow

Producer

                                                                Virtual

                                                                Device

Stream

Endpoint

Flow

Consumer

Virtual

Device

Object Request Broker

QoS

Agent

QoS

Agent

Notification

Service

sync.

events

                                                                       Figure 18  ˘  The Qu artz/ CORBA  Media Streaming Framework

Figure 18  shows an application scenario in which a video streaming application is built
using the Quartz/ CORBA  framework. The application specifies the characteristics of
the media stream, i.e.  the number of flows of audio and video and their expected
quality, which are obtained either from a user profile or through interaction with the
user. The CORBA  streaming mechanism handles the transmission of media between
partners, and also controls the flow of media and the membership of the conference. The

QoS Agent is informed of the QoS requirements associated to the media flows and
handles them accordingly.

The Quartz/CORBA framework simplifies the development of multimedia applications
by offering  a common middleware for the exchange of control and media data
transparently through the network. The application programmer does not have to deal
with details related to the kind of network protocol being used, the location of sources
and destinations of  data, or even the QoS requirements at network level. Instead, the
programmer uses high - level abstractions that hide the complexity incurred from
distribution and resource reservation, although having the possibility of interacting with
the lower - level com ponents if it becomes necessary.

The framework allows the programmer to construct a multimedia application by using
built - in classes of virtual devices and configuring them as necessary to provide the
desired output quality (i.e., the QoS required by the application). Virtual devices have to
be implemented according to the target platform based on the general structure provided
by the A/V streams mechanism.

The platform - independent nature of the Quartz architecture makes the framework able
to provide QoS to a wide range of applications running over several different
reservation protocols. The framework also provides means to specify and enforce the
synchronisation constraints that are necessary in some media presentations by using the

CORBA notification se rvice.

6.3  Application Scenarios

In the following sections we describe several application scenarios in the area of
distributed multimedia, showing how the Quartz/CORBA framework could be
employed as the basis for building multimedia applications.

6.3.1  Media Broad cast

One common application scenario in the area of distributed multimedia is the broadcast
of audio and/or video. Figu re 19  illustrates the use of the Quartz/CORBA framework to
implement a broadcast application. In thi s scenario, a media source broadcasts a video
signal through the network, to one (or more) receivers (i.e. media sinks).

In the video broadcast application scenario, the media flow is built by using the
abstractions provided by the CORBA A/V streams mechan ism. The virtual device, the
stream endpoint and the flow endpoint are present at both ends, while the control, made
through the stream control object, is located at the media source. Provision of QoS is
delegated to the QoS Agent, which is attached to bot h flow endpoints (i.e. the flow
producer and the flow consumer).

In a broadcast session, the quality of the broadcast is derived primarily from the media
source. The source defines the maximum quality of audio or video that will be possible
through the tra nsmission, and the quality of the presentation at the receiver will be
specified within the limits imposed by the media source.

In a similar way, the flow of media is controlled by the source. The destination cannot
influence the flow of media (e.g. stop or pause the broadcast signal).

In order to be added to the stream and receive the broadcast signal, the user has to get a
reference to the stream control object in the source and use this reference to call a bind
operation.

Media Source   Media Sink

Flow

Stream

Control

Stream

                                                                                                                    Endpoint

Flow

                                                                                                                   Producer

                                               Virtual

                                               Device

Stream

Endpoint

Flow

Consumer

Virtual

Device

Object    Request    Broker

QoS

Agent

QoS

Agent

Figu re 19  ˘  Video Broadcast

An analogy between this situation and a TV or radio broadcast is applicable. In both
cases the quality of the broadcast signal depends only on the source, but the quality of
the rendered audio or video can b e degraded according to the characteristics of the
receiver equipment. In addition, the signal is continuously broadcast, independently of
factors such as the number or receivers connected to it.

6.3.2  On - Demand Media

Another application scenario involving medi a transfer is the transmission of media on -
demand. In this case the receiver specifies its will to receive a specific audio or video
signal from the source.

The media sink should be able to control the QoS of the transmission, directly
influencing the med ia source. The requested QoS may influence the billing of the
service provided by the media source, in case of a private service subject to copyright.

The media sink is also able to control the flow of data (e.g. stop or pause the flow) in
the same way it does with locally stored media such as a videotape or an audio CD.

In this category of application, the media sink creates a stream between the input and
output devices. The corresponding stream control object, located at the sink, is used to
specify the r equired QoS for the transmission and to control the flow of data.

Media Source   Media Sink

Flow

Stream

Control

Stream

Endpoint

Flow

Producer

                                                        Virtual

                                                        Device

Stream

Endpoint

Flow

Consumer

Virtual

Device

Object    Request    Broker

QoS

Agent

QoS

Agent

Figure 20  ˘  On - Demand Video

Figure 20  shows the transmission of video on - demand from a media source (a  video
server). This scenario distinguishes itself from the previous one due to the location of
the stream control object, which is now located at the media sink.

6.3.3  Videoconference

The names `media flow´ and `media sink´ are relative. A component of a multi media
application can be source and sink at the same time, when more than one flow is being
transferred through the network.

The most common example of this category of application is the videoconference. In
this scenario, each partner has the components n ecessary to send and receive media

(usually audio and video). Each user locally controls the quality of the signal being
transmitted, and can also degrade the received signal during the rendering process.

One particular case of videoconference is one in wh ich only two partners are involved,
often called digital video telephony. Figure 21  shows a video telephony system
designed according to the Quartz/CORBA framework proposed by us. In this scenario,
each partner has an i nput and an output flow, which are represented by a flow producer
and a flow consumer respectively. As shown in the figure, the input and output flows
can be modelled as a single stream composed by two flows, one in each direction, and a
single virtual dev ice can represent the whole video phone. Alternatively, the media flow
could be represented as two streams each composed by a unidirectional flow, and the
input and output devices could be represented separately.

Flow 1

Flow 2

Calling Partner     Called Partner

Stream

Control

Stream

Endpoint

                                                                                               Flow

                                                                                   Producer

                                                     Virtual

                                                      Device

Stream

Endpoint

Virtual

Device

                                                                                                QoS

                                                                                           Agent

Flow

Consumer

QoS

Agent

Flow

Producer

QoS

Agent

Flow

Consumer

QoS

Agent

Object    Request    Broker

Figure 21  ˘  Video Telephony

The control over the stream (represented by the stream control object) is held by the
calling partner. This is justifiable if we make an analogy of this scenario with a
telephone call. In a telephone call, the caller usu ally controls the connection and
disconnection. This happens mainly because he is the one who is paying for the call.

In the particular case of the video telephony application, the caller also controls and is
charged according to the QoS requirements asso ciated to the call. The privacy of the
called partner is preserved because he has total control over his local devices, and can
choose not to answer the call or to redirect it to a media recording device that behaves
like an answering machine (or voice/vid eo mail).

In this application scenario, QoS is provided by the QoS Agents attached to each of the
flow endpoint objects. Since two flow endpoints are present at each side of the call, one
for input and another for output, two QoS Agents are needed in orde r to establish the

QoS on both the input and the output flows.

This scenario can easily evolve in order to become a multi - party conference by adding
new partners to the scenario and connecting them to the flows. In this case, flow
endpoints with support f or multipoint communication should be employed.

6.3.4  Media Session w ith Synchronisation

In a complex application, in which multiple flows of media related to each other are
being received by one particular destination, synchronisation between the media during
t he exhibition may be necessary. In this situation, output devices have to rebuild the
synchronisation patterns originally present when the media was produced.

One common scenario in which synchronisation of media is necessary is the
composition of multime dia documents with media received from different sources

[140] . Figure 22  shows a scenario in which a movie is retrieved from a server. The
image and the soundtrack are stored separately to allow the receiver to select between
different languages, but without the necessity of duplicating the video. However,
encoding video and audio separately obligates the receiver to execute the
synchronisation between the audio and the video signals receive d from different sources
possibly with different generation and transmission rates.

In this scenario, each of the sources has a flow producer, while the sink has a flow
consumer for each media. As occurred in the examples of on - demand video, the media
sink  controls the exhibition of the content of the multimedia document through the
stream control object. This object interacts with the stream endpoints in order to control
the flow of media data through the stream.

In order to enable synchronisation, the me dia sources issue synchronisation events that
are caught by the media sink in order to rebuild the original synchronisation pattern.

These events are produced by the flow producers, transmitted by the notification
service, and caught by the flow consumers.

Audio

Flow

                 Video

                    Flow

           Video Source

    Media Sink

Stream

Control

                                                                                                         Stream

                                                                                                  Endpoint

                                                                      Flow

                                                          Producer

                             Virtual

                             Device

Stream

Endpoint

Virtual

Device

                                                                        QoS

                                                                   Agent

Flow

Consumer

QoS

Agent

Flow

Consumer

QoS

Agent

                                                                                                                        Object Request Broker

   Audio Source

Stream

Endpoint

Flow

Producer

Virtual

Device

QoS

Agent

Notification    Service

Sync.

events

                                                                                               Figure 22  ˘  Multimedia Document with Synchronisation

6.4  Implementation of the Quartz/CORBA Framew ork

The Quartz/CORBA framework has been implemented by integrating an existing
implementation of the A/V s treaming mechanism with the prototype of Quartz
described in Chapter 5 . In order to simplify the implementation, we have not included
support for synchronisation in this prototype and in the application example that will be
pre sented in section 6.5 .

6.4.1  Implementation of the CORBA A/V Streams Mechanism

The CORBA A/V Streams mechanism adds to CORBA the ability to transfer
continuous media between distributed objects. The specification of the CORBA A/V
str eams mechanism was described in detail in section 2.4.3 .

We have an in - house implementation of the A/V streams mechanism that supports the
light profile of the standard defined by the OMG. This implementation was developed
by D avid O´Flanagan and described in his M.Sc. dissertation [111] . The support was
written in C++ using Iona´s Orbix 2.3 [73] . The implementation was carried out on top
of Windows NT 4.0 using Microsoft ´s Visual Development Studio 5.0. The
implementations of the TCP/IP and UDP/IP protocols (including UDP multicast)
provided by WinSock 2.0 [137]  were used for the transmission of continuous media
data.

Figure 23  shows the UML of the light profile of the CORBA A/V Streams mechanism.

This figure illustrates each of the interfaces described in IDL by the A/V streams
specification.

                                                                           MMDevi ce

                                                                        create _A()

                                                                        create _B( )

                                                                        bind( )

                                                                        bind _mcast( )

                                                                                        VDev

                                                          set _peer()

                                                          set _format( )

                                                          set _dev_params( )

                                                          configure( )

Basic_StreamCtrl
start( )
stop( )
destroy( )
opname( )

StreamCtrl
bind( )
bind _devs( )

StreamEndPoint
connect( )
request _connection( )
start( )
stop( )
destroy( )
modify _QoS( )

StreamEndpoint_A
multiconnect( )

StreamEndpoint_B
multiconnect( )

                                                                                        Figure 23  ˘  UML of the  CORBA A/V Streams Mechanism

The

                                MMDevice
                                                                                                          is the interface supported by the object responsible for initialising the
multimedia application, creating the media partners (the `A´ partner, which initialises
the connection, and the `B´ partner) and binding the m. The

VDev
 is the interface of the
virtual multimedia device, which is extended according to the particular characteristics
of the device. It provides mechanisms for configuration of the device and for setting the
media format. The stream control object s upports the interface

StreamCtrl
, which
inherits from

                                                                                               Basic
_

StreamCtrl
. It provides operations for controlling the flow of
data through the stream and additional binding operations. The stream endpoint is
responsible for providing operations for connecting  the flows, for controlling the flow
of data through the stream, and for setting QoS parameters. The stream endpoint is
specialised into interfaces for the `A´ and `B´ partners for providing operations that
allow the creation of multipoint connections.

A s tream is composed by one or more media flows. The light profile of the CORBA

A/V streams specification does not standardise how the individual flows are
implemented (this is covered by the full profile, though). In this implementation of the
standard, the structure described by the UML diagram shown in Figure 24  has been
adopted for implementing individual flows. According to this structure, the flow
endpoint interface provides operations for controlling the flow of data through th e
individual stream, for setting a routine that will interact with the virtual device (i.e. to
feed or to be fed with data), and for transferring data through the network channel.

FlowEndPoint

Start ( )

Stop ( )

SetStartRoutine ( )

TransferData ( )

QoSAgent

CFlowProducer

ConnectToPeer ( )

IOSender

CFlowConsumer

GoToListen ( )

ReserveQoS ( )

IOReceiver

Figure 24  ˘  UML of the  Flow EndPoint

The flow endpoint is specialised as flow consumers and flow producers, which have
operations specific to their corresponding communication roles and are associated to an

I/O object that provides the actual communication channel (i.e. an

IOS ender
 for the
flow producer and an

IOReceiver
 for the consumer). In particular, the I/O objects
provided by this implementation use TCP/IP for point - to - point communication and

UDP/IP multicast for point - to - multipoint channels.

The figure also shows that e ach flow endpoint is associated to a QoS Agent, which
during this phase of the implementation of the A/V streams mechanism corresponded to
a `dummý object. The next item explains how this object was replaced with the Quartz

QoS Agent, leading to the integ ration of the A/V streams implementation with the

Quartz architecture.

6.4.2  Integration of A/V Streams and Quartz

The implementation of the CORBA A/V streams mechanism described in the previous
item was adapted in order to use Quartz for provision of QoS. This is done through the
flow endpoint, which interacts with Quartz in order to specify the QoS requirements
imposed by the application. By separating the support for QoS from the communication
support (i.e., from the implementation of the A/V streams mechanism ) we have made
the middleware more portable and easier to implement, test and maintain.

The interaction between flow endpoints and Quartz comprises the following tasks:

·

                         initialisation of Quartz, when are identified the communication port and the process

                         th at will avail of services on which QoS requirements will be imposed;

·

                         request for enforcement of QoS requirements, which is done by calling the

                         QoSRequest()
 method of the QoS Agent during the establishment of a connection

                         between flow endpoints; and

·

                         receipt  of upcalls from the QoS Agent, which are issued in order to report QoS

                         adaptation, errors or warnings.

By performing these tasks, flow endpoints make the use of Quartz completely
transparent for the application, which only have to specify their QoS requir ements
through the QoS specification mechanisms that are provided by CORBA A/V streams.

QzAVStreamsFilter

Import ( )

Export ( )

QzTranslator

TranslateQoSDownwards ( )

TranslateQoSUpwards ( )

Figure 25  ˘  UML of the A/V Streams Filter

Since the CORBA A/V streams specification defines its own mechanisms for
specification of QoS, a filter had to be written in order to recognise the parameters
defined by A/V streams. The Quartz A/V streams filter is implemented by class

QzAVStreamsFilter
, which is shown in Figure 25 . This filter has ad ditional methods
to import and export from the format used by Quartz to store QoS parameters (i.e. the

QzQoS
                                               structure) to the format used by the A/V streams mechanism (i.e. the

AVStreams::QoS
class

)
.

The A/V streams filter imports parameters and values fr om the

AVStreams::QoS
 class
defined by the A/V streams specification and translates them into generic application

QoS parameters. Reverse translation is also executed by the filter in case of QoS
adaptation. The A/V streams QoS parameters are listed by Table 15 .

The mapping from A/V streams parameters into generic application - level QoS
parameters is shown by Table 16 . Parameters

A/V::AudioQuantisation
 and

A/V::VideoColourModel
, which define the encoding f ormat used by the application,
have no influence on the values of QoS parameters at lower abstraction levels.

Parameter Name  Description

A/V::AudioSampleSize  Size of audio sample (in bytes)

A/V::AudioSampleRate  Number of audio samples (in samples/second )

A/V::AudioNumChannels  Number of audio channels

A/V::AudioQuantisation  Quantisation (linear, u - law, A - law, GSM, etc.)

A/V::VideoFrameRate  Number of video frames (in frames/second)

A/V::VideoColourDepth  Number of bits representing colour for each pixel

A/V::VideoColourModel  Colour encoding (RGB, CMY, HSV, YIQ, etc.)

A/V::VideoResolutionHorz  Horizontal resolution of the image (in pixels)

A/V::VideoResolutionVert  Vertical resolution of the image (in pixels)

Table 15  ˘  A/V Strea ms QoS Parameters

                                          CORBA Audio

                        Streams Parameters

CORBA Video

Streams Parameters

Generic Application -

Level Parameters

A/V:: AudioSampleSize

*

A/V::AudioNumChannels

A/V::VideoColourDepth *

A/V::VideoResolutionHorz

*

A/V:: VideoResolutionVert

App::DataUnitS ize

A/V::AudioSampleRate  A/V::VideoFrameRate

App::DataUnitRate

             Table 16  ˘  Mapping between A/V Streams Parameters and Generic Parameters

The A/V streams QoS parameters, after being translated by the A/V streams filter, are
further translated by the Quartz translation unit and handed to the system agents
corresponding to the reservation mechanisms present in the system. At this point, the

RSVP protocol is used by the corresponding system agent in order to enforce QoS.

6.5  Application: T he Distributed M usic Rehearsal Studio

An application for music rehearsal over the network was written by John Segrave - Daly
for his final year project [133] . The distributed music rehearsal studio allows musicians
to play togeth er by using instruments connected to networked computers. This
application has strong QoS requirements, since users expect that factors such as network
or computing delays or lack of network bandwidth do not interfere with their musical
performance.

The hu man ear is able to notice differences of more than about 30 milliseconds in the
synchronisation of audio events. A difference higher than this amount between two
audio sources is enough to allow a listener to notice that the music is out - of - sync. As a
resu lt, the distributed music rehearsal studio must keep the delay between the
production and reproduction of audio signals within 30ms, otherwise the rehearsal
session will lose integrity [133] . Consequently, packets with a lifeti me exceeding this
limit should be discarded. This phenomenon sets the application apart from traditional
audio streaming and audio conference tools, which can tolerate much higher delays.

Figure 26  shows a usage scenario of the d istributed music rehearsal studio, in which
three musicians participate in a rehearsal. Each user has an audio source object,
responsible for broadcasting the audio produced by the instrument being played by him,
and audio sinks for each musician participa ting in the rehearsal.

                                                                                                       Send to Mixer

                                                                                                   AudioSource

                                                                                                             (Guitar)

                                                                                                        AudioSink

                                                                                                            (Drums)

                                                                                                        AudioSink

                                                                                                   (Bass Guitar)

                                                                                                        AudioSink

                                                                                                             (Guitar)

                                                                                      Machine A

Send to Mixer

AudioSource

(Drums)

AudioSink

(Bass Guitar)

AudioSink

(Guitar)

AudioSink

(Drums)

Machine B

AudioSource

(Bass Guitar)

AudioSink

(Drums)

AudioSink

(Guitar)

AudioSink

(Bass Guitar)

Send to Mixer

Machine C

Guitar

Multicast

Address

Drums

Multicast

Address

Bass Guitar

Multicast

Address

                                               Figure 26  ˘  Usage Scenario of the Distributed Music Rehearsal Studio

Audio sinks are connected to a mixer object, which is similar to a mixing desk. The
mixer object mixes the aud io sent by each musician and reproduces the resulting audio,
which is reproduced by the local machine and heard by the musician. This audio signal
gives feedback to the musician, who must play his instrument in accordance with what
the other musicians are playing.

The distributed rehearsal studio was built on top of the Quartz/CORBA framework,
which is responsible for enforcing the requirements imposed by the application. Audio
sources and sinks are virtual devices in the context of the A/V streams mechani sm.

Sources and sinks are connected to flow producers and consumers respectively, which
allow them to transfer the audio signal through the network. In addition, Quartz
enforces the QoS constraints imposed by the applications in order to avoid audio
packet s being delayed by a possible lack of resources at network or operating system
levels. Audio sampling and reproduction are performed by using, respectively, the
waveIn API and the Microsoft DirectSound API, an integrated part of DirectX 3.0 [98] .

Figure 27  shows the user interface of the distributed rehearsal studio. Through this
interface, the musician can create audio sources and sinks, and can select the quality
with which the audio is encoded. Audio  controls such as volume and panning (balance)
are also provided.

                                                                     Figure 27  ˘  Interface of the Distributed Music Rehearsal Studio

Tests with the prototype implementation of the distributed music rehearsal studio have
shown that d elays still largely exceed the desired limit of 30 milliseconds. This is due to
the unpredictable latency introduced by the waveIn API and by the audio drivers
provided by the operating system. Unfortunately, the API and the drivers do not provide
resource  reservation mechanisms that allow us to limit the latency. This does not affect
the role of the Quartz/CORBA framework, which is able to enforce QoS by reserving
bandwidth for the application and by shielding the application from any interference
caused b y excessive CPU usage.

6.6  Analysis of the Quartz/CORBA Framew ork

With the adoption of the CORBA architecture support ˘  both the client - server and
stream interaction models ˘  as the core of the distributed multimedia framework,
multimedia applications are giv en the ability to handle control data and stream data
uniformly using high - level abstractions. The object - oriented nature of CORBA provides
a large set of benefits to the application development process (e.g. reusability,
encapsulation, use of software eng ineering techniques, etc.). In addition, the adoption of
the CORBA streaming mechanism together with network protocols with multicast
capabilities makes efficient and scalable group communication feasible. Furthermore,
the framework supports the provision of QoS requirements described as A/V Streams

QoS parameters through the use of Quartz for translation and enforcement of QoS
requirements imposed by applications.

Several other proposals of programming supports for the development of multimedia
applicatio ns in open systems, which were presented in Chapter 3 , aim to achieve similar
results by adopting different approaches.

The ReTINA project [18]  has basically the same goals as our proposal, but the  adoption
of a binding model inherited from ODP introduces a new level of complexity that has to
be handled by the application programmer. Our approach maintains the simplicity and
transparency of the CORBA binding model, incorporating a binding paradigm
a ppropriate for multimedia applications through the introduction of a stream abstraction,
which allows connections with associated QoS specifications and multi - party
connections.

Furthermore, ReTINA proposes extensions to the CORBA IDL for the introduction of
stream interfaces. Major changes in the IDL are not likely to be well accepted by the

OMG and by the CORBA community, and may reduce the compatibility between
different ORBs. On the other hand, the Quartz/CORBA framework for distributed
multimedia appli cations that was proposed by us is entirely compatible with the current

OMG specifications for ORBs and for the IDL language.

The same considerations apply to the DIMMA [116]  and Amber [86]  projects
developed by APM that had a strong influence on the ReTINA project.

The XRM [88]  project is a proposal for a framework that provides multimedia
applications with QoS specification mechanisms together with an appropriate bindin g
architecture, called Xbind, which is built upon CORBA. XRM and Xbind, however, do
not provide some features that are provided by Quartz such as QoS enforcement at the
operating system level and resource adaptation.

The TAO project [129]  proposes optimisations on the communication support to
improve the performance achieved in method calls between clients and servers. Despite
recognising that a better performance has to be provided by the CORBA
communication protocols, we consi der that this is not sufficient for the provision of
transfer of media data, since high performance does not necessarily guarantee the QoS
requirements imposed by distributed multimedia applications.

Several other projects in the field of distributed mult imedia, such as SUMO [35]  and

DAVE [49] , do not adopt an approach based on standards for distributed object
computing, constraining their utilisation in open systems and limiting their acceptance
by  computer software developers. On the other hand, our multimedia framework adopts
an approach based on standard solutions (i.e. CORBA) in order to provide and
environment for development and execution of multimedia applications.

6.7  Summary

This chapter prese nted a framework for building multimedia applications. This
framework shows how Quartz can be used by middleware platforms such as CORBA in
order to allow applications to impose QoS constraints on the services provided by the
underlying system . An implemen tation of the Quartz/CORBA framework was
presented, together with a multimedia application that was built using the framework.

We have also analysed the achievements of the framework and compared it to similar
support for the development of multimedia appl ications.

7

Validation and

Evaluation

This chapter presents a series of validation tests, which were executed in the form of
application examples that were implemented using the Quartz prototype. In addition, we
analyse the characteristics of Quartz, takin g into account the requirements that were
imposed on it during the design phase. Finally, we compare Quartz to other supports for

QoS specification and enforcement that are described in the literature.

7.1  Validation Tests

We have implemented some application s on top of the prototype of Quartz in order to
analyse whether or not Quartz meets the requirements imposed during the design phase.

These applications ˘  the remote copy application, the telephone exchange application,
and a new version of the distributed  music rehearsal studio that is built directly on top
of the sockets API ˘  are described in the following sections. Further in this chapter, we
present some conclusions based on the experience obtained with these applications, and
provide some performance measurements that quantify the overhead imposed by Quartz
in the form of processing time.

7.1.1  The Remote Copy Application

In order to evaluate the behaviour of Quartz in an environment with multiple network -
level reservation protocols, we have implemented a Wi ndows - based version of the Unix
remote copy command. The ^
rcp
~ command allows users to transfer files between
machines interconnected by a network. Our ^
rcp
~ application goes beyond the Unix
command by providing a graphical interface that allows the user t o choose between
multiple network protocols and to specify QoS requirements that are to be observed in
the file transfer operation. This application uses Quartz to enforce its QoS requirements.

By using the graphical interface, which is shown by Figure 28 , the user is able to
specify the name of the file to be transferred and select the protocol to be used for data
transfer. The user can choose between three different communication protocols: TCP,

UDP and ATM. In the first two cas es, RSVP is used for resource reservation, while

ATM is used directly in the latter case.

The role played by the application (i.e. client or daemon/server) must be specified on
startup. Information needed to establish the connection also has to be provide d by
clients. This information consists of the host name, IP or ATM address and the
communication port of the destination. IP multicast is also supported. In this case, the
user has to specify an IP multicast address in the `target address´ field for the ( possibly
multiple) clients and the daemons.

Figure 28  ˘  The Remote Copy Application

In addition, the graphical interface allows the user to specify QoS requirements such as
the kind of guarantee (best - effort, unloaded or determi nistic), the size of data packets,
and the packet rate. These requirements are interpreted by the application filter for data
packet transfer, which is implemented by class

QzDataPacketFilter

. The QoS
parameters understood by this filter are listed by Table 17 .

Parameter Name  Description

DPkt::PacketSize [Min,Max]
Size of packets (in bytes)

DPkt::DelayBetweenPackets

[Min,Max]

Time between production of two consecutive
packets (in milliseconds)

DPkt::EndToEndDelay

[Min,Max]

Time between production and consumption of a
packet (in milliseconds)

DPkt::ErrorRatio [Max]
Acceptable error ratio (in bits per million)

DPkt::Guarantee
Guarantee level (best - effort, deterministic, etc.)

DPkt::SecurityLevel
Security level (none, encrypted, etc.)

                                                                                  Table 17  ˘  Parameters Recognised by the Data Packet Filter

The data packet filter performs the translation of these parameters into the generic set of
application parameters defined by Quartz. This translation step is very st raightforward,
since these parameters are very similar to the generic application parameters used by

Quartz. The parameters resulting from this first translation step are translated further
into system parameters and passed to the system agents that perfor m the necessary
reservation of resources at lower level. The application provides an interface for Quartz
so that it can perform upcalls in order to report errors, warnings or dynamic changes in

QoS.

This application was based on the sample provided togeth er with Intel´s implementation
of RSVP. The addition of Quartz as a means for reserving resources simplified the
application and allowed us to incorporate support for ATM without increasing
complexity. According to the protocol selected by the user, the co rresponding system
filter and agent are plugged into the QoS Agent, and from this point the translation of
parameters and the reservation of resources are handled directly by Quartz according to
the selected protocol.

The remote copy application shows us that Quartz is able to perform QoS reservations
by using both ATM and RSVP without interfering with the way the application
specifies QoS and requests QoS to be enforced. In addition, the application code is
simplified and made more portable by the use of Quartz due to the separation between
data transfer, which is performed by the application directly, and QoS enforcement,
which is executed by Quartz.

7.1.2  The Telephone Exchange Application

In order to show the use of Quartz in an environment distinct from the traditional
computing environment ˘  i.e. desktop machines interconnected by a computer network
such as the Internet ˘  we have implemented a software model of a telephone exchange.

Telecommunications systems are subject to QoS requirements stipulated by gov ernment
regulatory agencies (such as the FCC in the US, OFTEL in the UK and the ODTR in

Ireland), international organisations (such as the ITU - T) and internal standards defined
by telecom operators. Very strict limits on the time the system takes to proces s a phone
call are defined by the companies and regulatory bodies. Consequently, real - time
software has to be run on the telephone exchange so that the call set - up process can be
time bound. When these requirements are not fulfilled, besides the degradatio n of the
service provided to the consumer, it may result in hefty fines imposed by regulatory
bodies and, ultimately, in the suspension of the license to operate the
telecommunications service.

The processing of a telephone call passes through well - define d stages [48] , which are
illustrated in the state transition diagram in Figure 29 . Two of these stages, which are
performed by a computerised telephone exchange and are subject to QoS requirements,
are  of particular interest for this study.

The exchange is responsible, after the customer takes the phone off the hook, for
reserving a path from the customer´s equipment to the exchange. After that the
exchange has to perform an initialisation procedure. F irst, it has to identify the customer
by mapping the phone line through which the off - hook signal was received to a
directory number and a customer name, to whom the call will be charged afterwards.

The exchange is also responsible for identifying the clas s of service to which the
customer is subject. The class of service defines the way in which the call will be
handled, including charging methods and rates, authorisation for long - distance calls and
for using premium services, etc. After this is accomplish ed, a dial tone is sent to the

127

                                                                                                                    customer´s terminal. The time taken by this whole process is expected not to exceed the

                                                                                                                    limits imposed by regulatory bodies or by the companý s own quality standards,

                                                                                                                    characterising the first QoS requirement imposed on the ca ll initialisation process. We

                                                                                                                    refer to it as the ^dial - tone deadline~ from now on. In the figure, it is represented by the

                                                                                                                    time taken to change from state

b  to state

c .

In a second phase, after the customer dials the phone number to which he wants to be

co nnected, the exchange is responsible for routing the call to the destination, reserving

lines along the way. When the lines are reserved, a ring tone is sent to the caller and a

ringing signal is sent to the called phone. If an available route is not found  because there

are no lines available or because the called party is busy, a busy tone is sent to the

caller. The time taken to route the call and send a calling tone (or busy tone) to the

caller is also subject to limits, resulting in the second QoS requi rement imposed on the

call set - up process. We refer to this as the ^ring tone deadline~. It corresponds to the

time spent to change from state c  to state

d

Ring T one

Got Answer?

e

T alk

Route

Call

c

Dial T one

Initialise

Call

b

Idle

f

Busy T one

No

No

Yes

Yes

Figure 29  ˘  State Diagram of a Telephone Call

The call clean - up process is not subject to QoS requirements from the exchange´s point
of view. The quality of the phone line through which the conversation takes place is
also subjected to requirements, but this does  not interfere directly with the call
initialisation and routing process.

We have implemented a simplified software model of a telephone switch in order to
evaluate the capacity of Quartz as a mechanism for enforcing the QoS requirements
present in the cal l switching process, i.e. the dial tone and ring tone deadlines. In
addition, Quartz also performs the allocation of telephone circuits.

This application example is built on top of Windows NT and is totally written in C++.

An application filter for circu it switching, a system filter and agent for deadline - based
scheduling, and a system filter and agent for reservation of telephone circuits have been
written by us.

Class

                                                  QzCircuitSwitchFilter
 implements the application filter for circuit
switching. It rec ognises the parameters listed by Table 18 , which are proper for
applications such our telephone exchange simulator, and translates them into generic

QoS parameters.

Parameter Name  Description

CSw::CircuitType  Type of circuit (PO TS, ISDN, T1, E1, etc.)

CSw::CircuitDelay [Min,Max]  Total transmission delay (in milliseconds)

CSw::SwichingDelay [Min,Max]  Total switching delay (in milliseconds)

CSw::ErrorRatio [Max]  Transmission error (in %)

CSw::Guarantee  Guarantee level (best - eff ort, unloaded, etc.)

CSw::CircuitCost [Max]  Financial cost (in local currency per second)

CSw::SecurityLevel  Security level (none, encrypted, etc.)

                                                                         Table 18  ˘  Parameters Recognised by the Circuit Switch Filter

In order to simulat e the allocation of phone lines, we provide a system agent for
allocation of phone circuits implemented by classes

QzPhoneCircuitAgent
.

The phone circuit agent is used together with a system filter for phone circuits,
implemented by class

QzPhoneCircuitFi lter
. This filter translates the system -
specific parameters listed in Table 19  into the generic QoS parameters defined by

Quartz.

Parameter Name  Description

Phone::CircuitType  Type of circuit (POTS, ISDN, T1, E1, etc.)

Phone::C ircuitDelay [Min,Max]  Total transmission delay (in milliseconds)

Phone::ErrorRatio [Max]  Transmission error (in %)

Phone::Guarantee  Guarantee level (best - effort, unloaded, etc.)

Phone::CircuitCost [Max]  Financial cost ( in local currencyper second )

Pho ne::SecurityLevel  Security level (none, encrypted, etc.)

                                                                           Table 19  ˘  Parameters Recognised by the Phone Circuit Filter

Initially, the same operating system agent for Windows NT that was used in the other
examples was used by this ap plication. Later, a system agent and a system filter for
deadline - based process schedulers were written in order to take into account the
establishment of deadlines for the processing of switching tasks. The system agent and
the system filter for deadline schedulers are implemented by classes

QzDeadlineSchedAgent
 and

QzDeadlineSchedFilter
 respectively. The system -
specific QoS parameters understood by these components are listed by Table 20 .

Parameter Name  Description

DlSched::Dead line [Min,Max]  Processing deadline (in milliseconds)

DlSched::Guarantee  Guarantee level (best - effort, unloaded, etc.)

                                                    Table 20  ˘  Parameters Recognised by the Deadline Scheduling Filter

Our model of a telephone exchange is able to process 10 phone calls concurrently. For
each phone call, the exchange reserves the circuit from the customer´s equipment to the
exchange and sets the dial tone deadline for the call initialisation process. After the
customer dials the number of the called  terminal, a new reservation is performed, which
allocates a circuit from the exchange to the called terminal and sets the calling tone
deadline for the routing process.

Reservation of resources is simulated by the phone circuit agent, because the actual
a llocation of resources would require the presence of actual switching hardware.

Similarly, the deadline - based scheduling agent only simulates the scheduling of the
switching tasks, since the platform in which the application was implemented does not
provi de deadline - based scheduling mechanisms.

The telephone exchange application shows how QoS requirements very different from
those present in traditional computer applications can be expressed using the
specification mechanisms provided by Quartz. This exam ple also shows that, despite the
different nature of the platform that provides resources for the application, Quartz is
able to interpret the high - level requirements and perform resource reservations at the
low level.

7.1.3  The Distributed Music Rehearsal Studi o

A new version of the distributed music rehearsal studio has been built in order to
evaluate the use of Quartz as a mechanism for QoS enforcement that is used directly by
a multimedia application, instead of being used indirectly by applications through
m ultimedia middleware. This new version of the rehearsal studio uses sockets directly
instead of the CORBA A/V streaming mechanism for transferring media data.

Compared to the version described in section 6.5 , the functionality  of the application
and the user interface remained the same. The only difference can be found at
networking level, where the dependencies on CORBA have been removed. This made
the application more lightweight, reducing the executable by approximately 10 t imes
the original size, and less memory - hungry, reducing the memory allocated by the
application in about 30%. Despite these advantages, there was no noticeable
improvement in the overall performance of the audio transmission, since the problems
with the l atency originated from the waveIn API and from DirectSound.

This example shows that multimedia applications, such as the music rehearsal studio,
can avail of the QoS specification and enforcement mechanisms that are provided by

Quartz in order to have the ir QoS requirements fulfilled.

7.1.4  Results Achieved w ith the Validation Tests

Table 21  summarises the applications built using Quartz for test purposes. These
applications have been selected in order to demonstrate the fulfilment of the
requirements imposed on the Quartz architecture during the design process, which were
described in section 4.1  of this thesis.

Application  App. Filter  OS Agent & Filter  Network Agent & Filter

Remote Copy  Data Packet  WinN T  RSVP, ATM

Telephone

Exchange

Circuit Switch  Deadline Scheduler,

WinNT

Phone Circuit

Rehearsal Studio  A/V Streams  WinNT  RSVP

Table 21  ˘  Applications Built Using Quartz

An initial observation of the nature of the tests shows that  Quartz can be used in
different areas of application besides multimedia transfer, demonstrated previously by
the Quartz/CORBA framework and the rehearsal studio application. The test
applications show that Quartz is also suitable for specification and enf orcement of QoS
for data transfer applications (such as the remote copy example) and for real - time
applications (such as the telephone exchange model).

In addition, the tests described previously, including the rehearsal studio, show the
adequacy of the mechanisms for specification of QoS provided by Quartz. In each of the
examples, the QoS parameters seen by the application, either when it specifies its QoS
requirements or when it receives a QoS notification, are in the form of application -
specific param eters which are suitable for the particular application area.  The

Quartz/CORBA Framework (and consequently the rehearsal studio) uses parameters
describing the quality of audio and video streams. The format of these parameters is
defined by the A/V stream s specification and is translated by the corresponding filter.

On the other hand, the remote copy example uses a data packet filter that recognises
parameters for applications transferring data packets, while the telephone switch
application uses a differe nt set of parameters appropriate for circuit switched lines and
for deadline scheduling. An application filter translates application parameters into

Quartz - defined generic parameters in each case.

The remote copy example also shows that the resource prov ider can be changed without
interfering with the application code. The remote copy application shows that even
using a different network resource provider, which in this case could be either RSVP or

ATM, the user can obtain similar QoS - constrained services . This shows that the lower -
level reservation protocols supported by the networking infrastructure are made
transparent for the application. Consequently, applications using Quartz are highly
portable, since the code necessary for requesting QoS behaviour is kept unchanged
independently of the underlying system that is providing resources for the application.

On the other hand, the telephone exchange application shows that the component
responsible for the reservation of resources provided by the operating  system can be
exchanged in a similar way. In this case, we use either a simulator for deadline
scheduling or the same Windows NT agent used for the other examples for processing
and routing phone calls.

The multiplicity of operating system and network age nts and filters used by the
examples shows that Quartz can be used in different platforms, and that the filters can
be combined freely in order to reflect the characteristics of the underlying system.

7.1.5  Performance

Performance tests have shown that the ove rhead added by Quartz to the application is
very small. Table 22  shows typical values for the overhead imposed by Quartz for the
remote copy application. This data was obtained on a Pentium Pro 200 MHz by using
the profiling tools  that accompany Microsoft Visual C++ 5.0. The complete results of
the tests are shown in the appendix of this thesis.

                  ATM  RSVP

                 Initialisation of Reservation Protocols  N/A  24.859 ms

                 Initialisation of Quartz

346
m
s
9.272 ms

                 Overhead per Reservation  1.177  ms  1.220 ms

                 composed of:  QoS Specification

93
m
s  113
m
s

                   QoS Translation

759
m
s  991
m
s

                   QoS Reservation

325
m
s  116
m
s

Table 22  ˘  Overhead Imposed by Quartz

The total overhead caused by Quartz in a single request (i.e. the tim e taken to specify,
translate and interact with the resource reservation protocols) is about 1.2 millisecond
for both ATM and RSVP. This value is considerably less that it takes to open a socket

(about 10 ms) or to obtain the host name (which in our testbe d varied from 5 to 40 ms).

The initialisation of Quartz is also considerably fast even for RSVP, which takes
relatively long to initialise due to the amount of state information that has to be gathered
by both WinSock and Quartz; since in ATM the reservat ion mechanism is integrated
with the transport, no extra time is taken to initialise it.

During the tests we have used the real - time scheduling class provided by Windows NT
in order to reduce the influence of other processes in the results. The overhead,
h owever, can still vary about
±

4% for both RSVP and ATM under similar load
conditions due to unpredictability introduced by the system services that are used by

Quartz (i.e. the values shown in Table 22  have an error of
±

4%).

The  overhead caused by the initialisation of Quartz occurs only once, while the request
overhead occurs every time the application requests a new set of QoS requirements to
be enforced. There is no overhead imposed on the transmission of data, which depends
o nly on the networking infrastructure and on the resources reserved for the session.

7.2  Fulfilment of Requirements

The following items explain how the requirements imposed during the design phase,
which were listed in section 4.1 , are fulfilled by the Quartz architecture.

7.2.1  QoS Specification

Quartz allows users to specify QoS requirements according to the notion of QoS
understood by them. This is achieved by adopting a multi - step, extensible translation
mechanism.

The translation uni t understands parameters specified at application level by using
application filters, which can be selected from a library or written by the user. The
examples presented show that these filters can handle a wide variety of formats of QoS
parameters. These different sets of parameters, each one representing a different notion
of QoS present at application level, can be easily translated into a generic format used
internally by the translation unit as shown by the applications implemented using

Quartz.

Simil arly, the system filters were shown to be able to perform the translation of generic
parameters adopted by Quartz into QoS parameters meaningful at the lower level. These
filters were implemented for different reservation protocols with different notions o f

QoS, such as ATM and RSVP at the network level, and for the Windows NT real - time
support and for deadline - based schedulers at the operating system level, showing the
suitability of Quartz for handling QoS in heterogeneous systems.

At the same time, the a pplication and system filters are made easy to implement since
the main translation step is performed by the interpreter. The interpreter handles the
translation between different abstraction levels (i.e. translates parameters from the
application level in to the system level), balances requirements between the network and
the operating system, and performs QoS adaptation whenever necessary. Consequently,
these aspects do not have to be handled directly by the application or systems filters.

A typical filter  (such as the data packet filter and the RSVP filter) has less than 300
lines of code, and should take an average programmer less than one working day to
define the mapping between parameters, and then write and test the filter.

7.2.2  QoS Enforcement

The user i nterface defined by the Quartz QoS architecture hides from the user the details
regarding the way in which resources provided by both the network and the operating
system are reserved. This allows the application to have its QoS requirements enforced
indep endently of the characteristics of the sub - system that is providing the resources.

Quartz can be seen as a common interface to the diverse resource providers present in a
computing system. It has a common form of specification and notification of QoS,
des pite the fact that the resources have to be reserved by using different specification
methods. Consequently, the resource provider is made transparent for the user, which
interacts only with Quartz in order to obtain resources from the system.

Applicatio ns built on top of Quartz are able to have their QoS requirements enforced by
using different supports without having to change the way their QoS requirements are
specified. This is demonstrated by the remote copy example, which uses multiple
reservation p rotocols at network level (i.e. ATM and RSVP), and by the telephone
exchange application, which shows that the component responsible for the reservation
of resources provided by the operating system can be exchanged in a similar way. This
occurs because Qu artz provides full transparency from the lower - level reservation
protocols present at both network and operating system level in regard to the way they
handle QoS reservations.

7.2.3  Heterogeneity

The application examples show that Quartz can be used in conjunct ion with different
reservation protocols on different platforms. The differences in the lower - level support
are handled by Quartz without requiring the application to get involved. The application
code, in addition, does not have to be modified when the re source reservation protocol
present in the underlying system is replaced by a different one.

Despite the limited range of lower - level resource reservation mechanisms covered by
the prototype, we have deliberately chosen resource reservation mechanisms that  are
very different in nature so that we can assume that other system filters and agents can be
written in order to support other mechanisms for resource reservation.

Extension of the set of platforms supported is not a very complex task. Support for new
reservation mechanisms can be added to Quartz by writing a system agent and filter.

Like filters, simple system agents such as the ATM agent and the Windows NT agent
have about 300 lines of code and can be implemented and tested in no more than one
working  day by a programmer that is familiar with the reservation mechanisms
provided by the reservation protocol. Protocols with more complex APIs, however, can
take longer to implement and test. The RSVP agent, for example, has about 1000 lines
of code and we e stimate that it would take about a week for a programmer to rewrite it.

Similarly, different application areas have been covered by the examples implemented
on top of Quartz. Support for different notions of QoS present at different areas of
application wa s added by writing new application filters and then plugging these filters
into the QoS Agent. As a result, we can assume that other different areas of application
can be supported by Quartz without involving a high degree of complexity.

7.2.4  Support for Adapta tion

Adaptation is supported by Quartz at two levels:

·

                         Adaptation at application level; and

·

                         Transparent adaptation at system level.

Adaptation is initiated every time the allocation of resources changes at a lower level.

However, depending on the level at w hich it is performed by Quartz, adaptation has a
different effect from the application´s point of view.

Adaptation at system level occurs by rearranging the allocation of resources used by the
application, so that the same QoS requirements are enforced by  using a different set of
resources. This process is transparent for the application, since the QoS seen at
application level remains the same. This process is successful only when it is possible to
rearrange the balance of resources so that the QoS requir ements specified by the user
are fulfilled.

Adaptation at application level is initiated when adaptation at system level fails. In this
case, Quartz requests the application to perform adaptation by sending a notification
message to the application in the form of an upcall. The notification message carries
parameters understood at the application level, which are obtained by using the reverse
path of translation provided by the translation unit. Whenever an application receives a
request for adaptation, it has to adapt its QoS requirements and issue a new request for

QoS.

By incorporating these two mechanisms for adaptation, Quartz provides a robust
support for applications running on platforms in which the state of the resources might
change dynamically. S ome of the resource reservation protocols available at the
moment allow changes in the state of resources to happen at run - time, and consequently
it is important to make the QoS architecture able to handle this situation.

7.3  Comparison w ith other QoS Architec tures

Most of the QoS architectures found in the literature and presented in Chapter 3 ,
including Xbind [88]  and QUANTA [43] , are basically network - oriented (and mostly

ATM - oriented) architectures, i.e., they do not cover system - level QoS constraints.

The matter of translation and mapping is very simplified in Xbind and QUANTA
because QoS is handled at network level only. In addition, the tight integration of the
archite cture with the communication system that occurs in Xbind and also in QoS - A

[24]  constrains the flexibility and limits the extensibility of the architecture. On the
other hand, translation and mapping have a special role in Quar tz, which is able to cover
a wider range of QoS requirements specified at a higher level of abstraction.

QUANTA and ERDoS [26] [27]  adopt translation mechanisms similar to the one
proposed in this t hesis, but there are a few differences that can be observed. First, the
introduction of two sets of generic QoS parameters with a translator from one generic
set into the other reduces the work done by QoS filters, which can be added by the
application pro grammer and are easy to implement due to their low complexity. On the
other hand, QUANTA translators, equivalent to our system filters, involve a more
complex translation procedure and are not accessible to the user. As a consequence,
support for new areas  of application or network protocols would require changes in the
code of the middleware. ERDoS incorporates its translation mechanisms into the
resource and application agents, which can be written by the user as in Quartz.

However, due to the adoption of  an approach for provision of QoS based on monitoring
and adaptation, QoS enforcement through resource reservation is not provided by

ERDoS.

Like ERDoS, MMN [147]  also uses adaptation mechanisms instead of resource
reservation . This approach prevents the use of these architectures for implementing
applications with strong QoS requirements due to the lack of support for service
guarantees other than best - effort [52] .

Researchers at Lancaster say tha t a single QoS manager such as the QoS Broker in the

OMEGA architecture [101] [102]  `requires a huge amount of mapping and management
knowledge to support large - scale distributed applications, and th at service management
through a single entity is too centralised and severely inflexible´ [148] . We don’t incur
this problem because per - application QoS Agents encapsulate only the support
necessary for specification of QoS cap abilities for the corresponding application field
and interaction with the reservation protocols supported by the end - system. Flexibility
and extensibility are guaranteed by the use of filters and system - specific agents, instead
of a monolithic structure s uch as adopted by the QoS Broker. Issues regarding resource
reservation are handled by the corresponding protocol associated to the sub - system that
provides the resources, with system agents being responsible only for interfacing with
these protocols.

QuO  [156]  and Arcade [42]  are architectures that provide QoS languages for the
specification of QoS requirements. We could simulate the same functionality by
implementing application - level QoS filters that interpret the QoS languages used by

QuO and Arcade and translate the QoS requirements expressed with this language into
the generic application - level QoS parameters used by Quartz.

 QuO is a network - oriented architecture that adds mechanisms for QoS sp ecification to

 the client - server interaction model adopted by CORBA. Based on this approach, QoS

 requirements are specified in relation to method invocations issued between CORBA

 objects. However, the client - server interaction model is inappropriate for ap plications

 that use continuous media due to the necessity of modelling streams as a series of

 method invocations [37] . We believe that this approach is likely to impose limitations to

 the use of the QuO architecture.

 Arcade is  an example of a purely system - level QoS architecture based on a specific

 platform, in this case the Chorus kernel. Quartz could be easily made able to interact

 with this operating system by writing a system agent and a system filter that interface

 with th e QoS mechanisms provided by Chorus. In addition, Quartz allows the user to

 establish network QoS constraints.

 Table 23  is a new version of the table showed during the analysis of the state - of - the - art

 in the area of QoS architect ures, which was presented in section 3.13 . This new version

 of the table adds Quartz to the list of QoS architectures, and shows that our architecture

 has a number of features that is not matched by the other architectures foun d in the

 literature.

X
b
i
n
d

R
e

T

I

N

A

D

I

M

M

A

S

U

M

O

T

A

O

A
r
c
a
d
e

O

M

E

G

A

Q
o

S

˘

A

Q
u

O

Q

U

A

N

T

A

E

R

D
o

S

M

M

N

Q
u
a
r
t
z

                                                                                                      Multimedia Support

>

>

>

>

>

>

>

>

>

>

>

>

                                                                                                          Real - Time Support

>

>

>

>

>

>

>

>

                                QoS

   Specification

Extensible

>

>

>

                                                                                                   Network Reservation

>

>

>

>

>

>

>

>

                                                                                                                 O.S. Reservation

>

>

>

>

>

>

>

                                QoS

    Enforcement

Transparent

>

>

>

>

>

>

>

>

                                                                                                              Multiple Protocols

>

>

>

>
        Support for

Heterogeneity

Extensible

>

>

>

Notification

>

>

>

>

>

>

>
        Sup port for

          Adaptation

Transparent

>

>

>

                                                                      Table 23  ˘  Comparison of Quartz with other QoS Architectures

Quartz is suitable for open systems due to its capacity to interact with multiple
reser vation protocols at both network and operating system level. In addition, Quartz
provides support for QoS specification and enforcement to applications situated in
different application areas, and is able to handle resource adaptation either transparently
or by notifying the application. Furthermore, Quartz can be easily extended by the
application programmer in order to use other resource reservation protocols and to
provide QoS specification mechanisms appropriate for different application areas.

7.4  Summary

This chapter showed that Quartz provides an efficient service for applications requiring

QoS specification and enforcement in open distributed systems. Different areas of
application and underlying systems are covered by Quartz, as shown by the validation
tests implemented on top of the prototype of the architecture.

This chapter has also shown that Quartz provides a number of improvements when
compared to other architectures and frameworks for distributed multimedia that are
found in the literature.

8

C onclusions

The research project presented in this thesis has resulted in the design of an innovative

QoS architecture whose properties make it useful in an open environment where
applications require QoS - aware services to be provided by the underlying syst em.

This chapter summarises the characteristics of the Quartz architecture that make it
particularly useful in open systems. In addition, it presents the achievements of this
research project in the light of other work in this area of research, and sugges ts some
future developments making use of the proposed QoS architecture.

8.1  Background

Analysing the requirements of distributed applications, researchers have found that an
important class of applications is not satisfied with the best - effort approach to res ource
management offered by the computing platforms available today. Instead, these
applications impose more strict requirements on the services provided by the computing
platform, not only from the local machine but also the communication network and
othe r remote services. These requirements are called the quality of service (QoS)
required by the application.

The necessity of providing support for QoS enforcement drove the research community
to improve the support for resource reservation available in net works and operating
systems. In essence, this effort aims to make access to the resources provided to
applications behave in a more predictable fashion, avoiding the typical best - effort
resource management policies that are provided by most platforms.

Des pite the effort spent in the development of resource reservation protocols, there is
still a gap between what the application sees at its level ˘  i.e. its QoS requirements ˘
and what is provided by the underlying system ˘  i.e. protocols for reserving resou rces
such as bandwidth, processing power, and so on. This gap has to be filled by a
middleware layer in order to avoid application programmers having to deal with low -
level concepts necessary for interacting with resource reservation protocols.

Research on  middleware responsible for bridging the gap between applications and
resource reservation protocols has resulted in proposals for what are now called `QoS
architectures´. Examining the proposals for QoS architectures present in the literature
concerning t heir ability to provide support for the deployment of applications with QoS
requirements in open systems, we have identified several significant problems:

·

                         the way in which these architectures allow applications to specify their QoS

                         requirements typically s uits only a limited area of application, and often requires

                         QoS to be expressed in a low - level format that is unsuitable for the application;

·

                         requirements are often enforced either at network or operating system level, instead

                         of both, and the underlying system is not always made transparent to the application,

                         forcing it to deal with low - level issues;

·

                         these architectures are usually closely tied to a particular platform, such as a

                         particular networking infrastructure and/or operating system; and

·

                         dynamic resource adaptation is not always taken into account by architectures,

                         which ignore the fact that the state of resources can change at run - time in some

                         platforms.

With these problems in mind, we have designed and implemented a novel architecture
for QoS sp ecification and enforcement. This architecture, called Quartz, addresses the
limitations of previous proposals in this area.

8.2  The Quartz Architecture

Our main objective while developing Quartz was to design an architecture that would
provide QoS - constraine d services for a wide range of applications running in open,
distributed and heterogeneous systems. The solution adopted to deal with this situation
was to design Quartz in a way that would make it possible for the architecture to
reconfigure itself intern ally in order to fulfil the particular needs of the surrounding
environment. This was achieved by adopting a component - based design, with each
component being responsible for a particular task in dealing with a particular area of
application or with a spec ific resource reservation protocol.

In this design, an architectural core is populated with interchangeable components.

Different components handle the different notions of QoS present at application level,
allowing the architecture to understand the requ irements of different applications.

Similarly, other components are responsible for dealing with the different resource
reservation mechanisms that may be present in the underlying system

Quartz allows applications to specify their QoS requirements by usin g QoS parameters
appropriate for their particular application area. The parameters specified by
applications are handled internally by Quartz and translated into a format suitable for
performing resource reservations. After translating QoS parameters, Quar tz enforces

QoS by reserving resources provided by the underlying system. The reservation of
resources is done by interacting with resource reservation protocols provided by the
network and the operating system.

The implementation of the Quartz QoS archit ecture, together with a series of test
applications that make use of the QoS mechanisms provided by Quartz, demonstrated
that the requirements expected from the architecture prior to the design phase have been
achieved. Validation tests have shown that Qua rtz allows QoS to be specified in high -
level formats appropriate for different application areas; enforces QoS transparently
from the application´s point of view and at both network and operating system level;

and is able to use multiple reservation protoc ols in order to enforce the QoS
requirements of the application. Quartz also provides support for resource adaptation by
either transparently adapting QoS or by notifying the application that it has to reduce its
requirements. Moreover, we have verified th rough performance tests that the overhead
caused by Quartz is very small compared to related system activities.

In our understanding, Quartz, due to its unique combination of features, consists in an
important step forward in the design of architectures i ntended to bridge the gap between
applications in need of QoS - constrained services and the mechanisms for resource
reservation that are provided by underlying systems.

8.3  Contribution

The main advantages of Quartz are provided by its component - based architec tural
design, which makes it flexible and extensible and allows it to handle the different
notions of QoS present at application level and the heterogeneity found at system level
in open systems.

The interfaces used by the application to specify its QoS r equirements can be adapted in
order to recognise the different formats of QoS parameters that are appropriate for
different application areas. The application interface, however, is independent of the
reservation protocols present in the underlying system,  making them transparent for the
application. The provision of transparency from the lower - level resource reservation
protocols simplifies the task of building applications with QoS requirements and
significantly increases their portability.

Quartz is fle xible enough to adapt itself to dynamic changes in the underlying system by
replacing the components used internally by the architectural support. Whenever a new
resource provider and an associated resource reservation protocol are added to the
underlying system, a new component able to interact with the resource provider can be
added to the architecture in order to perform resource reservations on behalf of
applications. In this case, a component responsible for translating between the format
used by the n ew reservation protocol to express QoS requirements and the generic QoS
parameters used internally by Quartz must also be added to the translation unit of the
architecture.

Changes at application level can be also accommodated by Quartz. In order to
under stand the different ways used by applications to express their QoS requirements,

Quartz allows a translation component to be replaced. This component, the application
filter, is responsible for translating between the QoS parameters used by the application
and the generic QoS parameters used internally by Quartz.

New components can be selected from a library or, in cases where no appropriate
component is available, they can be written by the application programmer. Since each
component performs a very part icular role in the overall architecture, the knowledge
necessary for implementing them is limited. Independence between components, which
communicate through a set of well - defined interfaces, ensures that components can be
combined freely.

Transparent QoS  enforcement is another feature provided by Quartz, since the
architecture is designed in a way that the application is unaware of the mechanisms used
for resource reservation at lower levels. The interaction with resource reservation
mechanisms is perform ed by components of the architecture specialised for interacting
with each of the resource reservation protocols present in the underlying system.

Another important feature supported by Quartz is dynamic resource adaptation.

Adaptation is supported at both  system and application level. The architecture provides
mechanisms to receive notifications of any change in the QoS supported by the
platform. Whenever changes occur, the architecture tries to perform adaptation at
system level, rearranging the balance o f resources in order to compensate for any losses
resulting from the dynamic adaptation. When adaptation at system level is not feasible
due to the impossibility of compensating for the resources lost, the architecture informs
the application, which has to  degrade its QoS requirements.

In addition, Quartz is able to enforce QoS at both network and system level, in
comparison with other QoS architectures presented in the literature, which usually
concentrate on only one of them.

8.4  Perspectives for Future Work

Since Quartz can be deployed on different platforms and can provide QoS for different
areas of application, the possibilities of using the architecture are very diverse.

One of the possibilities for future work that we envisage for Quartz is the porting of the
prototype to a wider variety of computing platforms. At operating system level, it would
be interesting to add support for real - time operating systems such as Chorus [1 42] ,

VxWorks [151]  or Q NX [62] . Support for new reservation protocols at network level,
such as the Scalable Reservation Protocol (SRP) that is being developed by the IETF

[1] , could also be added in order to expand the p latform coverage. This would be done
by implementing new components of the architecture that interface with these
reservation protocols.

Being a component - based and extensible architecture, Quartz can also be modified in
order to implement new resource ba lancing algorithms and adaptation policies. In fact,

Quartz can be used as a toolkit for testing new policies and algorithms by writing new
components and plugging them into the architecture.

Another possibility for future work involving Quartz is in deve loping new applications
that make use of the architecture for QoS specification and enforcement. We foresee
several possibilities for Quartz and the Quartz/CORBA framework, more specifically in
the fields of distributed multimedia, real - time applications, and telecommunications.

In the area of distributed multimedia, we envisage the application of the

Quartz/CORBA framework in the scenarios described in Chapter 6, i.e. media
broadcast, media on demand and videoconference.

In the field of real - time applicat ions, two main areas are candidates to be explored:

manufacturing control and avionics.

In the area of telecommunications, it would be interesting to test the behaviour of the
telephone exchange example in a real telecommunications platform.

References

[1]  W . Almesberger, T. Ferrari and J. - Y. Le Boudec ^Scalable Resource Reservation

                                       for the Internet~, Internet Draft, November 1997.

[2]  Apple Computer Inc. ^QuickTime API Documentation~, Software

                                       Documentation, 1997. Available at developer.apple.com.

[3]  N. Audsley and  A. Burns ^Real Time System Scheduling~, Specification and

                                       Design for Dependability, PDCS ˘  Predictability Dependable Computer Systems

                                       ˘  ESPRIT, 1st Year Report, LAAS, Toulouse, May 1990.

[4]  Cristina Aurrecoechea, Andrew Campbell and Linda Hauw ^A Survey of Q uality

                                       of Service Architectures~, Distributed Multimedia Research Group (MPG),

                                       University of Lancaster, Internal report number MPG - 95 - 18.

[5]  O. Babaoglu and A. Schiper ^On Group Communication in Large - Scale

                                       Distributed Systems~, Broadcast (ESPRIT Basic Resea rch Project 6360)

                                       Technical Report No. 57, 1994.

[6]  F. Baker, R. Guerin and D. Kandlur ^Specification of Commited Rate Quality of

                                       Service~, Internet Draft, June 1996.

[7]  Sean Baker, Vinny Cahill and Paddy Nixon ^Bridging Boundaries: CORBA in

                                       Perspective~, IEEE I nternet Computing, Vol. 1, No. 5, pp. 52 - 57,

                                       September/October 1997.

[8]  Paul Barham ^A Fresh Approach to File System Quality of Service~, Proceedings

                                       of the 7th International Workshop on Network and Operating System Support for

                                       Digital Audio and Video (NOSSDA V´97), St. Louis, USA, May 1997.

[9]  Tsipora Barzilai, Dilip Kandlur, Ashish Mehra, Debajan Saha and Steve Wise

                                       ^Design and Implementation of an RSVP - based Quality of Service Architecture

                                       for Integrated Services Internet~, Proceedings of the 17th Internationa l

                                       Conference on Distributed Computer Systems (ICDCS´97), Baltimore, USA, May

                                       1997.

[10]  John Bates ^CaberNet Report: The State of the Art in Distributed and Dependable

                                       Computing~, CaberNet Technical Report, June 1998.

[11]  BEA Systems et al. ^Notification Service~, OMG Document Telecom/98 - 01 - 01,

                                       January 1998.

[12]  H.W.P. Beadle ^Experiments in Multipoint Multimedia Telecommunication~,

                                       IEEE Multimedia, Vol. 2 No. 2, Summer 1995.

[13]  Luc Bellissard, Slim Ben Atallah, Fabienne Boyer and Michel Riveill ^Distributed

                                       Application Co nfiguration~, INRIA Rhone - Alpes, Research Report RR - 3119,

                                       February 1997.

[14]  T. E. Bihari and P. Gopinath ^Object - Oriented Real - Time Systems: Concepts and

                                       Examples~, IEEE Computer, Vol. 25, No. 12, pp. 25 - 32, December 1992.

[15]  Manuel Billot, Valérie Issarny, Isab elle Puaut, Michel Banâtre ^A Proposal for

                                       Ensuring High Availability of Distributed Multimedia Applications~, Proceedings

                                       of the 15th International Symposium on Reliable Distributed Systems, Canada,

                                       October 1996.

[16]  U. Black ^ATM: Foundation for Broadband Ne tworks~, Prentice Hall, 1995.

[17]  Douglas Boling ^Programming Microsoft Windows CE~, Microsoft Press, 1998.

[18]  Pier Giorgio Bosco, Eirik Dahle, Michel Gien, Andrew Grace, Nicolas

                                       Mercouroff, Nathalie Perdigues, Jean - Bernard Stefani ^The ReTINA Project: an

                                       Overvi ew~, Chorus Systemes Technical Document RT/TR - 96 - 15, May 1996.

[19]  R. Braden, I. Zhang, S. Berson, S. Herzog, and S. Jamin ^Resource ReSerVation

                                       Protocol (RSVP) ˘  Version 1 Functional Specification~, Internet Enginnering

                                       Task Force, RFC 2205, September 1997.

[20]  T orsten Braun ^Internet Protocols for Multimedia Communications~, IEEE

                                       Multimedia, Vol. 4, No. 3, pp. 85 - 90, July - September 1997.

[21]  C. Brazdziunas ^IPng Support for ATM Services~, IETF RFC 1680, August 1994.

[22]  G. Booch, J. Rumbaugh and I. Jacobson ^The Unified Modelling Language User

                                       Guide~ , Addison - Wesley, 1998.

[23]  A. Burns and A. Wellings  ^Real - Time Systems and Programming Languages~,

                                       Second Edition, Addison - Wesley, 1997.

[24]  Andrew Campbell, Geoff Coulson and David Hutchison ^A Quality of Service

                                       Architecture~, ACM  Computer Communications Review, Vol. 24, No. 2, pp. 6 -

                                       27, April 1994. MPG Internal report number MPG - 94 - 08.

[25]  Andrew Campbell and Geoff Coulson ^A QoS adaptive transport system: design,

                                       implementation and experience~, ACM Multimedia´96, pp. 117 - 127, Novemb er

                                       1996.

[26]  Saurav Chateerjee, Bikash Sabata and Jaroslav J. Sydir ^ERDOS QoS

                                       Architecture~, SRI International, Technical Report, May 1998.

[27]  Sarauv Chatterjee, Michael Brown and Bikash Sabata ^Graceful Adaptation of

                                       Distributed Soft Real - Time Applications~, Pr oceedings of the 19
th

 IEEE Real -

                                       Time Systems Symposium (RTSS´98), Work in Progress session, Madrid, Spain,

                                       December 1998.

[28]  Shigang Chen ^Quality of Service in Heterogeneous Environments~, M.Sc.

                                       Thesis, Engineering College, University of Illinois at Urbana - C hampaign, 1997.

[29]  S. C. Cheng and J. A. Stankovic ^Scheduling Algorithms for Real - Time Systems

                                       ˘  A Brief Surveỹ , Hard Real - Time Systems : Tutorial, pp. 150 - 173, IEEE

                                       Computer Society Press, USA, July 1988.

[30]  Michael Clarke, Tom Fitzpatrick and Geoff Coulson ^ Adaptive System Support

                                       for Multimedia in Mobile End - Systems~, Proceedings of the 3rd Communications

                                       Networks Symposium, Manchester, U.K., July 1996. MPG Internal report number

                                       MPG - 96 - 24.

[31]  CNET ˘  France Télécom R&D Center ^Requirements for a Real - time ORB~,

                                       ReTINA Technical Report 96 - 08 (also Chorus Systemes Technical Document

                                       RT/TR - 96 - 08), June 1996.

[32]  R. Cole, D. Shur and C. Villamizar ^IP over ATM: A Framework Document~,

                                       IETF RFC 1932, April 1996.

[33]  George Colouris and Jean Dollimore ^Distributed Systems ˘  Co ncepts and

                                       Design~, Addison - Wesley Pub. Co., USA, 1988.

[34]  A. Conta and S. Deering ^Internet Control Message Protocol (ICMPv6) for the

                                       Internet Protocol Version 6 (IPv6) Specification~, Internet Enginnering Task

                                       Force, RFC 1885, December 1995.

[35]  G. Coulson, and  G.S. Blair, ^Meeting the Real - time Synchronisation

                                       Requirements of Multimedia in Open Distributed Systems~, Distributed Systems

                                       Engineering Journal (DSEJ), Vol. 1, No 1, pp. 135 - 144, 1994.

[36]  G. Coulson, G.S. Blair, J.B. Stefani, F. Horn, and L. Hazard ^Sup porting the Real -

                                       time Requirements of Continuous Media in Open Distributed Processing~,

                                       Computer Networks and ISDN Systems, Vol. 27, No. 8, July 1995.

[37]  G. Coulson and D. Waddington ^A CORBA Compliant Real - Time Multimedia

                                       Platform for Broadband Networks~, Pr oceedings of the International Workshop

                                       on Trends in Distributed Systems (TreDS), Lecture Notes in Computer Science

                                       Volume 1161, Aachen, Germany, October 1996.

[38]  Terry A. Critchley and K. C. Batty ^Open Systems: The Realitỹ , Prentice - Hall,

                                       New York, 1993.

[39]  Frederic Dang Tran, Victor Perebaskine, Jean - Bernard Stefani. Ben, Crawford,

                                       Andre Kramer and Dave Otway  ^Binding and Streams: the ReTINA Approach~,

                                       Chorus Systemes Technical Document RT/TR - 96 - 16, ReTINA Technical Report

                                       96 - 16, March 1996.

[40]  S. Deering and R. Hinden ^Internet Protocol, Version 6 (IPv6) Specification~,

                                       Internet Enginnering Task Force, RFC 1883, December 1995.

[41]  L. Delgrossi and L. Berger ^Internet Stream Protocol Version 2 (ST2) Protocol

                                       Specification ˘  Version ST2+~, Internet Enginnering Task Force, RFC 1819,

                                       August 1995.

[42]  Isabelle Demeure, Jocelyne Farhat, and F. Gasperoni ^A Scheduling Framework

                                       for the Automatic Support of Temporal QoS Constraints~, Proceedings of the

                                       Fourth International Workshop on Quality of Service, Paris, March 1996.

[43]  Sud heer Dharanikota and Kurt Maly ^QUANTA: Quality of Service Architecture

                                       for Native TCP/IP over ATM networks~, Old Dominion University, Department

                                       of Computer Science, Technical Report TR - 96 - 01, February 1996.

[44]  John Matthew Simon Doar ^Multicast in the Async hronous Transfer Mode

                                       Environment~, PhD Dissertation, St. John´s College, University of Cambridge,

                                       January 1993.

[45]  Manek Dubash, Rupert Goodwins and Alan Stevens ^The PC Magazine Guide to

                                       Voice and Data Integration~, PC Magazine, November 1998.

[46]  Margaret A. E llis and Bjarne Stroustrup ^The Annotated C++ Reference Manual~,

                                       Addison - Wesley Pub. Co., USA, 1990.

[47]  Dawson R. Engler, M. Frans Kaashoek, and James O’Toole Jr. ^Exokernel: An

                                       Operating System Architecture for Application - Level Resource Management~,

                                       Proceed ings of the Fifteenth Symposium on Operating Systems Principles,

                                       December 1995.

[48]  John E. Flood ^Telecommunications Switching, Traffic and Networks~, Prentice

                                       Hall International (UK) Limited, 1995.

[49]  J. A. Friesen, C. L. Yang, and R. E. Cline, Jr. ^DAVE: A Plu g - and - Play Model

                                       for Distributed Multimedia Application Development~, IEEE Parallel and

                                       Distributed Technology, Summer 1995.

[50]  B. Fuhrt ^Multimedia Systems ˘  An Overview~, IEEE Multimedia, Vol. 1 No. 1,

                                       Spring 1994.

[51]  Francisco Garcia, David Hutchison, Andreas  Mauthe and Nicholas Yeadon ^QoS

                                       Support for Distributed Multimedia Communications~, Proceedings of the 1st

                                       International Conference on Distributed Platforms, Dresden, Germany, 27

                                       February - 1 March 1996. MPG Internal report number MPG - 96 - 08.

[52]  Jan Gecsei ^Ad aptation in Distributed Multimedia Systems~, IEEE Multimedia,

                                       Vol. 4, No. 2, April - June 1997.

[53]  S. J. Gibbs and D. C. Tsichritzis ^Multimedia Programming~, ACM Press ˘

                                       Addison - Wesley, 1995.

[54]  Richard Golding and John Wilkes ^Persistent Storage for Distributed

                                       Applications~, Proceeding of the Eighth ACM SIGOPS European Workshop,

                                       Sintra, Portugal, September 1998.

[55]  Sreenivas Gollapudi ^A Multithreaded Client - Server Architecture for Distributed

                                       Multimedia Systems~, M.Sc. Thesis, Department of Computer Science,

                                       Univ ersity of New York at Buffalo, July 1996.

[56]  W. J. Goralski ^Introduction to ATM Networking~, McGraw - Hill, 1995.

[57]  Amit Gupta ^Multi - party Real - Time Communication in Computer Networks~,

                                       Ph.D. Dissertation, Computer Science Division, University of California at

                                       Berkeley, February 1996.

[58]  Timothy H. Harrison, David L. Levine and Douglas C. Schmidt ^The Design and

                                       Performance of a Real - time CORBA Event Service~, Proceedings of the 12th

                                       ACM Conference on Object - Oriented Programming Systems, Languages and

                                       Applications (OOPSLA´97), Atlanta, USA, October 1997.

[59]  H. Hartig et al. ^DROPS: OS Support for Distributed Multimedia Applications~,

                                       Desdresn University of Technology, Department of Computer Science, Internal

                                       Report, February 1998.

[60]  Mark Hayter and Derek McAuley ^The Des k Area Network~, Cambridge

                                       University Computer Laboratory, Technical Report 228, May 1991.

[61]  A. Herbert ^CORBA Extensions for Real - Time and Interactive Multimedia~,

                                       APM/ANSA External Paper 1311.02, Cambridge, UK, October 1994.

[62]  Dan Hildebrand ^An Architectura l Overview of QNX~, QNX Software Systems

                                       White Paper, available at www.qnx.com.

[63]  M. T. Hills ^Telecommunications Switching Principles~, George Allen & Unwin

                                       Limited, 1979.

[64]  Robert M. Hinden ^IP Next Generation Overview~ Sun Microsystems Technical

                                       Report, May  1995. Available at playground.sun.com.

[65]  Sungjune Hong, Youngjae Kim and Sunyoung Han ^Real - Time Inter - ORB

                                       Protocol on Distributed Environment~, Proceedings of the 1st IEEE International

                                       Symposium on Object - Oriented Real - Time Distributed Computing (ISORC´98 ),

                                       Kyoto, Japan, April 1998.

[66]  J. - F. Huard and A.A. Lazar, ^On QOS Mapping in Multimedia Networks~,

                                       Proceedings of the 21th IEEE International Computer Software and Application

                                       Conference  (COMPSAC ’97) , Washington, D.C., USA, August 1997.

[67]  Interactive Multim edia Association (IMA) ^IMA Recommended Practice ˘

                                       Multimedia Systems Service~, Second Draft, September 1994.

[68]  International Organization for Standardization (ISO) ^Information Technology ˘

                                       Open Systems Interconnection ˘  Basic Reference Model: The Basic Mod el~,

                                       ISO/IEC 7498 - 1 | ITU - T Recommendation X.200, July 1994.

[69]  International Organization for Standardization (ISO) ^Information Technology ˘

                                       Open Distributed Processing ˘  Reference Model: Overview~, ISO/IEC 10746 - 1,

                                       1998.

[70]  International Organization for Sta ndardization (ISO) ^Information Technology ˘

                                       Quality of Service ˘  Framework~, ISO/IEC 13236, 1998.

[71]  International Telecommunication Union, ^B - ISDN Protocol Reference Model and

                                       Its Application~, ITU - T Recommendation I.321, April 1991.

[72]  Iona Technologies ^Orbi xTalk White Paper~, April 1996.

[73]  Iona Technologies ^Orbix Programmer´s Guide~ and ^Orbix Reference Guide~,

                                       October 1997.

[74]  Iona Technologies, Lucent Technologies and Siemens - Nixdorf, ^Control and

                                       Management of Audio/Video Streams~, OMG Document Telecom/97 ˘ 05 ˘ 07,

                                       July 1997.

[75]  Iona Technologies ^Orbix MX ˘  A Distributed Object Framework for

                                       Telecommunication Service Development and Deployment~ Iona Technologies

                                       White Paper, April 1998.

[76]  Valérie Issarny, Christophe Bidan, Frédéric Leleu, Titos Saridakis ^ Towards

                                       S pecifying QoS - Enabling Software Architectures~, Proceedings of the Fifth IFIP

                                       International Workshop on Quality of Service (IWQOS’97), New York, USA,

                                       May 1997.

[77]  R. Joseph ^MHEG - 5: An Overview~, GMD Focus Technical Report, December

                                       1995.

[78]  Thomas V. Johnson an d Aidong Zhang ^A Framework for Supporting Quality -

                                       Based Presentations of Continuous Multimedia Streams~, Department of

                                       Computer Science, State University of New York at Buffalo, 1996.

[79]  J. - I. Jung ^Quality of Service in Telecommunications (Part I & II)~, IE EE

                                       Communications Magazine, Vol 34, No 8, pp - 108 - 117, August 1996.

[80]  Krishna Kavi, James C. Browne, Anand Triphati ^Computer Systems Research:

                                       The Pressure is On~, IEEE Computer, Vol. 32, No. 1, pp. 30 - 39, January 1999.

[81]  T. Kanezuka, and M. Takizawa ^Quality - based Flexibility in Distributed

                                       Objects~, Proceedings of the 1st IEEE International Symposium on Object -

                                       Oriented Real - Time Distributed Computing (ISORC´98), Kyoto, Japan, April

                                       1998.

[82]  H. Knoche and H. de Meer ^Quantitative QoS - Mapping: A Unifying Approach~ ,

                                       in ^Building QoS into Distributed Systems ˘  IFIP TC6 WG6.1 Fifth International

                                       Workshop on Quality of Service (IWQoS´97)~, Andrew Campbell and Klara

                                       Nahrstedt (Ed.), Chapman & Hall, May 1997.

[83]  H.  Kopetz ^Scheduling~, An Advanced Course on Distributed Sys tems, Estoril,

                                       Portugal, 1992.

[84]  H. Kopetz, G. Fohler, G. Gruensteidl, H. Kantz, G. Pospischil, P. Puschner, J.

                                       Reisinger, R. Schlatterbeck, W. Schuetz, A. Vrchoticky and R. Zainlinger ^Real -

                                       Time System Development: The Programming Model of MARS~, Proceedin gs of

                                       the International Symposium on Autonomous Decentralized Systems, p.190 - 199,

                                       Kawasaki, Japan, March 1993.

[85]  Christoforos E. Kozyrakis and David A. Peterson ^A New Direction for Computer

                                       Architecture Research~, IEEE Computer, Vol. 31, No. 11, November 19 98.

[86]  A. Kramer ^ANSAworks: Multi - Media Streams and CORBA~, ANSA Technical

                                       Report APM.1757.01, April 1996.

[87]  M. Laubach ^Classical IP and ARP over ATM~, Internet Enginnering Task Force,

                                       RFC 1577, January 1994.

[88]  A. A. Lazar, K. S. Lim, and F. Marconcini ^Realizi ng a Foundation for

                                       Programmability of ATM Networks with the Binding Architecture~, IEEE Journal

                                       on Selected Areas in Communications, No. 7, pp. 1214 - 1227, September 1996.

[89]  I. Leslie et al. ^The Design and Implementation of an Operating System to

                                       Support Di stributed Multimedia Applications~, IEEE Journal of Selected Areas in

                                       Communcations, September 1996.

[90]  G. Li ^Supporting Distributed Real - Time Computing~, PhD Thesis, University of

                                       Cambridge Computer Laboratory, Technical Report 322, August 1993.

[91]  G. Li ^Dist ributed Real - Time Objects : the ANSA Approach~, 1st IEEE

                                       Workshop on Object - Oriented Real - Time Dependable Systems, Dana Point, CA,

                                       USA, September 1994.

[92]  C. Lin, H. Chu and K. Nahrstedt ^A Soft Real - Time Scheduling Server on the

                                       Windows NT~, 2nd USENIX Windo ws NT Symposium, Seattle, WA, USA,

                                       August, 1998.

[93]  Thomas D. C. Little and Dinesh Venkatesh ^Prospects for Interactive Video on

                                       Demand~ IEEE Multimedia, Vol. 1 No. 3, Fall 1994.

[94]  S. Lu, K. - W. Lee and V. Bharghavan ^Adaptive Service in Mobile Computing

                                       Enviro nments~, in ^Building QoS into Distributed Systems ˘  IFIP TC6 WG6.1

                                       Fifth International Workshop on Quality of Service (IWQoS´97)~, Andrew

                                       Campbell and Klara Nahrstedt (Ed.), Chapman & Hall, May 1997.

[95]  T. Meyer - Boudnik and W. Effelsberg ^MHEG Explained~,     IEEE Multimedia,

                                       Vol. 2 No. 1, Spring 1995.

[96]  Microsoft Corporation ^Real - time Systems and Microsoft Windows NT~, White

                                       Paper, June 1995. Available at www.microsoft.com.

[97]  Microsoft Corporation ^DCOM: A Technical Overview~, White Paper, 1996.

                                       Available at ww w.microsoft.com.

[98]  Microsoft Corporation ^DirectX 3 Software Development Kit~, Software

                                       Documentation, 1996. Available at www.microsoft.com.

[99]  R. F. Mines, J. A. Friesen, and C. L. Yang ^DAVE: A Plug and Play Model for

                                       Distributed Multimedia Application Develo pment~, Proceedings of the ACM

                                       Multimedia 94 Conference (also Sandia Report SAND94 - 8233, July 1994), ACM

                                       Press, pp. 59 - 66, New York, 1994.

[100] Scott Mitchell, Hani Naguib, George Colouris and Tim Kindberg ^Dinamically

                                       Reconfiguring Multimedia Components: A Mod el - based Approach~, Proceeding

                                       of the Eighth ACM SIGOPS European Workshop, Sintra, Portugal, September

                                       1998.

[101] Klara Nahrstedt, Jonathan M. Smith, ^Design, Implementation and Experiences of

                                       the OMEGA Architecture~, Internal Report MS - CIS - 95 - 22, University o f

                                       Pennsylvania, May 1995.

[102] Klara Nahrstedt, Jonathan M. Smith ^The QoS Broker~, IEEE Multimedia, Vol.2,

                                       No.1, pp. 53 - 67, Spring 1995.

[103] Klara Nahrstedt, Ralf Steinmetz ^Resource Management in Multimedia

                                       Networked Systems~, IEEE Computer, pp. 52 - 64, May 1995.

[104] Klara Nahrstedt ^Experiences with QoS Brokerage and Enforcement~, 2nd

                                       International Conference on Multimedia Information Systems (ICMIS97),

                                       Chicago, IL, April, 1997.

[105] Object Management Group ^The Object Management Architecture Guide~, OMG

                                       Technical Document  92 - 11 - 1, September 1992.

[106] Object Management Group ^IDL C++ Language Mapping Specification~, OMG

                                       Document Number 94 - 9 - 14, September 1994.

[107] Object Management Group ^CORBAservices: Common Object Services

                                       Specification~, OMG Technical Document, March 1995 (Revi sed in November

                                       1996).

[108] Object Management Group ^CORBA 2.0 Specification~, OMG Technical

                                       Document 96 - 03 - 04, USA, March 1996.

[109] Object Management Group ˘  Telecommunication Domain Task Force ^Control

                                       and Management of A/V Streams ˘  Request for Proposals~, OMG T echnical

                                       Document Telecom/96 - 08 - 01, August 1996.

[110] Object Management Group´s Object Request Broker / Object Services Task Force

                                       ^Realtime Technologies ˘  Request for Information~, OMG Technical Document

                                       ORBOS/96 - 09 - 02, October 1996.

[111] David O´Flanagan ^An Imple mentation of the CORBA Audio/Video Streaming

                                       Service using RSVP~, M.Sc. Dissertation, University of Dublin ˘  Trinity College,

                                       Department of Computer Science, Technical Report TCD - CS - 1999 - 32, October

                                       1998.

[112] H. Okamura, Y. Ishikawa and M. Tokoro ^Toward Build ing the Flexible Systems

                                       on the Distributed Environment~, Proceedings of the OOPSLA´91 Workshop on

                                       Reflection and Metalevel Architectures in Object - Oriented Programming, October

                                       1991.

[113] R. O. Onvural ^Asynchronous Transfer Mode Networks ˘  Performance Issues~ ,

                                       Artech House, Second Edition, 1995.

[114] Open Software Foundation ^Distributed Computing Environment Overview~,

                                       OSF White Paper, OSF - DCE - PD - 1090 - 4, 1992.

[115] Maximilian Ott, Daniel Reininger, Wenjun Luo ^Adaptive and Scalable QoS for

                                       Multimedia using Hierarchical  Contracts~, Proceedings of ACM Multimedia´96,

                                       Boston, USA, November 1996.

[116] D. Otway ^DIMMA Overview~, ANSA Tech. Report APM.1439.02, April 1995.

[117] Palm Computing ^Palm OS Reference~, Software Documentation, 1999.

                                       Available at www.palm.com

[118] F. Panzieri and M. Rocetti ^Reliable Synchronization Support and Group -

                                       Membership Services for Distributed Multimedia Applications~, Broadcast

                                       (ESPRIT Basic Research Project 6360) Technical Report No. 90, 1995.

[119] Bjorn Pehrson, Per Gunningberg and Stephen Pink ^Distributed Mul timedia

                                       Applications on Gigabit Networks~, IEEE Network Magazine, pp. 26 - 35, January

                                       1992.

[120] Stephen M. Platt ^What Makes a Faster Processor? ~, Byte Magazine, March

                                       1999. Available at www.byte.com.

[121] Ian Pratt ^The User - Safe Device I/O Architecture~, Ph.D. dis sertation, King´s

                                       College, University of Cambridge, August 1997.

[122] K. Ramamritham and J. A. Stankovic, ^Scheduling Algorithms and Operating

                                       Systems Support for Real - Time Systems~, Proceedings of the IEEE, Vol. 82, No.

                                       1, pp. 55 - 67, January 1994.

[123] F. Reynolds,  R. Clark and F. Travostino ^Evolution of a Distributed, Real - Time,

                                       Object - Based Operating System~, Proceedings of the 1st IEEE International

                                       Symposium on Object - Oriented Real - Time Distributed Computing (ISORC´98),

                                       Kyoto, Japan, April 1998.

[124] R. Rooholamini  and V. Cherkassky ^ATM - Based Multimedia Servers~, IEEE

                                       Multimedia, Vol. 2 No. 1, Spring 1995.

[125] Debajan Saha ^Supporting Distributed Multimedia Applications on ATM

                                       Networks~, Ph.D. Dissertation, Department of Computer Science, University of

                                       Maryland, 1995.

[126] Richard E. Schantz ^Quality of Service~, in ^Encyclopedia of Distributed

                                       Computing~, Partha Dasgupta and Joseph Urban (Eds.), Kluwer Academic

                                       Publishers, 1998.

[127] Douglas C. Schmidt, Tim Harrison and Ehab Al - Shaer ^Object - Oriented

                                       Components for High - speed N etwork Programming~, Proceedings of the 1
st

                                       USENIX Conference on Object - Oriented Technologies (COOTS´95), Monterey,

                                       USA, June 1995.

[128] Douglas C. Schmidt and A. Gokhale ^The Performance of the CORBA Dynamic

                                       Invocation Interface and Dynamic Skeleton Interface over High - Speed ATM

                                       Networks~, Proceedings of the IEEE Globecom´96 Conference, London, England,

                                       November 1996.

[129] Douglas C. Schmidt, Aniruddha Gokhale, Timothy H. Harrison and Guru Parulkar

                                       ^A High Performance Endsystem Architecture for Real - Time CORBA~, IEE E

                                       Communications Magazine, Vol. 14, No. 2, February 1997.

[130] Douglas C. Schmidt, David Levine and Sumedh Mungee ^The Design of the TAO

                                       Real - Time Object Request Broker~, Computer Communications, Elsevier

                                       Science, Vol. 21, No. 4, April, 1998.

[131] H. Schulzrinne, S.  Casner, R. Frederick, and V. Jacobson ^RTP: A Transport

                                       Protocol for Real - Time Applications~, Internet Enginnering Task Force, RFC

                                       1889, January 1996.

[132] H. Schulzrinne, A. Rao and R. Lamphier ^Real - Time Streaming Protocol

                                       (RTSP)~, Internet Enginnering Task Force, Internet Draft, November 1996.

[133] John Segrave - Daly ^The Design and Implementation of a Distributed Music

                                       Rehearsal Studio Application~, University of Dublin ˘  Trinity College,

                                       Department of Computer Science, Final Year Project, June 1999
.

[134] S. Shenker, C. Partridge and R. Guerin ^Specification of Guaranteed Quality of

                                       Service~, Internet Enginnering Task Force, RFC 2212, September 1997.

[135] S. Shenker, J. Wroclawski ^General Characterization Parameters for Integrated

                                       Service Network Elements~, Internet Enginn ering Task Force, RFC 2215,

                                       September 1997.

[136] Richard A. Staehli ^Quality of Service Specification for Resource Management in

                                       Multimedia Systems~, Ph.D. Dissertation, Oregon Graduate Institute of Science

                                       and Technology, January 1996.

[137] Stardust Technologies ^W indows Sockets 2 Application Programming Interface,

                                       White Paper, Revision 2.2.0, May 1996.

[138] R. Steinmetz ^Analyzing the Multimedia Operating System~, IEEE Multimedia,

                                       Vol. 2 No. 1, Spring 1995.

[139] R. Steinmetz and L. C. Wolf ^Quality of Service: Where are we? ~ , in ^Building

                                       QoS into Distributed Systems ˘  IFIP TC6 WG6.1 Fifth International Workshop

                                       on Quality of Service (IWQoS´97)~, Andrew Campbell and Klara Nahrstedt (Ed.),

                                       Chapman & Hall, May 1997.

[140] E. Stoica, H. Abdel - Wahab and K. Maly ^Synchronization of Mult imedia Streams

                                       in Distributed Environments~, Old Dominion University, Department of

                                       Computer Science, Technical Report 97 - 19, February 1997.

[141] H.J. Stuttgen ^Network Evolution and Multimedia Communication~, IEEE

                                       Multimedia, Vol. 2 No. 3, Fall 1995.

[142] Sun Micro systems ^Sun Embedded Telecom Platform ˘  Combining the Power of

                                       Solaris Computing with the Real - Time Performance of the ChorusOS Operating

                                       System~, Sun White Paper, available at www.sun.com.

[143] Jaroslaw J. Sydir, Sarauv Chatterjee, Bikash Sabata ^Providing En d - to - End QoS

                                       Assurances in a CORBA - Based System~, Proceedings of the 1st IEEE

                                       International Symposium on Object - Oriented Real - Time Distributed Computing

                                       (ISORC´98), Kyoto, Japan, April 1998.

[144] Martin Timmerman and Jean - Christophe Monfret ^Windows NT as Real - Time

                                       OS~, Real - Time Magazine, Issue 1997/2, April 1997.

[145] Hideyuki Tokuda, Tatsuo Nakajima and Prithvi Rao ^Real - Time Mach: Towards

                                       a Predictable Real - Time System~, Proceedings of USENIX Mach Workshop,

                                       October 1990.

[146] A. Vogel, B. Kerherve, G. von Bachmannn, and J. Gecsei ^Distributed

                                       Multimedia and QoS: A Surveỹ , IEEE Multimedia, Vol. 2 No. 2, Summer 1995.

[147] D. Waddington, G. Coulson and D. Hutchinson, ^Specifying QoS for Multimedia

                                       Communications within a Distributed Programming Environment~, Proceedings

                                       of t he 3rd International COST237 Workshop: Multimedia Telecommunications

                                       and Applications, Lecture Notes in Computer Science Volume 1185, pp104 - 130,

                                       Barcelona, Spain, November 1996. MPG Internal report number MPG - 96 - 34.

[148] Daniel Waddington, Christopher Edwards and David Hutchison ^Resource

                                       Management for Distributed Multimedia Applications~, Proceedings of the

                                       Second European Conference on Multimedia Applications, Services and

                                       Techniques; Milan, Italy, May 21 - 23 1997; MPG Internal report number MPG -

                                       97 - 10.

[149] Daniel  Waddington and David Hutchison ^A General Model for QoS

                                       Adaptation~, MPG Internal report number MPG - 98 - 09, May 1998.

[150] Daniel Waddington and David Hutchison ^End - to - End QoS Provisioning through

                                       Resource Adaptation~, MPG Internal report number MPG - 98 - 10, Ma y 1998.

[151] Wind River Systems ^The Next Generation of Embedded Development Tools~,

                                       White Paper, available at www.wrs.com.

[152] J. Wroclawski ^The Use of RSVP with IETF Integrated Services~, Internet

                                       Enginnering Task Force, RFC 2210, September 1997.

[153] J. Wroclawski ^Specification of the Controlled - Load Network Element Service~,

                                       Internet Enginnering Task Force, RFC 2211, September 1997.

[154] Nicholas Yeadon, Andreas Mauthe, Francisco Garcia and David Hutchison ^QoS

                                       Filters: Addressing the Heterogeneity Gap~, Proceedings of  the European

                                       Workshop on Interactive Distributed Multimedia Systems and Services (IDMS

                                       96), Berlin, Germany, March 1996. MPG Internal report number MPG - 96 - 09.

[155] Nicholas Yeadon, Francisco Garcia, David Hutchison and Doug Shepherd

                                       ^Filters: QoS Support Mech anisms for Multipeer Communications~, IEEE Journal

                                       on Selected Areas in Computing (JSAC) special issue on Distributed Multimedia

                                       Systems and Technology, Volume 14, Number 7, September 1996, pp1245 - 1262.

                                       MPG Internal report number MPG - 96 - 31.

[156] John A. Zinky,  David E. Bakken, Richard E. Schantz ^Architectural Support for

                                       Quality of Service for CORBA Objects, Theory and Practice of Object Systems,

                                       Vol. 3 No. 1, January 1997.

Appendix

This appendix contains the performance measurements that were obtained with the
remote copy example, which was presented in section 7.1.1 . This data was used to
obtain the values for the overhead caused by the Quartz architecture that was analysed
in section 7.1.5 .

A.1  ATM

The table below shows the performance measurements obtained with the remote copy
application acting as a daemon and using the ATM protocol for transferring a 45Kb file
over the network. Values shown are average times per connection, in milliseconds,
obt ained for a sequence of 100 connection establishments and QoS reservations.

            Total Time

(Function+Child)

                                                                                                                      Effective

                                                                                                       Function Time

Hit

Count

Function Name

                                  3.33  3.33  1  _closesocket@4

                              6.214  6.214  1  _gethostbyname@4

                           33.988  33.988  1  _gethostname@8

                                  0.01  0.0 1  1  _inet_ntoa@4

                           11.817  11.817  47  _send@16

                   26752.07  0.002  1  _WinMain@16

                              0.117  0.117  1  _WSAAsyncSelect@16

                              0.008  0.008  1  _WSACleanup@0

                              0.531  0.531  1  _WSAConnect@28

                              0.503  0.503  1  _WSAConnect@28  w/o QoS

                              0.341  0.341  2  _WSAEnumProtocolsA@12

                              0.001  0.001  1  _WSAGetLastError@0

                              0.132  0.132  1  _WSAIoctl@36

                              1.127  1.127  1  _WSALookupServiceBeginW@12

                              0.134  0.134  1  _WSALookupServiceEnd@4

                              0.717  0.717  1  _WSALookupServiceNextW@16

                           17.782  17.782  1  _WSASocketA@24

                              7.622  7.622  2  _WSAStartup@8

                              0.007  0.00 7  1  AfxGetApp()

                              0.013  0.013  1  AfxGetModuleState()

                                  0.05  0.037  1  AfxInitialize()

                   26752.07  19.104  1  AfxWinMain()

                                  0.01  0.01  3  CComboBox::~CComboBox()

                              0.045  0.045  3  CComboBox::CComboBox()

                              0.919  0.919  3  CComboBox::SetCurSel()

                              0.002  0.002  1  CDialog: :~CDialog()

                              4.429  4.429  425  CDialog::AssertValid()

                              0.037  0.037  1  CDialog::CDialog()

                              0.045  0.045  1  CDialog::CheckAutoCenter()

                   26730.39  78.174  1  CDialog::DoModal()

                              0.326  0.326  426  CDialog::GetRuntimeClass()

                              1.651  1.478  1  CDialog::OnCancel()

                           41. 222  1.38  125  CDialog::OnCmdMsg()

                              4.818  1.016  1  CDialog::OnInitDialog()

                              0.002  0.002  1  CDialog::OnSetFont()

                                             0  0  1  CDialog::PreInitDialog()

                           73.325  25.569  184  CDialog::PreTranslateMessage()

                              0.012  0.012  7  CEdit::~CEdit()

                              0.169  0.169  7  CEdit::CEdit()

    222.494  197.991  104  CEdit::LineScroll()

           0.004  0.004  1  CFile::~CFile()

           0.003  0.003  1  CFile::CFile()

           0.191  0.191  47  CFileException::~CFileException()

           0.555  0.555  47  CFileException::CFileException()

           0.108  0.108  2  CMenu::AppendMenuA()

               0.08  0.001  1  CSampleApp::~CSampleApp()

           0.184  0  1  CSampleApp::CSampleApp()

26732.87  0.005  1  CSampleApp::InitInstance()

                          0  0  340  CSampleDlg::_GetBaseMessageMap()

               0.23  0.063  1  CSampleDlg::~CSampleDlg()

        34.333  0.732  1  CSampleDlg::ATMSender()

           2.245  0.005  1  CSa mpleDlg::CSampleDlg()

           5.697  0.021  2  CSampleDlg::DoDataExchange()

        40.965  0.023  1  CSampleDlg::FillLocalAddress()

               0.52  0.179  1  CSampleDlg::FindProtocols()

           0.536  0.536  1143  CSampleDlg::GetMessageMap()

           7.612  0.004  1  CSampleDlg::InitWS2()

           5.149  0.028  1  CSampleDlg::OnAsyncSelectATM()

                          0  0  1  CSampleDlg::OnCancel()

        37.914  1.235  1  CSampleDlg::OnConnect()

        58.686  0.037  1  CSampleDlg::OnInitDialog()

               0.23  0.006  2  CSampleDlg::OnPaint()

3302.541  3003.988  47  CSampleDlg::OnTimer()

    299.147  0.225  52  CSamp leDlg::PrintStatus()

           0.246  0.246  13  CString::~CString()

           0.006  0.006  8  CString::CString()

           0.083  0.083  5  CString::CString()

           0.001  0.001  1  CString::IsEmpty()

           0.083  0.083  1  CString::LoadStringA()

           0.061  0.061  55  CString::operator char const *()

        10 .344  10.344  104  CString::operator+=()

           0.071  0.071  7  CString::operator=()

               0.08  0.08  1  CWinApp::~CWinApp()

           4.527  4.527  371  CWinApp::AssertValid()

           0.184  0.184  1  CWinApp::CWinApp()

           0.007  0.007  1  CWinApp::Enable3dControls()

           0.027  0.018  1  CWinApp::Ex itInstance()

           0.465  0.465  371  CWinApp::GetRuntimeClass()

           0.003  0.003  1  CWinApp::InitApplication()

           1.905  1.905  1  CWinApp::LoadIconA()

           0.238  0.238  289  CWinThread::GetMainWnd()

           0.308  0.308  183  CWinThread::IsIdleMessage()

        89.245  12.291  184  CWinThrea d::PreTranslateMessage()

           1.022  0.969  102  CWinThread::ProcessMessageFilter()

26553.78  23132.97  184  CWinThread::PumpMessage()

           0.374  0.374  661  CWnd::ContinueModal()

        98.274  34.241  833  CWnd::DefWindowProcA()

        14.102  13.813  1  CWnd::DestroyWindow()

           0.0 27  0.027  2  CWnd::DoDataExchange()

           0.023  0.023  1  CWnd::EndModalLoop()

           0.003  0.003  2  CWnd::GetSuperWndProcAddr()

               0.16  0.16  1  CWnd::GetSystemMenu()

           0.111  0.111  185  CWnd::IsFrameWnd()

           0.009  0.009  2  CWnd::IsIconic()

           0.068  0.068  4  CWnd::KillTimer()

           0.048  0.047  2  CWnd::OnChildNotify()

        45.078  3.977  135  CWnd::OnCommand()

           0.215  0.011  2  CWnd::OnPaint()

               0.67  0.263  47  CWnd::OnTimer()

3429.514  36.696  1151  CWnd::OnWndMsg()

                          0  0  1  CWnd::PostNcDestroy()

           0.003  0.003  1  CWnd::PreSubclassWindow()

           2.63 7  0.072  2  CWnd::SetIcon()

           0.089  0.089  1  CWnd::SetTimer()

           66.82  66.463  56  CWnd::SetWindowTextA()

           1.934  0.013  1  CWnd::UpdateData()

3455.938  0.878  1151  CWnd::WindowProc()

           0.003  0.003  2  DDV_MinMaxFloat()

           0.003  0.003  2  DDV_MinMaxInt()

           1.065  1.065  2  DDV_MinMaxLong()

           1.991  1.991  6  DDX_CBString()

           0.633  0.633  20  DDX_Control()

           0.806  0.779  8  DDX_Text()

           0.599  0.58  2  DDX_Text()

           0.235  0.22  2  DDX_Text()

           0.315  0.298  2  DDX_Text()

           0.389  0.389  31  operator delete()

           0.567  0.567  62  operator new()

           0.018  0.018  5  operator==()

           0.001  0  1  QzApplication::QzApplication()

               0.01  0  1  QzATMAgent::‘scalar deleting destructor’()

               0.01  0  1  QzATMAgent::‘vector deleting destructor’()

           0.001  0  1  QzATMAgent::~QzATMAgent()

           0.067  0.056  1  QzATMAgent::Init()

           0.0 15  0.002  1  QzATMAgent::InitWS2()

           0.545  0.043  1  QzATMAgent::QoSRequest()

           0.072  0.003  1  QzATMAgent::QzATMAgent()

                          0  0  3  QzATMFilter::QzATMFilter()

               0.31  0.003  1  QzATMFilter::TranslateQoSDownwards()

           0.001  0.001  1  QzBypassFilter::QzBypassFilter()

           0.0 02  0.002  4  QzSystemAgent::~QzSystemAgent()

           0.006  0.006  4  QzSystemAgent::QzSystemAgent()

           0.001  0  1  QzDataPacketFilter::QzDataPacketFilter()

           0.118  0.029  1  QzDataPacketFilter::TranslateQoSDownwards()

           0.002  0.002  2  QzNetworkAgent::~QzNetworkAgent()

           0 .003  0  2  QzNetworkAgent::QzNetworkAgent()

           0.001  0  1  QzOSAgent::~QzOSAgent()

           0.001  0  1  QzOSAgent::QzOSAgent()

           0.145  0.002  2  QzQoS::‘scalar deleting destructor’()

           0.145  0.002  2  QzQoS::‘vector deleting destructor’()

           0.128  0.003  3  QzQoS::~QzQoS()

           0 .261  0.261  33  QzQoS::GetParam()

                          0  0  12  QzQoS::GetParam()

           0.003  0.003  6  QzQoS::QzQoS()

           0.613  0.16  33  QzQoS::SetParam()

                              0.036  0  1  QzQoSAgent::‘scalar deleting destructor’()

                              0.036  0  1  QzQoSAgent::‘vector deleting destructor’()

                              0.028  0.004  1  QzQoSA gent::~QzQoSAgent()

                              0.178  0.009  3  QzQoSAgent::AgentFactory()

                                  0.25  0.008  1  QzQoSAgent::Init()

                              1.314  0.004  1  QzQoSAgent::QoSRequest()

                              0.096  0.005  1  QzQoSAgent::QzQoSAgent()

                              0.073  0.044  1  QzRSVPAgent::‘scalar deleting destructor’()

                              0.073  0.044  1  Q zRSVPAgent::‘vector deleting destructor’()

                              0.018  0.003  1  QzRSVPAgent::~QzRSVPAgent()

                              0.002  0.002  1  QzRSVPAgent::CleanUp()

                              0.062  0.06  1  QzRSVPAgent::QzRSVPAgent()

                                             0  0  3  QzRSVPFilter::QzRSVPFilter()

                              0.023  0.023  13  QzTranslation::QzTranslation()

                              0 .049  0.028  3  QzInterpreter::QzInterpreter()

                              0.233  0.039  1  QzInterpreter::TranslateQoSDownwards()

                              0.003  0.003  3  QzUpcall::QzUpcall()

                              0.013  0.002  1  QzWinNTAgent::‘scalar deleting destructor’()

                              0.013  0.002  1  QzWinNTAgent::‘vector deleting destructor’( )

                              0.002  0.001  1  QzWinNTAgent::~QzWinNTAgent()

                                  0.08  0.06  1  QzWinNTAgent::Init()

                              0.337  0.236  1  QzWinNTAgent::QoSRequest()

                              0.003  0.002  1  QzWinNTAgent::QzWinNTAgent()

                              0.002  0.001  2  QzWinNTFilter::QzWinNTFilter()

                              0.098  0.003  1  QzWinNTFilter::Transla teQoSDownwards()

A.2  UDP + RSVP

These are the results of the performance measurements obtained with the remote copy
application using UDP for data transfer and RSVP for resource reservation. The same
test scenario that was used for measuring the performa nce of the application when using
the ATM protocol was applied in this case.

           Total Time

(Function+Child)

                                                                                                                       Effective

                                                                                                        Function Time

Hit

Count

Function Name

                             0.945  0.945  2  _closesocket@4

                          19.917  19.917  4  _gethostbyname@4

                          10.966  10.966  2  _gethostname@8

                             0. 112  0.112  52  _htons@4

                             0.105  0.105  5  _inet_addr@4

                             0.621  0.621  50  _inet_ntoa@4

                             0.001  0.001  1  _ntohl@4

                          23.274  23.274  47  _sendto@24

                  12548.99  97.302  1  _WinMain@16

                             0.014  0.014  1  _WSACleanup@0

                             1.024  1.024  4  _WSAEnumProtocolsA@12

                          11.533  11.533  3  _W SAIoctl@36

                          18.695  18.695  2  _WSASocketA@24

                                 9.73  9.73  2  _WSAStartup@8

                                 0.06  0.06  1  AfxInitialize()

           0.097  0.097  1  CSampleApp::~CSampleApp()

           0.241  0.241  1  CSampleApp::CSampleApp()

12451.69  11943.65  1  CSampleApp::InitInstance()

                          0  0  327  CSampleDlg::_ GetBaseMessageMap()

           0.171  0.171  1  CSampleDlg::~CSampleDlg()

           3.054  3.052  1  CSampleDlg::CsampleDlg()

           7.279  7.279  2  CSampleDlg::DoDataExchange()

       20.641  0.028  1  CSampleDlg::FillLocalAddress()

           0.788  0.233  1  CSampleDlg::FindProtocols()

           0.902  0.902  11 03  CSampleDlg::GetMessageMap()

               9.72  0.004  1  CSampleDlg::InitWS2()

                          0  0  1  CSampleDlg::OnCancel()

           53.28  1.86  1  CSampleDlg::OnConnect()

               61.7  25  1  CSampleDlg::OnInitDialog()

           0.432  0.432  2  CSampleDlg::OnPaint()

    385.566  12.856  47  CSampleDlg::OnTimer()

       353.54  353.591  50  CSampleDlg::PrintStatus()

       49.473  0.469  1  CSampleDlg::UDPSender()

           0.002  0.001  1  QzApplication::QzApplication()

                          0  0  2  QzATMFilter::QzATMFilter()

                          0  0  1  QzBypassFilter::QzBypassFilter()

                          0  0  3  QzSystemAgent::~QzSystemAgent()

           0.003  0.003  3  QzSystemAgent::QzSystemAgent()

                          0  0  1  QzDataPacketFilter::QzDataPacketFilter()

           0.161  0.05  1  QzDataPacketFilter::TranslateQoSDownwards()

                          0  0  1  QzNetworkAgent::~QzNetworkAgent()

           0.001  0  1  QzNetworkAgent::QzNetworkAgent()

                          0  0  1  QzOSAgent::~Q zOSAgent()

                          0  0  1  QzOSAgent::QzOSAgent()

           0.136  0.019  2  QzQoS::‘scalar deleting destructor’()

           0.136  0.019  2  QzQoS::‘vector deleting destructor’()

           0.116  0.116  2  QzQoS::~QzQoS()

           0.186  0.186  43  QzQoS::GetParam()

                          0  0  12  QzQoS::GetParam()

           0.002  0.00 2  5  QzQoS::QzQoS()

           0.725  0.725  32  QzQoS::SetParam()

           1.709  0.011  1  QzQoSAgent::‘scalar deleting destructor’()

           1.709  0.011  1  QzQoSAgent::‘vector deleting destructor’()

           1.698  0.006  1  QzQoSAgent::~QzQoSAgent()

           0.105  0.031  2  QzQoSAgent::AgentFactory(u nsigned int,char

*)

           9.163  0.007  1  QzQoSAgent::Init()

       21.176  0.007  1  QzQoSAgent::QoSRequest()

           0.109  0.003  1  QzQoSAgent::QzQoSAgent()

           1.683  0.014  1  QzRSVPAgent::‘scalar deleting destructor’()

           1.683  0.014  1  QzRSVPAgent::‘vector deleting destructor’( )

           1.669  0.03  1  QzRSVPAgent::~QzRSVPAgent()

               1.64  0.004  1  QzRSVPAgent::CleanUp()

           5.214  0.008  1  QzRSVPAgent::FillLocalAddress()

               0.64  0.171  1  QzRSVPAgent::FindProtocols()

           9.079  0.297  1  QzRSVPAgent::Init()

           0.058  0.044  1  QzRSVPAgent::InitWS2()

       20.2 08  0.006  1  QzRSVPAgent::QoSRequest()

                             0.074  0.072  1  QzRSVPAgent::QzRSVPAgent()

                                 9.18  0.01  1  QzRSVPAgent::RSVPOpenSocket()

                             9.825  0.011  1  QzRSVPAgent::RSVPRegister

                             1.034  0.004  1  QzRSVPAgent::RSVPRelSender()

                             0.757  0.018  1  QzRSVPAgent::RSVPSender

                                            0  0  3  QzRSVPFilter::QzRSVPFilter()

                             0.413  0.075  1  QzRSVPFilter::TranslateQoSDownwards()

                             0.015  0.015  12  QzTranslation::QzTranslation

                                 0.06  0.041  3  QzInterpreter::QzInterpreter()

                                 0.27  0.055  1  QzInterpreter::TranslateQoSDownwards()

                             0.001  0.001  3  QzUpcall ::QzUpcall()

                             0.009  0.011  1  QzWinNTAgent::‘scalar deleting destructor’()

                             0.009  0.011  1  QzWinNTAgent::‘vector deleting destructor’()

                                            0  0  1  QzWinNTAgent::~QzWinNTAgent()

                             0.077  0.077  1  QzWinNTAgent::Init()

                             0.461  0.313  1  QzWinNTAgent::QoSRequest()

                                            0  0.001  1  QzWinNTAgent::QzWinNTAgent()

                                            0  0  2  QzWinNTFilter::QzWinNTFilter()

                             0.147  0.045  1  QzWinNTFilter::TranslateQoSDownwards()

A.3  TCP + RSVP

These are the results of the performance measurements obtained with the ^
rcp
~
application using TCP for dat a transfer and RSVP for resource reservation. The same
test procedure that was used in the last two cases was applied here.

           Total Time

(Function+Child)

                                                                                                                       Effective

                                                                                                        Function Time

Hit

Count

Function Name

                             9.884  9.884  2  _closesocket@4

                             0.687  0.687  1  _connect@ 12

                             0.002  0.002  1  _GetCurrentProcess@0

                          19.704  19.704  4  _gethostbyname@4

                          10.708  10.708  2  _gethostname@8

                             0.003  0.003  1  _GetModuleHandleA@4

                             0.013  0.013  1  _GetStartupInfoA@4

                             0.004  0.004  6  _htons@4

                             0.118  0.118  5  _inet_addr@4

                             0.046  0.046  3  _inet_nto a@4

                          76.114  76.114  47  _send@16

                             0.285  0.285  1  _SetPriorityClass@8

                             0.028  0.028  1  _setsockopt@20

                  14111.97  26.879  1  _WinMain@16

                             1.742  1.742  1  _WSAAsyncSelect@16

                             0.016  0.016  1  _WSACleanup@0

                             0.994  0.994  4  _WSAEnumProtocolsA@12

                             0.003  0.003  1  _WSAGe tLastError@0

                          23.841  23.841  3  _WSAIoctl@36

                          111.24  111.24  2  _WSASocketA@24

                             9.591  9.591  2  _WSAStartup@8

                             0.057  0.057  1  AfxInitialize()

                             0.093  0.093  1  CSampleApp::~CSampleApp()

           0.251  0.251  1  CSampleApp::CSampleApp

14085.09  13281.14  1  CSampleApp::In itInstance()

           0.072  0.072  323  CSampleDlg::_GetBaseMessageMap()

               0.17  0.17  1  CSampleDlg::~CSampleDlg()

           2.516  2.514  1  CSampleDlg::CSampleDlg()

               8.13  8.13  2  CSampleDlg::DoDataExchange()

       20.833  0.034  1  CSampleDlg::FillLocalAddress()

           0.756  0.224  1  CSam pleDlg::FindProtocols()

               1.27  1.27  1040  CSampleDlg::GetMessageMap()

           9.581  0.006  1  CSampleDlg::InitWS2()

    160.594  0.232  1  CSampleDlg::OnAsyncSelectTCP()

                          0  0  1  CSampleDlg::OnCancel()

    121.013  1.875  1  CSampleDlg::OnConnect()

       67.974  30.347  1  CSampleDl g::OnInitDialog()

           0.159  0.159  1  CSampleDlg::OnPaint()

    448.215  11.75  47  CSampleDlg::OnTimer()

    477.656  476.973  51  CSampleDlg::PrintStatus()

    117.208  0.298  1  CSampleDlg::TCPSender()

           0.002  0.001  1  QzApplication::QzApplication()

           0.003  0.001  2  QzATMFi lter::QzATMFilter()

           0.002  0.002  1  QzBypassFilter::QzBypassFilter()

                          0  0  3  QzSystemAgent::~QzSystemAgent()

           0.004  0.004  3  QzSystemAgent::QzSystemAgent()

           0.004  0.003  1  QzDataPacketFilter::QzDataPacketFilter()

           0.195  0.09  1  QzDataPacketFilter::Translat eQoSDownwards()

           0.002  0.002  1  QzNetworkAgent::~QzNetworkAgent()

           0.002  0.001  1  QzNetworkAgent::QzNetworkAgent()

           0.001  0.001  1  QzOSAgent::~QzOSAgent()

           0.003  0.002  1  QzOSAgent::QzOSAgent()

           0.129  0.023  2  QzQoS::‘scalar deleting destructor’()

           0.129  0.023  2  QzQoS::‘vector deleting destructor’()

           0.108  0.108  3  QzQoS::~QzQoS()

           0.208  0.208  43  QzQoS::GetParam()

           0.009  0.009  12  QzQoS::GetParam()

           0.007  0.007  6  QzQoS::QzQoS()

           0.708  0.708  32  QzQoS::SetParam()

           9.525  0.013  1  QzQoSAgent::‘scalar deleti ng destructor’()

           9.525  0.013  1  QzQoSAgent::‘vector deleting destructor’()

           9.512  0.01  1  QzQoSAgent::~QzQoSAgent()

           0.117  0.028  2  QzQoSAgent::AgentFactory()

           9.149  0.009  1  QzQoSAgent::Init()

    119.025  0.016  1  QzQoSAgent::QoSRequest()

               0.13  0.01  1  QzQo SAgent::QzQoSAgent()

           9.487  0.017  1  QzRSVPAgent::‘scalar deleting destructor’()

           9.487  0.017  1  QzRSVPAgent::‘vector deleting destructor’()

               9.47  0.04  1  QzRSVPAgent::~QzRSVPAgent()

           9.429  0.006  1  QzRSVPAgent::CleanUp()

           5.257  0.008  1  QzRSVPAgent::FillL ocalAddress()

           0.629  0.167  1  QzRSVPAgent::FindProtocols()

           9.061  0.287  1  QzRSVPAgent::Init()

           0.056  0.04  1  QzRSVPAgent::InitWS2()

    117.998  0.018  1  QzRSVPAgent::QoSRequest()

           0.082  0.08  1  QzRSVPAgent::QzRSVPAgent()

101.933  0.014  1  QzRSVPAgent::RSVPOp enSocket()

    14.519  0.016  1  QzRSVPAgent::RSVPRegister()

       8.375  0.009  1  QzRSVPAgent::RSVPRelSender()

       1.042  0.018  1  QzRSVPAgent::RSVPSender

                      0  0  3  QzRSVPFilter::QzRSVPFilter()

       0.452  0.104  1  QzRSVPFilter::TranslateQoSDownwards()

       0.022  0.022  12  QzTrans lation::QzTranslation()

       0.059  0.04  3  QzInterpreter::QzInterpreter()

       0.306  0.079  1  QzInterpreter::TranslateQoSDownwards()

       0.002  0.002  3  QzUpcall::QzUpcall()

       0.015  0.013  1  QzWinNTAgent::‘scalar deleting destructor’()

       0.015  0.013  1  QzWinNTAgent::‘ve ctor deleting destructor’()

       0.003  0.002  1  QzWinNTAgent::~QzWinNTAgent()

       0.078  0.078  1  QzWinNTAgent::Init()

       0.449  0.013  1  QzWinNTAgent::QoSRequest()

       0.007  0.004  1  QzWinNTAgent::QzWinNTAgent()

       0.001  0.001  2  QzWinNTFilter::QzWinNTFilter()

       0.146  0. 044  1  QzWinNTFilter::TranslateQoSDownwards()